{"text_format":"3","workbook":"xls","n_sheets":9,"sheets":["回潮","加料","真空回潮","API封装需求","300加料","加料——001","Sheet6","Sheet1","进叶柜"],"not_rendered":{"external_links":1,"defined_names":3},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"回潮","index":0,"n_rows":41,"n_cols":17,"rows_kept":41,"merged":[[1,0,38,0],[1,1,8,1],[9,1,23,1],[19,2,22,2],[19,3,22,3],[19,4,22,4],[19,5,22,5],[19,7,22,7],[19,8,22,8],[19,9,22,9],[24,1,29,1],[30,1,36,1],[37,1,38,1]],"flags":["formulas_cached_only"]}
["工序","操作按钮","组件封装","业务说明","参数说明","API接口名","写入点位","检查点位","测试状态","测试方法","测试输入","测试输出","测试点位变化","备注","API状态","按键逻辑"]
["5千回潮","设备预热","预热启动-松散回潮",null,"无","L5KYPHC_YRSTART_HC","YT6022_C_SJ2116_PREHEAT_START",null,"配置测试完成","get","无","{\n    \"result\": {\n        \"plcResults\": [\n            {\n                \"tagAddress\": \"FIX.YT6022_C_WQ2126_PREHEAT_START.F_CV\",\n                \"value\": 1,\n                \"isSetSuccessful\": true,\n                \"message\": \"写入成功\"\n            },\n            {\n                \"tagAddress\": \"FIX.YT6022_C_WQ2126_PREHEAT_STOP.F_CV\",\n                \"value\": 0,\n                \"isSetSuccessful\": true,\n                \"message\": \"写入成功\"\n            }\n        ],\n        \"sucessful\": true,\n        \"message\": \"批量写入---成功\"\n    },\n    \"success\": true,\n    \"error\": null\n}","FIX.YT6022_C_SJ2116_PREHEAT_START.F_CV 1\nFIX.YT6022_C_SJ2116_PREHEAT_STOP.F_CV  0",null,null,"Fix32.THISNODE.YT6022_C_SJ2116_PREHEAT_START.F_CV = 1\nFix32.THISNODE.YT6022_C_SJ2116_PREHEAT_STOP.F_CV = 0"]
[null,null,"预热启动-薄片",null,"无","L5KYPHC_YRSTART_BP","YT6022_C_WQ2126_PREHEAT_START",null,"配置测试完成","get","无","{\n    \"result\": {\n        \"plcResults\": [\n            {\n                \"tagAddress\": \"FIX.YT6022_C_SJ2116_PREHEAT_START.F_CV\",\n                \"value\": 1,\n                \"isSetSuccessful\": true,\n                \"message\": \"写入成功\"\n            },\n            {\n                \"tagAddress\": \"FIX.YT6022_C_SJ2116_PREHEAT_STOP.F_CV\",\n                \"value\": 0,\n                \"isSetSuccessful\": true,\n                \"message\": \"写入成功\"\n            }\n        ],\n        \"sucessful\": true,\n        \"message\": \"批量写入---成功\"\n    },\n    \"success\": true,\n    \"error\": null\n}","FIX.YT6022_C_WQ2126_PREHEAT_START.F_CV 1\nFIX.YT6022_C_WQ2126_PREHEAT_STOP.F_CV  0",null,null,"Fix32.THISNODE.YT6022_C_WQ2126_PREHEAT_START.F_CV = 1\nFix32.THISNODE.YT6022_C_WQ2126_PREHEAT_STOP.F_CV = 0"]
[null,null,"松散预热温度值设定",null,"温度值","L5KYPHC_YPHC_YRWDSET(float Temp)","YT6022_VALUE_WQ2116_P_SET_1",null,"配置测试完成","post",36.5,null,"FIX.YT6022_VALUE_WQ2116_P_SET_1.F_CV   36.5",null,null,"Fix32.THISNODE.YT6022_VALUE_WQ2116_P_SET_1.F_CV"]
[null,null,"薄片预热温度值设定",null,"温度值","L5KYPHC_BPHC_YRWDSET(float Temp)","YT6022_VALUE_WQ2126_P_SET_1",null,"配置测试完成","post",36.5,null,"FIX.YT6022_VALUE_WQ2126_P_SET_1.F_CV  36.5",null,null,"Fix32.THISNODE.YT6022_VALUE_WQ2126_P_SET_1.F_CV"]
[null,null,"松散预热生产温度值设定",null,"温度值","L5KYPHC_YPHC_YXWDSET(float Temp)","YT6022_VALUE_WQ2116_PID4_SP",null,"配置测试完成","post",36.5,null,"FIX.YT6022_VALUE_WQ2116_PID4_SP.F_CV   36.5",null,null,"Fix32.THISNODE.YT6022_VALUE_WQ2116_PID4_SP.F_CV"]
[null,null,"薄片预热生产温度值设定",null,"温度值","L5KYPHC_BPHC_YXWDSET(float Temp)","YT6022_VALUE_WQ2126_PID4_SP",null,"配置测试完成","post",36.5,null,"FIX.YT6022_VALUE_WQ2126_PID4_SP.F_CV   36.5",null,null,"Fix32.THISNODE.YT6022_VALUE_WQ2126_PID4_SP.F_CV"]
[null,null,"预热结束-松散回潮",null,"无","L5KYPHC_YRCLOSE_HC","YT6022_C_SJ2116_PREHEAT_STOP",null,"配置测试完成","get","无",null,"FIX.YT6022_C_SJ2116_PREHEAT_START.F_CV 0\nFIX.YT6022_C_SJ2116_PREHEAT_STOP.F_CV  1",null,null,"Fix32.THISNODE.YT6022_C_SJ2116_PREHEAT_START.F_CV = 0\nFix32.THISNODE.YT6022_C_SJ2116_PREHEAT_STOP.F_CV = 1"]
[null,null,"预热结束-薄片",null,"无","L5KYPHC_YRCLOSE_BP","YT6022_C_WQ2126_PREHEAT_STOP",null,"配置测试完成","get","无",null,"FIX.YT6022_C_WQ2126_PREHEAT_START.F_CV 0\nFIX.YT6022_C_WQ2126_PREHEAT_STOP.F_CV 1\n",null,null,"Fix32.THISNODE.YT6022_C_WQ2126_PREHEAT_START.F_CV = 0\nFix32.THISNODE.YT6022_C_WQ2126_PREHEAT_STOP.F_CV = 1"]
[null,"组合启动","生产路径选择（真空）",null,"真空回潮","L5KYPHC_ZHQD_PATHSELECT_ZK","YT6022_TASK1_R09（真空））",null,"配置测试完成","get",null,null,"FIX.YT6022_TASK1_R09.F_CV   1","(需要增加路径取消接口)\n具备切换功能，取消清除两个？",null,"writevalue 1, \"Fix32.THISNODE.YT6022_TASK1_R09.F_CV\", 1\n","If Readvalue(\"Fix32.THISNODE.YT6022_TASK1_R06.F_CV\", 1) = 0 Then\n   writevalue 1, \"Fix32.THISNODE.YT6022_TASK1_R06.F_CV\", 1 = True\nElse\n   writevalue 0, \"Fix32.THISNODE.YT6022_TASK1_R06.F_CV\", 1\nEnd If"]
[null,null,"生产路径选择（薄片）",null,"薄片旁线","L5KYPHC_ZHQD_BP_PATHSELECT_BP","YT6022_TASK1_R06（薄片）",null,"配置测试完成","get",null,null,"FIX.YT6022_TASK1_R06.F_CV   1",null,null,"Fix32.THISNODE.YT6022_TASK1_R06.F_CV = 1"]
[null,null,"生产路径取消（真空）",null,"真空回潮取消","L5KYPHC_ZHQD_PATHCANCEL_ZK","YT6022_TASK1_R09（真空）",null,"配置测试完成","get",null,null,"FIX.YT6022_TASK1_R09.F_CV   0",null,null,"Fix32.THISNODE.YT6022_TASK1_R09.F_CV = 0"]
[null,null,"生产路径取消（薄片）",null,"薄片旁线取消","L5KYPHC_ZHQD_PATHCANCEL_BP","YT6022_TASK1_R06（薄片）",null,"配置测试完成","get",null,null,"FIX.YT6022_TASK1_R06.F_CV    0",null,null,"Fix32.THISNODE.YT6022_TASK1_R06.F_CV = 0"]
[null,null,"工单信息下发",null,"工单号、批次号、牌号","L5KYPHC_ZHQD_GDMSGWRITE(string GDNum,string BatchNum,string BrandNum) JSON方式","YT6022_MIXENTRYID（工单）/YT6022_MIXBATCHNO（批次）/YT6022_MIXBRAND（牌号）",null,"配置测试完成","post",null,null,"FIX.YT6022_MIXENTRYID（工单）/YT6022_MIXBATCHNO（批次）/YT6022_MIXBRAND（牌号）",null,null,"Fix32.THISNODE.YT6022_MIXENTRYID.A_CV = \nFix32.THISNODE.YT6022_MIXBATCHNO.A_CV = \nFix32.THISNODE.YT6022_YT6022_MIXBRAND.A_CV = "]
[null,null,"批开始",null,"无","L5KYPHC_ZHQD_BATCHSTART","YT6022_TASK1_BSTART  1\nYT6022_TASK1_BSTOP  0",null,"配置测试完成","get",null,null,"FIX.YT6022_TASK1_BSTART.F_CV 1\nFIX.YT6022_TASK1_BSTOP.F_CV 0",null,null,"Fix32.THISNODE.YT6022_TASK1_BSTART.F_CV = 1\nFix32.THISNODE.YT6022_TASK1_BSTART.F_CV = 0"]
[null,null,"生产关联选中",null,null,"L5KYPHC_ZHQD_REFSELECT","JK_YT6022_TANK1_TAG",null,null,"get",null,null,"FIX.JK_YT6022_TANK1_TAG.F_CV  1",null,null,"Fix32.THISNODE.JK_YT6022_TANK1_TAG.F_CV = 1"]
[null,null,"生产关联取消",null,null,"L5KYPHC_ZHQD_REFCANCEL","JK_YT6022_TANK1_TAG",null,null,"get",null,null,"FIX.JK_YT6022_TANK1_TAG.F_CV 0",null,null,"Fix32.THISNODE.JK_YT6022_TANK1_TAG.F_CV = 0"]
[null,null,"进预配柜条件验证","柜冲突判断，柜路径选中，柜信息写入，柜号写入；\n需要反馈选柜结果，如果是选柜失败，\n需要反馈失败信息，例如-柜冲突???  \n（过程存在信息返回、接口是否访问)","单柜号","L5KYPHC_ZHQD_YPGCHECK(string GPno1) 参数示例：\"YP04\"","JK_YT6022_TASK1_A04（YP04）/JK_YT6022_TASK1_A03（YP05）/JK_YT6022_TASK1_A02（YP06）/JK_YT6022_TASK1_A01（YP07）","JK_YT6022_YP04_INT_UNITERR\n/JK_YT6022_YP05_INT_UNITERR\n/JK_YT6022_YP06_INT_UNITERR\n/JK_YT6022_YP07_INT_UNITERR","输入值  YP04,YP05,YP06,PR07\n根据输入值分别将点位置1","post",null,null,"JK_YT6022_YP04_INT_UNITERR\n/JK_YT6022_YP05_INT_UNITERR\n/JK_YT6022_YP06_INT_UNITERR\n/JK_YT6022_YP07_INT_UNITERR"]
[null,null,"进预配柜取消验证",null,"单柜号","L5KYPHC_ZHQD_YPGCANCEL(string GPno1)参数示例：\"YP04\"","JK_YT6022_TASK1_A04_CLEAR\nJK_YT6022_TASK1_A03_CLEAR\nJK_YT6022_TASK1_A02_CLEAR\nJK_YT6022_TASK1_A01_CLEAR\n",null,"输入值  YP04,YP05,YP06,YP07\n根据输入值分别将点位置0","post",null,null,"JK_YT6022_TASK1_A04_CLEAR 1\nJK_YT6022_TASK1_A03_CLEAR 1\nJK_YT6022_TASK1_A02_CLEAR 1\nJK_YT6022_TASK1_A01_CLEAR 1\n",null,null,"Fix32.THISNODE.JK_YT6022_TASK1_A04.F_CV = 0\nFix32.THISNODE.JK_YT6022_TASK1_A03.F_CV = 0\nFix32.THISNODE.JK_YT6022_TASK1_A02.F_CV = 0\nFix32.THISNODE.JK_YT6022_TASK1_A01.F_CV = 0"]
[null,null,"进预配柜信息下发",null,"单柜号、批次号、牌号","L5KYPHC_ZHQD_YPGINFOSET(string GPNum,string BatchNum,string BrandNum) JSON方式：参数示例{\"GPNum\":\"YP04\",\"BatchNum\":\"456\",\"BrandNum\":\"789\"}","YT6022_GP_2139R_JOB(YP04批次)\n/YT6022_GP_2139R_BRAND（牌号）",null,null,"post",null,null,"YT6022_GP_2139R_JOB(YP04批次)\n/YT6022_GP_2139R_BRAND（牌号）"]
[{"$nulls":6},"YT6022_GP_2139L_JOB(YP05批次)\n/YT6022_GP_2139L_BRAND（牌号）",{"$nulls":5},"YT6022_GP_2139L_JOB(YP05批次)\n/YT6022_GP_2139L_BRAND（牌号）"]
[{"$nulls":6},"YT6022_GP_2138R_JOB(YP06批次)\n/YT6022_GP_2138R_BRAND（牌号）",{"$nulls":5},"YT6022_GP_2138R_JOB(YP06批次)\n/YT6022_GP_2138R_BRAND（牌号）"]
[{"$nulls":6},"YT6022_GP_2138L_JOB(YP07批次)\n/YT6022_GP_2138L_BRAND（牌号）",{"$nulls":5},"YT6022_GP_2138L_JOB(YP07批次)\n/YT6022_GP_2138L_BRAND（牌号）"]
[null,null,"设备组合启动",null,"无","L5KYPHC_ZHQD_START","YT6022_IN_TASK1_START",null,null,"get",null,null,"FIX.YT6022_IN_TASK1_START.F_CV   1",null,null,"\nFix32.THISNODE.YT6022_IN_TASK1_START.F_CV = 1"]
[null,"生产提升","生产提升-松散回潮",null,"无","L5KYPHC_TS_YPHCSTART","YT6022_WPL3373_ASEND",null,null,"get",null,null,"FIX.YT6022_WPL3373_ASEND.F_CV    1"]
[null,null,"强制提升-松散回潮",null,"无","L5KYPHC_TS_YPHCFORCE","YT6022_WPL3373_FORCEASEND",null,null,"get",null,null,"FIX.YT6022_WPL3373_FORCEASEND.F_CV    1"]
[null,null,"强制停止提升-松散回潮",null,"无","L5KYPHC_TS_YPHCSTOP","YT6022_WPL3373_FORCESTOP",null,null,"get",null,null,"FIX.YT6022_WPL3373_FORCESTOP.F_CV    1"]
[null,null,"生产提升-薄片",null,"无","L5KYPHC_TS_BPHCSTART","YT6022_WPL2122_ASEND",null,null,"get",null,null,"FIX.YT6022_WPL2122_ASEND.F_CV     1"]
[null,null,"强制提升-薄片",null,"无","L5KYPHC_TS_BPHCFORCE","YT6022_WPL2122_FORCEASEND",null,null,"get",null,null,"FIX.YT6022_WPL2122_FORCEASEND.F_CV     1"]
[null,null,"强制停止提升-薄片",null,"无","L5KYPHC_TS_BPHCSTOP","YT6022_WPL2122_FORCESTOP",null,null,"get",null,null,"FIX.YT6022_WPL2122_FORCESTOP.F_CV     1"]
[null,"组合停止","批结束【确认】",null,"无","L5KYPHC_ZHSTOP_BATCH_END","YT6022_TASK1_BSTOP  1\nYT6022_TASK1_BSTART  0",null,null,"get",null,null,"FIX.YT6022_TASK1_BSTOP.F_CV      1\n\nFIX.YT6022_TASK1_BSTART.F_CV      0",null,null,"writevalue 1, \"Fix32.THISNODE.YT6022_IN_TASK1_FINISH.F_CV\", 1\nwritevalue 0, \"Fix32.THISNODE.YT6022_TASK1_NODEA.F_CV\", 1\nwritevalue 0, \"Fix32.THISNODE.YT6022_TASK1_ROUTE.F_CV\", 1\n"]
[null,null,"任务结束",null,"无","L5KYPHC_ZHSTOP_TASK_END",{"$nulls":3},"get",null,null,"FIX.YT6022_IN_TASK1_FINISH.F_CV      1\nFIX.YT6022_TASK1_NODEA.F_CV      1\nFIX.YT6022_TASK1_ROUTE.F_CV      1",null,null,"writevalue 1, \"Fix32.THISNODE.YT6022_IN_TASK1_FINISH.F_CV\", 1\nwritevalue 0, \"Fix32.THISNODE.YT6022_TASK1_NODEA.F_CV\", 1\nwritevalue 0, \"Fix32.THISNODE.YT6022_TASK1_ROUTE.F_CV\", 1\n"]
[null,null,"批次清零",null,"无","L5KYPHC_ZHSTOP_CLEAR_BATCH","JK_YT6022_MIXENTPC_CLEAR","JK_YT6022_MIXENTPC_UNITERR",null,"get",null,null,"FIX.JK_YT6022_MIXENTPC_CLEAR.F_CV  1\nFIX.JK_YT6022_MIXENTPC_UNITERR.F_CV  输出\n",null,null,"\nFix32.THISNODE.YT6022_3374_CLEAR.F_CV=1/称3374清零\nFix32.THISNODE.YT6022_2123_CLEAR.F_CV=1/称2123清零\nFix32.THISNODE.YT6022_2113_CLEAR.F_CV = 1/称2113清零\nFix32.THISNODE.YT6022_C_SJ2116_STUFF_CL1.F_CV = 1/2116前加水量累计清\nFix32.THISNODE.YT6022_C_SJ2116_STUFF_CL2.F_CV = 1/2116后加水量累计清\nFix32.THISNODE.YT6022_C_WQ2126_STUFF_CL1.F_CV = 1/2116前加水量累计清\nFix32.THISNODE.YT6022_C_WQ2126_STUFF_CL2.F_CV = 1/2116后加水量累计清？？？现在没有\n\n\n"]
[null,null,"生产清零？？",null,"无","L5KYPHC_ZHSTOP_CLEAR_PRODINFO","JK_YT6022_MIXENTSC_CLEAR","JK_YT6022_MIXENTSC_UNITERR",null,"get",null,null,"FIX.JK_YT6022_MIXENTSC_CLEAR.F_CV  1\nFIX.JK_YT6022_MIXENTSC_UNITERR.F_CV  输出",null,null,"WriteValue \"\", \"FIX32.THISNODE.YT6022_MIXBATCHNO.A_CV\", 2 /预混段当前批次号\nWriteValue \"0\", \"FIX32.THISNODE.YT6022_MIXBATCHSEQ.F_CV\", 2 /批次顺序\nWriteValue \"\", \"FIX32.THISNODE.YT6022_MIXBRAND.A_CV\", 2  /预混段当前牌号\nWriteValue \"\", \"FIX32.THISNODE.YT6022_MIXENTRYID.A_CV\", 2 /EntryID\nWriteValue \"\", \"FIX32.THISNODE.YT6022_MIXINGP1.A_CV\", 2 /预计入柜号1\nWriteValue \"0\", \"FIX32.THISNODE.YT6022_MIXINGP1AMOUNT.F_CV\", 2/入1柜料量\nWriteValue \"\", \"FIX32.THISNODE.YT6022_MIXINGP2.A_CV\", 2/预计入柜号2\nWriteValue \"0\", \"FIX32.THISNODE.YT6022_MIXINGP2AMOUNT.F_CV\", 2/入2柜料量\nWriteValue \"\", \"FIX32.THISNODE.YT6022_MIXINGP3.A_CV\", 2/预计入柜号3\nWriteValue \"0\", \"FIX32.THISNODE.YT6022_MIXINGP3AMOUNT.F_CV\", 2/入3柜料量\nWriteValue \"0\", \"FIX32.THISNODE.YT6022_MIXINGPQTY.F_CV\", 2/生成物料入的柜子数量\nWriteValue \"\", \"FIX32.THISNODE.YT6022_MIXJHJSSJ.A_CV\", 2/预混段计划结束时间\nWriteValue \"\", \"FIX32.THISNODE.YT6022_MIXJHKSSJ.A_CV\", 2/预混段计划开始时间\nWriteValue \"\", \"FIX32.THISNODE.YT6022_MIXOUTGP.A_CV\", 2/预混段出柜号\nWriteValue \"0\", \"FIX32.THISNODE.YT6022_MIXPRODMIX.F_CV\", 2/产出物是否汇集\nWriteValue \"0\", \"FIX32.THISNODE.YT6022_MIXROAD.F_CV\", 2/生产工艺路线\nWriteValue \"\", \"FIX32.THISNODE.YT6022_MIXSTUFFBRAND.A_CV\", 2/预混段当前料液牌号\nWriteValue \"0\", \"FIX32.THISNODE.YT6022_MIXWEIGHT.F_CV\", 2/预混段当前重量","\n"]
[null,null,"预配柜进柜路径清零【确认】",null,"无","L5KYPHC_ZHSTOP_CLEAR_YPGPATH","YT6022_TASK1_NODEA\n",null,null,"get",null,null,"FIX.YT6022_TASK1_NODEA.F_CV  0\nFIX.YT6022_TASK1_ROUTE.F_CV  0"]
[null,null,"预配柜信息清零【待定】",null,"无","L5KYPHC_ZHSTOP_CLEAR_YPGINFO",{"$nulls":3},"get"]
[null,null,"设备组合停止",null,"无","L5KYPHC_ZHSTOP_STOP","YT6022_IN_TASK1_STOP",null,null,"get",null,null,"FIX.YT6022_IN_TASK1_STOP.F_CV  1"]
[null,"辅助操作","单机/联机【待定】","需根据昆船系统的单机/联机功能把所有段都单独封装","段号","L5KYPHC_FK_DeviceLink(string DeviceName,Bool Bsel)???",{"$nulls":3},"post",{"$nulls":3},"建议放到6月份之后再梳理","建议放到6月份之后再梳理"]
[null,null,"故障复位","参考昆船原的功能？","无","L5KYPHC_FK_AlarmReset","YT6022_CONTROL_YT6022_RESET",null,null,"get",null,null,"FIX.YT6022_CONTROL_YT6022_RESET.F_CV  1"]
[]
[{"$nulls":4},"5000叶片线WQ2选择[]","L5KYPHC_WQ2_SLELECT","YT6022_WQ2_SEL",{"$nulls":6},1,"NO"]

{"sheet":"加料","index":1,"n_rows":52,"n_cols":17,"rows_kept":52,"merged":[[1,0,51,0],[1,1,4,1],[5,1,12,1],[13,1,23,1],[24,1,26,1],[27,1,49,1],[28,2,38,2],[40,2,48,2],[50,1,51,1]],"flags":["formulas_cached_only"]}
["工序","操作按钮","组件封装","业务说明","参数说明","API接口名","API请求方式","API传入参数","API接口检查点位","API接口写入点","触发脚本","备注","API状态","IFIX点位","代码生成","配置文件","代码标记"]
["5千加料","设备预热","预热启动",null,"无","L5KYPJL_SBYR_START","get",null,null,"FIX.YT6022_C_SJ2147_PREHEAT_START.F_CV 1\nFIX.YT6022_C_SJ2147_PREHEAT_STOP.F_CV 0","      Fix32.THISNODE.YT6022_C_SJ2147_PREHEAT_START.F_CV = 1\n      Fix32.THISNODE.YT6022_C_SJ2147_PREHEAT_STOP.F_CV = 0",null,null,"YT6022_C_SJ2147_PREHEAT_START\n","case \"api/L5KYPJL_SBYR_START\":  //预热启动\n                    rlt = AppUtil.WriteFunction(AppUtil.GetConfig(ModuleEnum.JL),\"L5KYPJL_SBYR_START\"); \n                    break;",{"$error":"#REF!"}]
[null,null,"预热温度值设定",null,"温度值","L5KYPJL_SBYR_YRWDSET(float Temp)","post","36  【整数】",null,"FIX.YT6022_VALUE_SJ2147_P_SET_1.F_CV 输出","Fix32.THISNODE.YT6022_VALUE_SJ2147_P_SET_1.F_CV",null,null,"YT6022_VALUE_SJ2147_P_SET_1",{"$error":"#REF!"},null,"post"]
[null,null,"预热生产温度值设定",null,"温度值","L5KYPJL_SBYR_YXWDSET(float Temp)","post","36  【整数】",null,"FIX.YT6022_VALUE_SJ2147_PID1_SP.F_CV  输出","Fix32.THISNODE.YT6022_VALUE_SJ2147_PID1_SP.F_CV",null,null,"YT6022_VALUE_SJ2147_PID1_SP",{"$error":"#REF!"},null,"post"]
[null,null,"预热结束",null,"无","L5KYPJL_SBYR_CLOSE","get",null,null,"FIX.YT6022_C_SJ2147_PREHEAT_START.F_CV  0\nFIX.YT6022_C_SJ2147_PREHEAT_STOP.F_CV  1","       Fix32.THISNODE.YT6022_C_SJ2147_PREHEAT_START.F_CV = 0\n       Fix32.THISNODE.YT6022_C_SJ2147_PREHEAT_STOP.F_CV = 1",null,null,"\nYT6022_C_SJ2147_PREHEAT_STOP","case \"api/L5KYPJL_SBYR_CLOSE\":  //预热结束\n                    rlt = AppUtil.WriteFunction(AppUtil.GetConfig(ModuleEnum.JL),\"L5KYPJL_SBYR_CLOSE\"); \n                    break;",{"$error":"#REF!"}]
[null,"要料","料筒选择-料筒1",null,"无","L5KYPJL_YL_Tank1Select","get",null,null,"FIX.YT6022_SJ2147_TANK1_SEL.F_CV  1\nFIX.YT6022_SJ2147_TANK2_SEL.F_CV  0","\n       Fix32.THISNODE.YT6022_SJ2147_TANK1_SEL.F_CV = 1\n       Fix32.THISNODE.YT6022_SJ2147_TANK2_SEL.F_CV = 0",null,null,"YT6022_SJ2147_TANK1_SEL\n        ","case \"api/L5KYPJL_YL_Tank1Select\":  //料筒选择-料筒1\n                    rlt = AppUtil.WriteFunction(AppUtil.GetConfig(ModuleEnum.JL),\"L5KYPJL_YL_Tank1Select\"); \n                    break;",{"$error":"#REF!"}]
[null,null,"料筒选择-料筒2",null,"无","L5KYPJL_YL_Tank2Select","get",null,null,"FIX.YT6022_SJ2147_TANK2_SEL.F_CV  1\nFIX.YT6022_SJ2147_TANK1_SEL.F_CV  0","       Fix32.THISNODE.YT6022_SJ2147_TANK2_SEL.F_CV = 1\n       Fix32.THISNODE.YT6022_SJ2147_TANK1_SEL.F_CV = 0",null,null,"YT6022_SJ2147_TANK2_SEL\n         ","case \"api/L5KYPJL_YL_Tank2Select\":  //料筒选择-料筒2\n                    rlt = AppUtil.WriteFunction(AppUtil.GetConfig(ModuleEnum.JL),\"L5KYPJL_YL_Tank2Select\"); \n                    break;",{"$error":"#REF!"}]
[null,null,"要料信息下发-料筒1",null,"料液重量、料液代码、批次号","L5KYPJL_YL_Tank1Info_Set(object info)","post","{\"Weight\":1200,\"BrandNo\":\"sdfsf\",BatchNo:\"sfsdfsdf\"}",null,"FIX.YT6022_SJ2147Tank1AskQty.F_CV  （重量）\nFIX.YT6022_SJ2147Tank1AskBrand.A_CV  （代码）FIX.YT6022_SJ2147Tank1AskBatch.A_CV  （批次）",{"$nulls":3},"YT6022_SJ2147Tank1AskQty（重量）\n/YT6022_SJ2147Tank1AskBrand（代码）\n/YT6022_SJ2147Tank1AskBatch（批次）",{"$error":"#REF!"},null,"post"]
[null,null,"要料信息下发-料筒2",null,"料液重量、料液代码、批次号","L5KYPJL_YL_Tank2Info_Set(object info)","post","{\"Weight\":1200,\"BrandNo\":\"sdfsf\",BatchNo:\"sfsdfsdf\"}",null,"FIX.YT6022_SJ2147Tank2AskQty.F_CV（重量）\nFIX.YT6022_SJ2147Tank2AskBrand.A_CV（代码）\nFIX.YT6022_SJ2147Tank2AskBatch.A_CV（批次）",{"$nulls":3},"YT6022_SJ2147Tank2AskQty（重量）\n/YT6022_SJ2147Tank2AskBrand（代码）\n/YT6022_SJ2147Tank2AskBatch（批次）",{"$error":"#REF!"},null,"post"]
[null,null,"要料请求-料筒1",null,"无","L5KYPJL_YL_Tank1_Set","get",null,null,"FIX.YT6022_SJ2147_TANK1_REQUEST.F_CV 1","if Fix32.THISNODE.YT6022_SJ2147_TANK1_REUSING.F_CV = 0 and Fix32.THISNODE.YT6022_SJ2147_TANK1_CLEARING.F_CV = 0 and Fix32.THISNODE.YT6022_SJ2147_PIPE1_BACK.F_CV = 0  then\nif  Fix32.THISNODE.YT6022_SJ2147Tank1AskBrand.A_CV <> \"\"\n   Fix32.THISNODE.YT6022_SJ2147Tank1AskBatch.A_CV = ComboBox1.Text\n   Fix32.THISNODE.YT6022_SJ2147Tank1AskBrand.A_CV = ComboBox2.Text\n   Fix32.THISNODE.YT6022_SJ2147Tank1AskQty.f_cv = TextBox1.Text\n   Fix32.THISNODE.YT6022_SJ2147_TANK1_REQUEST.f_cv = 1",null,null,"YT6022_SJ2147_TANK1_REQUEST"]
[null,null,"要料请求-料筒2",null,"无","L5KYPJL_YL_Tank2_Set","get",null,null,"FIX.YT6022_SJ2147_TANK2_REQUEST.F_CV  1","if  Fix32.THISNODE.YT6022_SA2224_PIPE2_SPAYING.F_CV = 0 and Fix32.THISNODE.YT6022_SA2224_TANK2_CLEARING.F_CV = 0 and Fix32.THISNODE.YT6022_SA2224_PIPE2_BACK.F_CV = 0  then\n if    Fix32.THISNODE.YT6022_SJ2147Tank2AskBatch.A_CV = ComboBox3.Text\n   Fix32.THISNODE.YT6022_SJ2147Tank2AskBrand.A_CV = ComboBox4.Text\n   Fix32.THISNODE.YT6022_SJ2147Tank2AskQty.f_cv = TextBox2.Text\n   Fix32.THISNODE.YT6022_SJ2147_TANK2_REQUEST.f_cv = 1",null,null,"YT6022_SJ2147_TANK2_REQUEST"]
[null,null,"取消要料-料筒1",null,"无","L5KYPJL_YL_Tank1Cancel","get",null,null,"FIX.YT6022_SJ2147_TANK1_REQUEST.F_CV 0","FIX.YT6022_SJ2147_TANK1_REQUEST.F_CV 0",null,null,"YT6022_SJ2147_TANK1_REQUEST","case \"api/L5KYPJL_YL_Tank1Cancel\":  //取消要料-料筒1\n                    rlt = AppUtil.WriteFunction(AppUtil.GetConfig(ModuleEnum.JL),\"L5KYPJL_YL_Tank1Cancel\"); \n                    break;",{"$error":"#REF!"}]
[null,null,"取消要料-料筒2",null,"无","L5KYPJL_YL_Tank2Cancel","get",null,null,"FIX.YT6022_SJ2147_TANK2_REQUEST.F_CV 0","FIX.YT6022_SJ2147_TANK2_REQUEST.F_CV 0",null,null,"YT6022_SJ2147_TANK2_REQUEST","case \"api/L5KYPJL_YL_Tank2Cancel\":  //取消要料-料筒2\n                    rlt = AppUtil.WriteFunction(AppUtil.GetConfig(ModuleEnum.JL),\"L5KYPJL_YL_Tank2Cancel\"); \n                    break;",{"$error":"#REF!"}]
[null,"组合启动","工单信息下发",null,"工单号、批次号、牌号","L5KYPJL_ZHStart_GDInfoSet(string YPno,string BatchNo,string BrandNo)","post","{\"YPNo\":1200,\"BatchNo\":\"sdfsf\",BrandNo:\"sfsdfsdf\"}",null,"FIX.YT6022_LeafEntryID.A_CV （工单）\nFIX.YT6022_LeafBatchNo.A_CV （批次）\nFIX.YT6022_LeafBrand.A_CV （牌号）",{"$nulls":3},"YT6022_LeafEntryID（工单）\n/YT6022_LeafBatchNo（批次）\n/YT6022_LeafBrand（牌号）","case \"api/L5KYPJL_ZHStart_GDInfoSet(string YPno,string BatchNo,string BrandNo)\":  //工单信息下发\n                    rlt = AppUtil.WriteFunction(AppUtil.GetConfig(ModuleEnum.JL),\"L5KYPJL_ZHStart_GDInfoSet(string YPno,string BatchNo,string BrandNo)\"); \n                    break;",{"$error":"#REF!"},"MUL"]
[null,null,"批开始",null,"无","L5KYPJL_ZHStart_BatchStart","get",null,null,"FIX.YT6022_TASK2_bSTART.F_CV  1\nFIX.YT6022_TASK2_bSTOP.F_CV  0","     Fix32.THISNODE.YT6022_TASK2_bSTART.F_CV = 1\n     Fix32.THISNODE.YT6022_TASK2_bSTOP.F_CV = 0",null,null,"YT6022_TASK2_bSTART\n  ","case \"api/L5KYPJL_ZHStart_BatchStart\":  //批开始\n                    rlt = AppUtil.WriteFunction(AppUtil.GetConfig(ModuleEnum.JL),\"L5KYPJL_ZHStart_BatchStart\"); \n                    break;",{"$error":"#REF!"}]
[null,null,"出预配柜条件验证",null,"柜号","L5KYPJL_ZHStart_OutYPGCheck(string YPGno)","post","YP04/YP05/YP06/YP07","JK_YT6022_YP04_OUT_UNITERR\nJK_YT6022_YP05_OUT_UNITERR\nJK_YT6022_YP06_OUT_UNITERR\nJK_YT6022_YP07_OUT_UNITERR","FIX.JK_YT6022_TASK1_B04.F_CV 1\nFIX.JK_YT6022_TASK1_B03.F_CV 1\nFIX.JK_YT6022_TASK1_B02.F_CV 1\nFIX.JK_YT6022_TASK1_B01.F_CV 1",{"$nulls":3},"YP04/JK_YT6022_TASK1_B04\nYP05/JK_YT6022_TASK1_B03\nYP06/JK_YT6022_TASK1_B02\nYP07/JK_YT6022_TASK1_B01",{"$error":"#REF!"},null,"post"]
[null,null,"出预配柜取消",null,"柜号","L5KYPJL_ZHStart_OutYPGCancel(string YPno)","post","YP04/YP05/YP06/YP07",null,"FIX.YT6022_task2_B04.F_CV   0\nFIX.YT6022_task2_B03.F_CV   0\nFIX.YT6022_task2_B02.F_CV   0\nFIX.YT6022_task2_B01.F_CV   0","YP07/writevalue 0, \"Fix32.THISNODE.YT6022_task2_B01.F_CV\", 1\nYP06/writevalue 0, \"Fix32.THISNODE.YT6022_task2_B02.F_CV\", 1\nYP05/writevalue 0, \"Fix32.THISNODE.YT6022_task2_B03.F_CV\", 1\nYP04/writevalue 0, \"Fix32.THISNODE.YT6022_task2_B04.F_CV\", 1\n",null,null,"YP07/YT6022_task2_B01\nYP06/YT6022_task2_B02\nYP05/YT6022_task2_B03\nYP04/YT6022_task2_B04"]
[null,null,"出预配柜信息下发（待定）",null,"柜号","L5KYPJL_ZHStart_OutPGInfoSet(string YPGno)","post","YP04/YP05/YP06/YP07",null,"YT6022_GP_2139R_JOB(YP04批次)\n/YT6022_GP_2139R_BRAND（牌号）\nYT6022_GP_2139L_JOB(YP05批次)\n/YT6022_GP_2139L_BRAND（牌号）\nYT6022_GP_2138R_JOB(YP06批次)\n/YT6022_GP_2138R_BRAND（牌号）\nYT6022_GP_2138L_JOB(YP07批次)\n/YT6022_GP_2138L_BRAND（牌号）",{"$nulls":3},"YT6022_GP_2139R_JOB(YP04批次)\n/YT6022_GP_2139R_BRAND（牌号）\nYT6022_GP_2139L_JOB(YP05批次)\n/YT6022_GP_2139L_BRAND（牌号）\nYT6022_GP_2138R_JOB(YP06批次)\n/YT6022_GP_2138R_BRAND（牌号）\nYT6022_GP_2138L_JOB(YP07批次)\n/YT6022_GP_2138L_BRAND（牌号）",{"$error":"#REF!"},null,"post"]
[null,null,"启用生产关联",null,"无","L5KYPJL_REF_START","get",null,null,"   FIX.YT630_IN_TASK2_LINK.F_CV  1   ",{"$nulls":3},"  YT630_IN_TASK2_LINK"]
[null,null,"取消生产关联",null,"无","L5KYPJL_REF_CANCEL","get",null,null,"   FIX.YT630_IN_TASK2_LINK.F_CV  0",{"$nulls":3},"  YT630_IN_TASK2_LINK"]
[null,null,"进叶柜条件验证",null,"柜号","L5KYPJL_ZHStart_InYGCheck(string YGno）","post","YG01~YG24","JK_YT630_A1_IN_UnitErr  读1正常\nJK_YT630_A2_IN_UnitErr\nJK_YT630_A3_IN_UnitErr\nJK_YT630_A4_IN_UnitErr\nJK_YT630_A5_IN_UnitErr\nJK_YT630_A6_IN_UnitErr\nJK_YT630_A7_IN_UnitErr\nJK_YT630_A8_IN_UnitErr\nJK_YT630_A9_IN_UnitErr\nJK_YT630_A10_IN_UnitErr\nJK_YT630_A11_IN_UnitErr\nJK_YT630_A12_IN_UnitErr\nJK_YT630_A13_IN_UnitErr\nJK_YT630_A14_IN_UnitErr\nJK_YT630_A15_IN_UnitErr\nJK_YT630_A16_IN_UnitErr\nJK_YT630_A17_IN_UnitErr\nJK_YT630_A18_IN_UnitErr\nJK_YT630_A19_IN_UnitErr\nJK_YT630_A20_IN_UnitErr\n","Fix32.THISNODE.JK_YT630_IN_TASK2.F_CV",{"$nulls":3},"YG02/JK_YT630_IN_task2_A01 （写1）\nYG04/JK_YT630_IN_task2_A02\nYG06/JK_YT630_IN_task2_A03\nYG08/JK_YT630_IN_task2_A04\nYG10/JK_YT630_IN_task2_A05\nYG12/JK_YT630_IN_task2_A06\nYG14/JK_YT630_IN_task2_A07\nYG16/JK_YT630_IN_task2_A08\nYG01/JK_YT630_IN_task2_A09\nYG03/JK_YT630_IN_task2_A10\nYG05/JK_YT630_IN_task2_A11\nYG07/JK_YT630_IN_task2_A12\nYG09/JK_YT630_IN_task2_A13\nYG11/JK_YT630_IN_task2_A14\nYG13/JK_YT630_IN_task2_A15\nYG15/JK_YT630_IN_task2_A16\nYG18/JK_YT630_IN_task2_A17\nYG20/JK_YT630_IN_task2_A18\nYG22/JK_YT630_IN_task2_A19\nYG24/JK_YT630_IN_task2_A20",{"$error":"#REF!"},null,"post"]
[null,null,"进页柜取消",null,"柜号","L5KYPJL_ZHStart_InYGCancel(string YGno）","post","YG01~YG24",null,"YG02/YT630_IN_task2_A01.F_CV （写0）\nYG04/YT630_IN_task2_A02\nYG06/YT630_IN_task2_A03\nYG08/YT630_IN_task2_A04\nYG10/YT630_IN_task2_A05\nYG12/YT630_IN_task2_A06\nYG14/YT630_IN_task2_A07\nYG16/YT630_IN_task2_A08\nYG01/YT630_IN_task2_A09\nYG03/YT630_IN_task2_A10\nYG05/YT630_IN_task2_A11\nYG07/YT630_IN_task2_A12\nYG09/YT630_IN_task2_A13\nYG11/YT630_IN_task2_A14\nYG13/YT630_IN_task2_A15\nYG15/YT630_IN_task2_A16\nYG18/YT630_IN_task2_A17\nYG20/YT630_IN_task2_A18\nYG22/YT630_IN_task2_A19\nYG24/YT630_IN_task2_A20",{"$nulls":3},"YG02/JK_YT630_IN_task2_A01 （写0）\nYG04/JK_YT630_IN_task2_A02\nYG06/JK_YT630_IN_task2_A03\nYG08/JK_YT630_IN_task2_A04\nYG10/JK_YT630_IN_task2_A05\nYG12/JK_YT630_IN_task2_A06\nYG14/JK_YT630_IN_task2_A07\nYG16/JK_YT630_IN_task2_A08\nYG01/JK_YT630_IN_task2_A09\nYG03/JK_YT630_IN_task2_A10\nYG05/JK_YT630_IN_task2_A11\nYG07/JK_YT630_IN_task2_A12\nYG09/JK_YT630_IN_task2_A13\nYG11/JK_YT630_IN_task2_A14\nYG13/JK_YT630_IN_task2_A15\nYG15/JK_YT630_IN_task2_A16\nYG18/JK_YT630_IN_task2_A17\nYG20/JK_YT630_IN_task2_A18\nYG22/JK_YT630_IN_task2_A19\nYG24/JK_YT630_IN_task2_A20"]
[null,null,"进叶柜信息下发",null,"柜号、批次号、牌号","L5KYPJL_ZHStart_InYgInfoSet(string YGNo,string BatchNo,string BrandNo)","post","{\"YGNo\":\"YG01\",\"BatchNo\":\"sdfsf\",BrandNo:\"sfsdfsdf\"}",null,"YG01/YT630_1129A_JOB.A_CV（批次）/YT630_1129A_BRAND（牌号）（A_CV）\nYG02/YT630_1129_JOB/YT630_1129_BRAND\nYG03/YT630_1129_1A_JOB/YT630_1129_1A_BRAND\nYG04/YT630_1129_1_JOB/YT630_1129_1_BRAND\nYG05/YT630_1129_2A_JOB/YT630_1129_2A_BRAND\nYG06/YT630_1129_2_JOB/YT630_1129_2_BRAND\nYG07/YT630_1129_3A_JOB/YT630_1129_3A_BRAND\nYG08/YT630_1129_3_JOB/YT630_1129_3_BRAND\nYG09/YT630_1129_4A_JOB/YT630_1129_4A_BRAND\nYG10/YT630_1129_4_JOB/YT630_1129_4_BRAND\nYG11/YT630_1129_5A_JOB/YT630_1129_5A_BRAND\nYG12/YT630_1129_5_JOB/YT630_1129_5_BRAND\nYG13/YT630_1129_6A_JOB/YT630_1129_6A_BRAND\nYG14/YT630_1129_6_JOB/YT630_1129_6_BRAND\nYG15/YT630_1129_7A_JOB/YT630_1129_7A_BRAND\nYG16/YT630_1129_7_JOB/YT630_1129_7_BRAND\nYG18/YT630_1153_JOB/YT630_1153_BRAND\nYG20/YT630_1153_1_JOB/YT630_1153_1_BRAND\nYG22/YT630_1153_2_JOB/YT630_1153_2_BRAND\nYG24/YT630_1153_3_JOB/YT630_1153_3_BRAND",{"$nulls":3},"YG01/YT630_1129A_JOB（批次）/YT630_1129A_BRAND（牌号）\nYG02/YT630_1129_JOB/YT630_1129_BRAND\nYG03/YT630_1129_1A_JOB/YT630_1129_1A_BRAND\nYG04/YT630_1129_1_JOB/YT630_1129_1_BRAND\nYG05/YT630_1129_2A_JOB/YT630_1129_2A_BRAND\nYG06/YT630_1129_2_JOB/YT630_1129_2_BRAND\nYG07/YT630_1129_3A_JOB/YT630_1129_3A_BRAND\nYG08/YT630_1129_3_JOB/YT630_1129_3_BRAND\nYG09/YT630_1129_4A_JOB/YT630_1129_4A_BRAND\nYG10/YT630_1129_4_JOB/YT630_1129_4_BRAND\nYG11/YT630_1129_5A_JOB/YT630_1129_5A_BRAND\nYG12/YT630_1129_5_JOB/YT630_1129_5_BRAND\nYG13/YT630_1129_6A_JOB/YT630_1129_6A_BRAND\nYG14/YT630_1129_6_JOB/YT630_1129_6_BRAND\nYG15/YT630_1129_7A_JOB/YT630_1129_7A_BRAND\nYG16/YT630_1129_7_JOB/YT630_1129_7_BRAND\nYG18/YT630_1153_JOB/YT630_1153_BRAND\nYG20/YT630_1153_1_JOB/YT630_1153_1_BRAND\nYG22/YT630_1153_2_JOB/YT630_1153_2_BRAND\nYG24/YT630_1153_3_JOB/YT630_1153_3_BRAND",{"$error":"#REF!"},null,"post"]
[null,null,"设备组合启动",null,"无","L5KYPJL_ZHStart_Start","get",null,null,"     THISNODE.YT630_IN_TASK2_START.F_CV  1\n     THISNODE.YT6022_IN_TASK2_START.F_CV  1","      Fix32.THISNODE.YT630_IN_TASK2_START.F_CV = 1\n       Fix32.THISNODE.YT6022_IN_TASK2_START.F_CV = 1",null,null,"    YT630_IN_TASK2_START\n    YT6022_IN_TASK2_START","case \"api/L5KYPJL_ZHStart_Start\":  //设备组合启动\n                    rlt = AppUtil.WriteFunction(AppUtil.GetConfig(ModuleEnum.JL),\"L5KYPJL_ZHStart_Start\"); \n                    break;",{"$error":"#REF!"}]
[null,"生产提升","生产提升",null,"无","L5KYPJL_TS_TSStart","get",null,null,"YT6022_WPL2141_ASEND.F_CV  1",{"$nulls":3},"YT6022_WPL2141_ASEND","case \"api/L5KYPJL_TS_TSStart\":  //生产提升\n                    rlt = AppUtil.WriteFunction(AppUtil.GetConfig(ModuleEnum.JL),\"L5KYPJL_TS_TSStart\"); \n                    break;",{"$error":"#REF!"}]
[null,null,"强制提升",null,"无","L5KYPJL_TS_TSForceStart","get",null,null,"YT6022_WPL2141_FORCEASEND.F_CV  1",{"$nulls":3},"YT6022_WPL2141_FORCEASEND","case \"api/L5KYPJL_TS_TSForceStart\":  //强制提升\n                    rlt = AppUtil.WriteFunction(AppUtil.GetConfig(ModuleEnum.JL),\"L5KYPJL_TS_TSForceStart\"); \n                    break;",{"$error":"#REF!"}]
[null,null,"强制停止提升",null,"无","L5KYPJL_TS_TSForceStop","get",null,null,"YT6022_WPL2141_FORCESTOP.F_CV  1",{"$nulls":3},"YT6022_WPL2141_FORCESTOP","case \"api/L5KYPJL_TS_TSForceStop\":  //强制停止提升\n                    rlt = AppUtil.WriteFunction(AppUtil.GetConfig(ModuleEnum.JL),\"L5KYPJL_TS_TSForceStop\"); \n                    break;",{"$error":"#REF!"}]
[null,"组合停止","批结束",null,"无","L5KYPJL_ZHStop_BatchEnd","get",null,null,"     FIX.YT6022_TASK2_bSTOP.F_CV  1\n     FIX.YT6022_TASK2_bSTART.F_CV  0","     Fix32.THISNODE.YT6022_TASK2_bSTOP.F_CV = 1\n     Fix32.THISNODE.YT6022_TASK2_bSTART.F_CV = 0",null,null,"  YT6022_TASK2_bSTOP\n  YT6022_TASK2_bSTART","case \"api/L5KYPJL_ZHStop_BatchEnd\":  //批结束\n                    rlt = AppUtil.WriteFunction(AppUtil.GetConfig(ModuleEnum.JL),\"L5KYPJL_ZHStop_BatchEnd\"); \n                    break;",{"$error":"#REF!"}]
[null,null,"余料回收","管路余料回到料筒","无","L5KYPJL_ZHStopRec_Pipe_InTank","get",null,null,"     FIX.YT6022_SJ2147_PIPE_CLEAR.F_CV  0\n     FIX.YT6022_SJ2147_PIPE_REUSE.F_CV  1","if  Fix32.THISNODE.YT6022_STATE_SJ2147_PREFILL.F_CV = 0 and Fix32.THISNODE.YT6022_STATE_SJ2147_WORK.F_CV = 0 and Fix32.THISNODE.YT6022_SA2224_TANK2_CLEA.F_CV = 0 and Fix32.THISNODE.YT6022_SA2224_TANK2_SPA.F_CV = 0  then\nFix32.THISNODE.YT6022_SJ2147_PIPE_CLEAR.f_cv = 0\n     Fix32.THISNODE.YT6022_SJ2147_PIPE_REUSE.f_cv = 1",null,null,"YT6022_SJ2147_PIPE_REUSE","case \"api/L5KYPJL_ZHStopRec_Pipe_InTank\":  //余料回收\n                    rlt = AppUtil.WriteFunction(AppUtil.GetConfig(ModuleEnum.JL),\"L5KYPJL_ZHStopRec_Pipe_InTank\"); \n                    break;",{"$error":"#REF!"}]
[{"$nulls":3},"管路余料取消回到料筒","无","L5KYPJL_ZHStopRec_Pipe_InTankCANCEL","get",null,null,"     FIX.YT6022_SJ2147_PIPE_CLEAR.F_CV  0\n     FIX.YT6022_SJ2147_PIPE_REUSE.F_CV  0","     Fix32.THISNODE.YT6022_SJ2147_PIPE_CLEAR.f_cv = 0\n     Fix32.THISNODE.YT6022_SJ2147_PIPE_REUSE.f_cv = 0",null,null,"YT6022_SJ2147_PIPE_REUSE"]
[{"$nulls":3},"回料到料房-料筒1","无","L5KYPJL_ZHStopRec_Tank1_InMRoom","get",null,null,"     FIX.YT6022_SJ2147_TANK1_REQUEST.F_CV  0\n     FIX.YT6022_SJ2147_TANK1_CLEAR_S.F_CV  0\n     FIX.YT6022_SJ2147_TANK1_REUSE.F_CV  1","     Fix32.THISNODE.YT6022_SJ2147_TANK1_REQUEST.f_cv = 0\n     Fix32.THISNODE.YT6022_SJ2147_TANK1_CLEAR_S.f_cv = 0\n     Fix32.THISNODE.YT6022_SJ2147_TANK1_REUSE.f_cv = 1","(取消回料？)",null,"YT6022_SJ2147_TANK1_REUSE","case \"api/L5KYPJL_ZHStopRec_Tank1_InMRoom\":  //\n                    rlt = AppUtil.WriteFunction(AppUtil.GetConfig(ModuleEnum.JL),\"L5KYPJL_ZHStopRec_Tank1_InMRoom\"); \n                    break;",{"$error":"#REF!"}]
[{"$nulls":3},"取消回料到料房-料筒1",null,"L5KYPJL_ZHStopRec_Tank1_InMRoomCANCEL","get",null,null,"     FIX.YT6022_SJ2147_TANK1_REQUEST.F_CV  0\n     FIX.YT6022_SJ2147_TANK1_CLEAR_S.F_CV  0\n     FIX.YT6022_SJ2147_TANK1_REUSE.F_CV  0","     Fix32.THISNODE.YT6022_SJ2147_TANK1_REQUEST.f_cv = 0\n     Fix32.THISNODE.YT6022_SJ2147_TANK1_CLEAR_S.f_cv = 0\n     Fix32.THISNODE.YT6022_SJ2147_TANK1_REUSE.f_cv = 0",null,null,"YT6022_SJ2147_TANK1_REUSE"]
[{"$nulls":3},"回料到料房-料筒2","无","L5KYPJL_ZHStopRec_Tank2_InMRoom","get",null,null,"     FIX.YT6022_SJ2147_TANK2_REQUEST.F_CV  0\n     FIX.YT6022_SJ2147_TANK2_CLEAR_S.F_CV  0\n     FIX.YT6022_SJ2147_TANK2_REUSE.F_CV  1","Fix32.THISNODE.YT6022_SA2224_TANK2_ALLOW_IN.F_CV = 0 and Fix32.THISNODE.YT6022_SA2224_TANK2_CLEARING.F_CV = 0 and Fix32.THISNODE.YT6022_SA2224_PIPE2_BACK.F_CV = 0\n If Fix32.THISNODE.YT6022_SJ2147_TANK2_REUSE.f_cv = 1 Then\n   If MsgBox(\"确定要取消料桶2回料吗？\", vbYesNo, \"回料\") = vbYes Then\n     Fix32.THISNODE.YT6022_SJ2147_TANK2_REQUEST.f_cv = 0\n     Fix32.THISNODE.YT6022_SJ2147_TANK2_CLEAR_S.f_cv = 0\n     Fix32.THISNODE.YT6022_SJ2147_TANK2_REUSE.f_cv = 0\n     Call Modlogin.Oplog((0), (0), (1), \"取消料桶2回料\")\n   End If\n Else\n   If MsgBox(\"确定要料桶2回料吗？\", vbYesNo, \"回余料\") = vbYes Then\n     Fix32.THISNODE.YT6022_SJ2147_TANK2_REQUEST.f_cv = 0\n     Fix32.THISNODE.YT6022_SJ2147_TANK2_CLEAR_S.f_cv = 0\n     Fix32.THISNODE.YT6022_SJ2147_TANK2_REUSE.f_cv = 1\n   End If\n   Call Modlogin.Oplog((0), (0), (1), \"料桶2回料\")\n End If",null,null,"YT6022_SJ2147_TANK2_REUSE","case \"api/L5KYPJL_ZHStopRec_Tank2_InMRoom\":  //\n                    rlt = AppUtil.WriteFunction(AppUtil.GetConfig(ModuleEnum.JL),\"L5KYPJL_ZHStopRec_Tank2_InMRoom\"); \n                    break;",{"$error":"#REF!"}]
[{"$nulls":3},"取消回料到料房-料筒2","无","L5KYPJL_ZHStopRec_Tank2_InMRoomCANCEL","get",null,null,"     FIX.YT6022_SJ2147_TANK2_REQUEST.F_CV  0\n     FIX.YT6022_SJ2147_TANK2_CLEAR_S.F_CV  0\n     FIX.YT6022_SJ2147_TANK2_REUSE.F_CV  0",{"$nulls":3},"YT6022_SJ2147_TANK2_REUSE"]
[{"$nulls":3},"管路清洗","无","L5KYPJL_ZHStopRec_Pipe_Clear","get",null,null,"     FIX.YT6022_SJ2147_PIPE_REUSE.F_CV  0\n     FIX.YT6022_SJ2147_PIPE_CLEAR.F_CV  1","Fix32.THISNODE.YT6022_SA2224_TANK2_SPA.F_CV = 0\nIf Fix32.THISNODE.YT6022_SJ2147_PIPE_CLEAR.f_cv = 1 Then\n    If MsgBox(\"确定要取消清洗管路吗？\", vbYesNo, \"清洗管路\") = vbYes Then\n     Fix32.THISNODE.YT6022_SJ2147_PIPE_REUSE.f_cv = 0\n     Fix32.THISNODE.YT6022_SJ2147_PIPE_CLEAR.f_cv = 0\n     Call Modlogin.Oplog((0), (0), (1), \"取消清洗管路\")\n    End If\n  Else\n    If MsgBox(\"确定要清洗管路吗？\", vbYesNo, \"清洗管路\") = vbYes Then\n     Fix32.THISNODE.YT6022_SJ2147_PIPE_REUSE.f_cv = 0\n     Fix32.THISNODE.YT6022_SJ2147_PIPE_CLEAR.f_cv = 1\n     Call Modlogin.Oplog((0), (0), (1), \"清洗管路\")\n    End If\n  End If",null,null,"YT6022_SJ2147_PIPE_CLEAR","case \"api/L5KYPJL_ZHStopRec_Pipe_Clear\":  //\n                    rlt = AppUtil.WriteFunction(AppUtil.GetConfig(ModuleEnum.JL),\"L5KYPJL_ZHStopRec_Pipe_Clear\"); \n                    break;",{"$error":"#REF!"}]
[{"$nulls":3},"取消管路清洗","无","L5KYPJL_ZHStopRec_Pipe_ClearCANCEL","get",null,null,"    FIX.YT6022_SJ2147_PIPE_REUSE.F_CV  0\n     FIX.YT6022_SJ2147_PIPE_CLEAR.F_CV  0",{"$nulls":3},"YT6022_SJ2147_PIPE_CLEAR"]
[{"$nulls":3},"料筒清洗-料筒1","无","L5KYPJL_ZHStopRec_Tank1_Clear","get",null,null,"     FIX.YT6022_SJ2147_TANK1_REQUEST.F_CV  0\n     FIX.YT6022_SJ2147_TANK1_REUSE.F_CV 0\n     FIX.YT6022_SJ2147_TANK1_CLEAR_S.F_CV  1\n     FIX.YT6022_SJ2147Tank1Brand.A_CV \n     FIX.YT6022_SJ2147Tank1LotID2.A_CV \n     FIX.YT6022_SJ2147Tank1LotID1.A_CV  ","Fix32.THISNODE.YT6022_SJ2147_TANK1_REUSING.F_CV = 0 and Fix32.THISNODE.YT6022_SJ2147_TANK1_ALLOW_IN.F_CV = 0 and Fix32.THISNODE.YT6022_VALUE_SJ2147_P_CUR_16.F_CV < 10\n If Fix32.THISNODE.YT6022_SJ2147_TANK1_CLEAR_S.f_cv = 1 Then\n    If MsgBox(\"确定要取消清洗料桶吗？\", vbYesNo, \"清洗料桶\") = vbYes Then\n     Fix32.THISNODE.YT6022_SJ2147_TANK1_REQUEST.f_cv = 0\n     Fix32.THISNODE.YT6022_SJ2147_TANK1_REUSE.f_cv = 0\n     Fix32.THISNODE.YT6022_SJ2147_TANK1_CLEAR_S.f_cv = 0\n     Call Modlogin.Oplog((0), (0), (1), \"取消清洗料桶\")\n    End If\n  Else\n    If MsgBox(\"确定要清洗料桶吗？\", vbYesNo, \"清洗料桶\") = vbYes Then\n     Fix32.THISNODE.YT6022_SJ2147_TANK1_REQUEST.f_cv = 0\n     Fix32.THISNODE.YT6022_SJ2147_TANK1_REUSE.f_cv = 0\n     Fix32.THISNODE.YT6022_SJ2147_TANK1_CLEAR_S.f_cv = 1\n     Fix32.THISNODE.YT6022_SJ2147Tank1Brand.A_CV = \"\"\n     Fix32.THISNODE.YT6022_SJ2147Tank1LotID2.A_CV = \"\"\n     Fix32.THISNODE.YT6022_SJ2147Tank1LotID1.A_CV = \"\"\n     Call Modlogin.Oplog((0), (0), (1), \"清洗料桶\")\n    End If\n  End If",null,null,"YT6022_SJ2147_TANK1_CLEAR_S","case \"api/L5KYPJL_ZHStopRec_Tank1_Clear\":  //\n                    rlt = AppUtil.WriteFunction(AppUtil.GetConfig(ModuleEnum.JL),\"L5KYPJL_ZHStopRec_Tank1_Clear\"); \n                    break;",{"$error":"#REF!"}]
[{"$nulls":3},"料筒清洗取消-料筒1","无","L5KYPJL_ZHStopRec_Tank1_ClearCANCEL","get",null,null,"     FIX.YT6022_SJ2147_TANK1_REQUEST.F_CV  0\n     FIX.YT6022_SJ2147_TANK1_REUSE.F_CV  0\n     FIX.YT6022_SJ2147_TANK1_CLEAR_S.F_CV  0",{"$nulls":3},"YT6022_SJ2147_TANK1_CLEAR_S"]
[{"$nulls":3},"料筒清洗-料筒2","无","L5KYPJL_ZHStopRec_Tank2_Clear","get",null,null,"     FIX.YT6022_SJ2147_TANK2_REQUEST.F_CV  0\n     FIX.YT6022_SJ2147_TANK2_REUSE.F_CV  0\n     FIX.YT6022_SJ2147_TANK2_CLEAR_S.F_CV  1\n     FIX.YT6022_SJ2147Tank2Brand.A_CV \n     FIX.YT6022_SJ2147Tank2LotID1.A_CV \n     FIX.YT6022_SJ2147Tank2LotID2.A_CV  ","Fix32.THISNODE.YT6022_SA2224_TANK2_ALLOW_IN.F_CV = 0 and Fix32.THISNODE.YT6022_SA2224_PIPE2_SPAYING.F_CV = 0 and Fix32.THISNODE.YT6022_SA2224_PIPE2_CLEARING.F_CV = 0 and Fix32.THISNODE.YT6022_VALUE_SJ2147_P_CUR_17.F_CV < 10\n If Fix32.THISNODE.YT6022_SJ2147_TANK2_CLEAR_S.f_cv = 1 Then\n    If MsgBox(\"确定要取消清洗料桶吗？\", vbYesNo, \"清洗料桶\") = vbYes Then\n     Fix32.THISNODE.YT6022_SJ2147_TANK2_REQUEST.f_cv = 0\n     Fix32.THISNODE.YT6022_SJ2147_TANK2_REUSE.f_cv = 0\n     Fix32.THISNODE.YT6022_SJ2147_TANK2_CLEAR_S.f_cv = 0\n     Call Modlogin.Oplog((0), (0), (1), \"取消清洗料桶\")\n    End If\n  Else\n    If MsgBox(\"确定要清洗料桶吗？\", vbYesNo, \"清洗料桶\") = vbYes Then\n     Fix32.THISNODE.YT6022_SJ2147_TANK2_REQUEST.f_cv = 0\n     Fix32.THISNODE.YT6022_SJ2147_TANK2_REUSE.f_cv = 0\n     Fix32.THISNODE.YT6022_SJ2147_TANK2_CLEAR_S.f_cv = 1\n     Fix32.THISNODE.YT6022_SJ2147Tank2Brand.A_CV = \"\"\n     Fix32.THISNODE.YT6022_SJ2147Tank2LotID1.A_CV = \"\"\n     Fix32.THISNODE.YT6022_SJ2147Tank2LotID2.A_CV = \"\"\n     Call Modlogin.Oplog((0), (0), (1), \"清洗料桶\")\n    End If",null,null,"YT6022_SJ2147_TANK2_CLEAR_S","case \"api/L5KYPJL_ZHStopRec_Tank2_Clear\":  //\n                    rlt = AppUtil.WriteFunction(AppUtil.GetConfig(ModuleEnum.JL),\"L5KYPJL_ZHStopRec_Tank2_Clear\"); \n                    break;",{"$error":"#REF!"}]
[{"$nulls":3},"料筒清洗取消-料筒2","无","L5KYPJL_ZHStopRec_Tank2_ClearCANCEL","get",null,null,"     FIX.YT6022_SJ2147_TANK2_REQUEST.F_CV  0\n     FIX.YT6022_SJ2147_TANK2_REUSE.F_CV  0\n     FIX.YT6022_SJ2147_TANK2_CLEAR_S.F_CV  0",{"$nulls":3},"YT6022_SJ2147_TANK2_CLEAR_S"]
[null,null,"信息清零","批结束","无","L5KYPJL_ZHStopInfoClear_BatchEnd","get",null,null,"     FIX.YT6022_TASK2_bSTOP.F_CV  1\n     FIX.YT6022_TASK2_bSTART.F_CV  0","     Fix32.THISNODE.YT6022_TASK2_bSTOP.F_CV = 1\n     Fix32.THISNODE.YT6022_TASK2_bSTART.F_CV = 0\n  Fix32.THISNODE.YT6022_YSTJ.F_CV = Fix32.THISNODE.YT6022_YSTJ.F_CV + Fix32.THISNODE.YT6022_VALUE_SJ2147_W_P4.F_CV\n    ",null,null,"YT6022_TASK2_bSTOP","case \"api/L5KYPJL_ZHStopInfoClear_BatchEnd\":  //信息清零\n                    rlt = AppUtil.WriteFunction(AppUtil.GetConfig(ModuleEnum.JL),\"L5KYPJL_ZHStopInfoClear_BatchEnd\"); \n                    break;",{"$error":"#REF!"}]
[{"$nulls":3},"任务结束加料段","无","L5KYPJL_ZHStopInfoClear_TankClear","get",null,null,"FIX.YT6022_IN_TASK2_FINISH.F_CV 1\nFIX.YT6022_task2_NODEB.F_CV 1\nFIX.YT6022_task2_ROUTE.F_CV 1","\nwritevalue 1, \"Fix32.THISNODE.YT6022_IN_TASK2_FINISH.F_CV\", 1\nwritevalue 0, \"Fix32.THISNODE.YT6022_task2_NODEB.F_CV\", 1\nwritevalue 0, \"Fix32.THISNODE.YT6022_task2_ROUTE.F_CV\", 1",null,null,"YT6022_IN_TASK2_FINISH","case \"api/L5KYPJL_ZHStopInfoClear_TankClear\":  //\n                    rlt = AppUtil.WriteFunction(AppUtil.GetConfig(ModuleEnum.JL),\"L5KYPJL_ZHStopInfoClear_TankClear\"); \n                    break;",{"$error":"#REF!"}]
[{"$nulls":3},"进柜段任务结束","无","L5KYPJL_ZHStopInfoClear_TankEND","get",null,"   FIX.JK_YT630_IN_TASK2_FINISH_OK.F_CV 1","   FIX.JK_YT630_IN_TASK2_FINISH.F_CV 1","If MsgBox(\"是否任务结束？\", vbOKCancel + vbQuestion) = vbOK Then\n\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_A03.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_A01.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_A02.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_A04.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_A05.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_A06.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_A07.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_A08.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_A09.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_A10.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_A11.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_A12.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_A13.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_A14.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_A15.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_A16.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_A17.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_A18.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_A19.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_A20.F_CV\"\n\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_R04.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_R05.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_R06.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_R07.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_R08.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_R09.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_R10.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_R11.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_R14.F_CV\"\n\n\nEnd If\nCall Modlogin.Oplog((1), (0), (1), \"叶片进柜任务2—5000任务结束 \")\n",null,null,"FIX.YT630_IN_TASK2_A03.F_CV  0\nFIX.YT630_IN_TASK2_A01.F_CV\nFIX.YT630_IN_TASK2_A02.F_CV\nFIX.YT630_IN_TASK2_A04.F_CV\nFIX.YT630_IN_TASK2_A05.F_CV\nFIX.YT630_IN_TASK2_A06.F_CV\nFIX.YT630_IN_TASK2_A07.F_CV\nFIX.YT630_IN_TASK2_A08.F_CV\nFIX.YT630_IN_TASK2_A09.F_CV\nFIX.YT630_IN_TASK2_A10.F_CV\nFIX.YT630_IN_TASK2_A11.F_CV\nFIX.YT630_IN_TASK2_A12.F_CV\nFIX.YT630_IN_TASK2_A13.F_CV\nFIX.YT630_IN_TASK2_A14.F_CV\nFIX.YT630_IN_TASK2_A15.F_CV\nFIX.YT630_IN_TASK2_A16.F_CV\nFIX.YT630_IN_TASK2_A17.F_CV\nFIX.YT630_IN_TASK2_A18.F_CV\nFIX.YT630_IN_TASK2_A19.F_CV\nFIX.YT630_IN_TASK2_A20.F_CV\n"]
[{"$nulls":3},"批次清零","无","L5KYPJL_ZHStopInfoClear_BatchClear","get",null,"FIX.JK_YT6022_LEAFBPC_CLEAR_OK.F_CV 1","FIX.JK_YT6022_LEAFBPC_CLEAR.F_CV 1","\nFix32.THISNODE.YT6022_C_SJ2147_WATER_CLEAR.F_CV=1/累计加水量清零\n\nFix32.THISNODE.YT6022_2143_CLEAR.F_CV = 1/称2143清零\nFix32.THISNODE.YT6022_C_SJ2147_STUFF_CL1.F_CV = 1/加料机2147加料量累计清零",null,null,"JK_YT6022_LEAFBPC_CLEAR","case \"api/L5KYPJL_ZHStopInfoClear_BatchClear\":  //\n                    rlt = AppUtil.WriteFunction(AppUtil.GetConfig(ModuleEnum.JL),\"L5KYPJL_ZHStopInfoClear_BatchClear\"); \n                    break;",{"$error":"#REF!"}]
[{"$nulls":3},"生产清零","无","L5KYPJL_ZHStopInfoClear_ProdClear","get",null,"FIX.JK_YT6022_LEAFBSC_CLEAR_OK.F_CV 1","FIX.JK_YT6022_LEAFBSC_CLEAR.F_CV 1","WriteValue \"\", \"FIX32.THISNODE.YT6022_LEAFBATCHNO.A_CV\", 2 /叶片段当前批次号\nWriteValue \"0\", \"FIX32.THISNODE.YT6022_LEAFBATCHSEQ.F_CV\", 2 /批次顺序\nWriteValue \"\", \"FIX32.THISNODE.YT6022_LEAFBRAND.A_CV\", 2  /叶片段当前牌号\nWriteValue \"\", \"FIX32.THISNODE.YT6022_LEAFENTRYID.A_CV\", 2 /EntryID\nWriteValue \"\", \"FIX32.THISNODE.YT6022_LEAFINGP1.A_CV\", 2 /预计入柜号1\nWriteValue \"0\", \"FIX32.THISNODE.YT6022_LEAFINGP1AMOUNT.F_CV\", 2/入1柜料量\nWriteValue \"\", \"FIX32.THISNODE.YT6022_LEAFINGP2.A_CV\", 2/预计入柜号2\nWriteValue \"0\", \"FIX32.THISNODE.YT6022_LEAFINGP2AMOUNT.F_CV\", 2/入2柜料量\nWriteValue \"\", \"FIX32.THISNODE.YT6022_LEAFINGP3.A_CV\", 2/预计入柜号3\nWriteValue \"0\", \"FIX32.THISNODE.YT6022_LEAFINGP3AMOUNT.F_CV\", 2/入3柜料量\nWriteValue \"0\", \"FIX32.THISNODE.YT6022_LEAFINGPQTY.F_CV\", 2/生成物料入的柜子数量\nWriteValue \"\", \"FIX32.THISNODE.YT6022_LEAFJHJSSJ.A_CV\", 2/叶片段计划结束时间\nWriteValue \"\", \"FIX32.THISNODE.YT6022_LEAFJHKSSJ.A_CV\", 2/叶片段计划开始时间\nWriteValue \"\", \"FIX32.THISNODE.YT6022_LEAFOUTGP.A_CV\", 2/预混柜出柜号\nWriteValue \"0\", \"FIX32.THISNODE.YT6022_LEAFPRODMIX.F_CV\", 2/产出物是否汇集\nWriteValue \"0\", \"FIX32.THISNODE.YT6022_LEAFROAD.F_CV\", 2/生产工艺路线\nWriteValue \"\", \"FIX32.THISNODE.YT6022_LEAFSTUFFBRAND.A_CV\", 2/叶片段当前料液牌号\nWriteValue \"0\", \"FIX32.THISNODE.YT6022_LEAFWEIGHT.F_CV\", 2/叶片段当前重量",null,null,"JK_YT6022_LEAFBSC_CLEAR","case \"api/L5KYPJL_ZHStopInfoClear_ProdClear\":  //\n                    rlt = AppUtil.WriteFunction(AppUtil.GetConfig(ModuleEnum.JL),\"L5KYPJL_ZHStopInfoClear_ProdClear\"); \n                    break;",{"$error":"#REF!"},"NUL"]
[{"$nulls":3},"出预配柜路径清零","柜号","L5KYPJL_ZHStopInfoClear_OutYPG_PathClear(string YPNo)","post","YP04/YP05/YP06/YP07",null,"YT6022_TASK2_B04\n/YT6022_TASK2_B03\n/YT6022_TASK2_B02\n/YT6022_TASK2_B01",{"$nulls":3},"YT6022_TASK2_B04\n/YT6022_TASK2_B03\n/YT6022_TASK2_B02\n/YT6022_TASK2_B01","case \"api/L5KYPJL_ZHStopInfoClear_OutYPG_PathClear(string YPNo)\":  //\n                    rlt = AppUtil.WriteFunction(AppUtil.GetConfig(ModuleEnum.JL),\"L5KYPJL_ZHStopInfoClear_OutYPG_PathClear(string YPNo)\"); \n                    break;",{"$error":"#REF!"},"MUL"]
[{"$nulls":3},"出预配柜信息清零","柜号","L5KYPJL_ZHStopInfoClear_OutYPG_InfoClear(string YPNo)","post","YP04/YP05/YP06/YP07",null,"YT6022_GP_2139R_JOB(YP04批次)\n/YT6022_GP_2139R_BRAND（牌号）\nYT6022_GP_2139L_JOB(YP05批次)\n/YT6022_GP_2139L_BRAND（牌号）\nYT6022_GP_2138R_JOB(YP06批次)\n/YT6022_GP_2138R_BRAND（牌号）\nYT6022_GP_2138L_JOB(YP07批次)\n/YT6022_GP_2138L_BRAND（牌号）",{"$nulls":3},"YT6022_GP_2139R_JOB(YP04批次)\n/YT6022_GP_2139R_BRAND（牌号）\nYT6022_GP_2139L_JOB(YP05批次)\n/YT6022_GP_2139L_BRAND（牌号）\nYT6022_GP_2138R_JOB(YP06批次)\n/YT6022_GP_2138R_BRAND（牌号）\nYT6022_GP_2138L_JOB(YP07批次)\n/YT6022_GP_2138L_BRAND（牌号）","case \"api/L5KYPJL_ZHStopInfoClear_OutYPG_InfoClear(string YPNo)\":  //\n                    rlt = AppUtil.WriteFunction(AppUtil.GetConfig(ModuleEnum.JL),\"L5KYPJL_ZHStopInfoClear_OutYPG_InfoClear(string YPNo)\"); \n                    break;",{"$error":"#REF!"},"MUL"]
[{"$nulls":3},"进叶柜路径清零","进叶柜号","L5KYPJL_ZHStopInfoClear_InYG_PathClear(string YGNo)","post","YG01~YG24",null,"YG02/JK_YT630_IN_task2_A01 （写0）\nYG04/JK_YT630_IN_task2_A02\nYG06/JK_YT630_IN_task2_A03\nYG08/JK_YT630_IN_task2_A04\nYG10/JK_YT630_IN_task2_A05\nYG12/JK_YT630_IN_task2_A06\nYG14/JK_YT630_IN_task2_A07\nYG16/JK_YT630_IN_task2_A08\nYG01/JK_YT630_IN_task2_A09\nYG03/JK_YT630_IN_task2_A10\nYG05/JK_YT630_IN_task2_A11\nYG07/JK_YT630_IN_task2_A12\nYG09/JK_YT630_IN_task2_A13\nYG11/JK_YT630_IN_task2_A14\nYG13/JK_YT630_IN_task2_A15\nYG15/JK_YT630_IN_task2_A16\nYG18/JK_YT630_IN_task2_A17\nYG20/JK_YT630_IN_task2_A18\nYG22/JK_YT630_IN_task2_A19\nYG24/JK_YT630_IN_task2_A20",{"$nulls":3},"YG02/JK_YT630_IN_task2_A01 （写0）\nYG04/JK_YT630_IN_task2_A02\nYG06/JK_YT630_IN_task2_A03\nYG08/JK_YT630_IN_task2_A04\nYG10/JK_YT630_IN_task2_A05\nYG12/JK_YT630_IN_task2_A06\nYG14/JK_YT630_IN_task2_A07\nYG16/JK_YT630_IN_task2_A08\nYG01/JK_YT630_IN_task2_A09\nYG03/JK_YT630_IN_task2_A10\nYG05/JK_YT630_IN_task2_A11\nYG07/JK_YT630_IN_task2_A12\nYG09/JK_YT630_IN_task2_A13\nYG11/JK_YT630_IN_task2_A14\nYG13/JK_YT630_IN_task2_A15\nYG15/JK_YT630_IN_task2_A16\nYG18/JK_YT630_IN_task2_A17\nYG20/JK_YT630_IN_task2_A18\nYG22/JK_YT630_IN_task2_A19\nYG24/JK_YT630_IN_task2_A20","case \"api/L5KYPJL_ZHStopInfoClear_InYG_PathClear(string YGNo)\":  //\n                    rlt = AppUtil.WriteFunction(AppUtil.GetConfig(ModuleEnum.JL),\"L5KYPJL_ZHStopInfoClear_InYG_PathClear(string YGNo)\"); \n                    break;",{"$error":"#REF!"},"MUL"]
[{"$nulls":3},"进叶柜信息清零（单机操作）","进叶柜号","L5KYPJL_ZHStopInfoClear_InYG_InfoClear(string YGNo)","post","YG01~YG24",null,"YG01/YT630_1129A_JOB（批次）/YT630_1129A_BRAND（牌号）\nYG02/YT630_1129_JOB/YT630_1129_BRAND\nYG03/YT630_1129_1A_JOB/YT630_1129_1A_BRAND\nYG04/YT630_1129_1_JOB/YT630_1129_1_BRAND\nYG05/YT630_1129_2A_JOB/YT630_1129_2A_BRAND\nYG06/YT630_1129_2_JOB/YT630_1129_2_BRAND\nYG07/YT630_1129_3A_JOB/YT630_1129_3A_BRAND\nYG08/YT630_1129_3_JOB/YT630_1129_3_BRAND\nYG09/YT630_1129_4A_JOB/YT630_1129_4A_BRAND\nYG10/YT630_1129_4_JOB/YT630_1129_4_BRAND\nYG11/YT630_1129_5A_JOB/YT630_1129_5A_BRAND\nYG12/YT630_1129_5_JOB/YT630_1129_5_BRAND\nYG13/YT630_1129_6A_JOB/YT630_1129_6A_BRAND\nYG14/YT630_1129_6_JOB/YT630_1129_6_BRAND\nYG15/YT630_1129_7A_JOB/YT630_1129_7A_BRAND\nYG16/YT630_1129_7_JOB/YT630_1129_7_BRAND\nYG18/YT630_1153_JOB/YT630_1153_BRAND\nYG20/YT630_1153_1_JOB/YT630_1153_1_BRAND\nYG22/YT630_1153_2_JOB/YT630_1153_2_BRAND\nYG24/YT630_1153_3_JOB/YT630_1153_3_BRAND",{"$nulls":3},"YG01/YT630_1129A_JOB（批次）/YT630_1129A_BRAND（牌号）\nYG02/YT630_1129_JOB/YT630_1129_BRAND\nYG03/YT630_1129_1A_JOB/YT630_1129_1A_BRAND\nYG04/YT630_1129_1_JOB/YT630_1129_1_BRAND\nYG05/YT630_1129_2A_JOB/YT630_1129_2A_BRAND\nYG06/YT630_1129_2_JOB/YT630_1129_2_BRAND\nYG07/YT630_1129_3A_JOB/YT630_1129_3A_BRAND\nYG08/YT630_1129_3_JOB/YT630_1129_3_BRAND\nYG09/YT630_1129_4A_JOB/YT630_1129_4A_BRAND\nYG10/YT630_1129_4_JOB/YT630_1129_4_BRAND\nYG11/YT630_1129_5A_JOB/YT630_1129_5A_BRAND\nYG12/YT630_1129_5_JOB/YT630_1129_5_BRAND\nYG13/YT630_1129_6A_JOB/YT630_1129_6A_BRAND\nYG14/YT630_1129_6_JOB/YT630_1129_6_BRAND\nYG15/YT630_1129_7A_JOB/YT630_1129_7A_BRAND\nYG16/YT630_1129_7_JOB/YT630_1129_7_BRAND\nYG18/YT630_1153_JOB/YT630_1153_BRAND\nYG20/YT630_1153_1_JOB/YT630_1153_1_BRAND\nYG22/YT630_1153_2_JOB/YT630_1153_2_BRAND\nYG24/YT630_1153_3_JOB/YT630_1153_3_BRAND","case \"api/L5KYPJL_ZHStopInfoClear_InYG_InfoClear(string YGNo)\":  //\n                    rlt = AppUtil.WriteFunction(AppUtil.GetConfig(ModuleEnum.JL),\"L5KYPJL_ZHStopInfoClear_InYG_InfoClear(string YGNo)\"); \n                    break;",{"$error":"#REF!"},"MUL"]
[null,null,"设备组合停止",null,"无","L5KYPJL_ZHStop_Stop","get",null,null,"       FIX.YT630_IN_TASK2_STop.F_CV  1\n       FIX.YT6022_IN_TASK2_STOP.F_CV  1","       Fix32.THISNODE.YT630_IN_TASK2_STop.F_CV = 1\n       Fix32.THISNODE.YT6022_IN_TASK2_STOP.F_CV = 1",null,null,"YT6022_IN_TASK2_STOP","case \"api/L5KYPJL_ZHStop_Stop\":  //设备组合停止\n                    rlt = AppUtil.WriteFunction(AppUtil.GetConfig(ModuleEnum.JL),\"L5KYPJL_ZHStop_Stop\"); \n                    break;",{"$error":"#REF!"}]
[null,"辅助操作","单机/联机",null,"段号","L5KYPJL_FK_DeviceLink(string DeviceName,Bool Bsel)",{"$nulls":8},{"$error":"#REF!"},null,"post"]
[null,null,"故障复位（两个复位，一起）",null,"无","L5KYPJL_FK_AlarmReset","get",null,null,"FIX.YT6022_CONTROL_YT6022_RESET.F_CV  1",{"$nulls":3},"YT6022_CONTROL_YT6022_RESET","case \"api/L5KYPJL_FK_AlarmReset\":  //故障复位（两个复位，一起）\n                    rlt = AppUtil.WriteFunction(AppUtil.GetConfig(ModuleEnum.JL),\"L5KYPJL_FK_AlarmReset\"); \n                    break;",{"$error":"#REF!"}]

{"sheet":"真空回潮","index":2,"n_rows":37,"n_cols":12,"rows_kept":37,"merged":[[1,0,36,0],[1,1,8,1],[2,2,3,2],[5,2,6,2],[7,2,8,2],[9,1,14,1],[15,1,26,1],[27,1,34,1],[28,2,29,2],[30,2,34,2],[35,1,36,1]],"flags":["formulas_cached_only"]}
["工序","操作按钮","组件封装","业务说明","参数说明","API接口名","测试状态","备注","API状态"]
["5K真空回潮","生产启动","工单信息下发",null,"工单号、批次号、牌号",{"$nulls":4},"YT618A_BATCHNO（批次）\n/YT618A_ENTRYID(工单)\n/YT618A_BRAND(牌号)"]
[null,null,"生产路径选择","3K回潮路径选择",{"$nulls":5},"YT618_WL3000_SELECT",null," If Fix32.THISNODE.YT618_WL3000_SELECT.F_CV = 0 Then\n    If (MsgBox(\"是否需要选择真空回潮3000线供料\", vbOKCancel, \"选择3000线供料\") = vbOK) Then\n       Fix32.THISNODE.YT618_WL3000_SELECT.F_CV = 1\n       Fix32.THISNODE.YT618_WL5000_SELECT.F_CV = 0\n       Call Modlogin.Oplog((1), (0), (1), \"YT618选择真空回潮3000线供料\")\n    End If\n Else\n   If (MsgBox(\"是否需要取消选择真空回潮3000线供料\", vbOKCancel, \"选择3000线供料\") = vbOK) Then\n      Fix32.THISNODE.YT618_WL3000_SELECT.F_CV = 0\n      Fix32.THISNODE.YT618_WL5000_SELECT.F_CV = 1\n      Call Modlogin.Oplog((1), (0), (1), \"YT618取消选择真空回潮3000线供料\")\n   End If\n End If"]
[{"$nulls":3},"5K回潮路径选择",{"$nulls":5},"YT618_WL5000_SELECT"]
[null,null,"批开始",{"$nulls":6},"YT618_TASK1_BSTART"]
[null,null,"设备打自动","设备1组打自动",{"$nulls":5},"YT618_TASK1_AUTO"]
[{"$nulls":3},"设备2组打自动",{"$nulls":5},"YT618_TASK2_AUTO"]
[null,null,"组合启动","设备1组合启动",{"$nulls":5},"YT618_TASK1_START"]
[{"$nulls":3},"设备2组合启动",{"$nulls":5},"YT618_TASK2_START"]
[null,"生产提升","3353生产提升",{"$nulls":6},"YT618_WP3353_CONSET1"]
[null,null,"3353强制提升",{"$nulls":6},"YT618_WP3353_CONSET2"]
[null,null,"3353强制停止",{"$nulls":6},"YT618_WP3353_CONSET3"]
[null,null,"3360生产提升",{"$nulls":6},"YT618_WP3360_CONSET1"]
[null,null,"3360强制提升",{"$nulls":6},"YT618_WP3360_CONSET2"]
[null,null,"3360强制停止",{"$nulls":6},"YT618_WP3360_CONSET3"]
[null,"A/B锅切换","选择A锅",{"$nulls":6},"YT618_WZ1_SELECT"]
[null,null,"选择B锅",{"$nulls":6},"YT618_WZ2_SELECT"]
[null,null,"取消A锅选择",{"$nulls":6},"YT618_WZ1_SELECT"]
[null,null,"取消B锅选择",{"$nulls":6},"YT618_WZ2_SELECT"]
[null,null,"A锅启动"]
[null,null,"B锅启动"]
[null,null,"A锅停止"]
[null,null,"B锅停止"]
[null,null,"A锅前实际进锅数量设定",null,"进锅数",{"$nulls":4},"YT618_UNIT_12_INFO"]
[null,null,"B锅前实际进锅数量设定",null,"进锅数",{"$nulls":4},"YT618_UNIT_14_INFO"]
[null,null,"A锅前实际进箱数量设定",null,"进箱数",{"$nulls":4},"YT618_WZ1_INNUM_SET"]
[null,null,"B锅前实际进箱数量设定",null,"进箱数",{"$nulls":4},"YT618_WZ2_INNUM_SET"]
[null,"生产停止","批结束",{"$nulls":6},"YT618_TASK1_BSTOP"]
[null,null,"组合停止","设备1组合停止",{"$nulls":5},"YT618_TASK1_STOP"]
[{"$nulls":3},"设备2组合停止",{"$nulls":5},"YT618_TASK2_STOP"]
[null,null,"信息清零","任务结束"]
[{"$nulls":3},"批次清零",{"$nulls":6},"清零按钮","YT618_WZ_VALUE_CLEAR"]
[{"$nulls":3},"生产清零"]
[{"$nulls":3},"3354电子秤清零",{"$nulls":5},"YT618_CK3354_CLEAR"]
[{"$nulls":3},"3361电子秤清零",{"$nulls":5},"YT618_CK3361_CLEAR"]
[null,"辅助操作","单机/联机"]
[null,null,"故障复位",{"$nulls":6},"YT618_RESET"]

{"sheet":"API封装需求","index":3,"n_rows":3,"n_cols":1,"rows_kept":3,"flags":["formulas_cached_only"]}
["支持单点位下发/读取"]
["支持批量点位下发/读取"]
["支持条件验证"]

{"sheet":"300加料","index":4,"n_rows":138,"n_cols":12,"rows_kept":138,"merged":[[1,0,39,0],[1,1,4,1],[5,1,10,1],[11,1,19,1],[19,11,22,11],[20,1,22,1],[23,1,37,1],[24,2,29,2],[30,2,36,2],[38,1,39,1],[41,0,60,0],[41,1,44,1],[45,1,50,1],[52,1,54,1],[55,1,58,1],[55,2,57,2],[59,1,60,1],[62,0,98,0],[62,1,65,1],[66,1,71,1],[72,1,80,1],[81,1,83,1],[84,1,96,1],[85,2,88,2],[89,2,95,2],[97,1,98,1],[100,0,137,0],[100,1,103,1],[104,1,109,1],[110,1,118,1],[119,1,121,1],[122,1,135,1],[123,2,127,2],[128,2,134,2],[136,1,137,1]],"flags":["formulas_cached_only"]}
["工序","操作按钮","组件封装","业务说明","参数说明","API接口名","请求类型","测试状态","备注","API状态","写入点位","检查点位"]
["5千加料","设备预热","预热启动",null,"无","L5KYPJL_SBYR_START","Get",{"$nulls":3},"YT6022_C_WQ2126_PREHEAT_START"]
[null,null,"预热温度值设定",null,"温度值","L5KYPJL_SBYR_YRWDSET(float Temp)","Post",{"$nulls":3},"YT6022_C_SJ2116_PREHEAT_START"]
[null,null,"预热生产温度值设定",null,"温度值","L5KYPJL_SBYR_YXWDSET(float Temp)","Post",{"$nulls":3},"YT6022_VALUE_WQ2126_P_SET_1"]
[null,null,"预热结束",null,"无","L5KYPJL_SBYR_CLOSE","Get",{"$nulls":3},"YT6022_VALUE_WQ2116_P_SET_1"]
[null,"要料","料筒选择-料筒1",null,"无","L5KYPJL_YL_Tank1Select","Get",{"$nulls":3},"YT6022_VALUE_WQ2126_PID4_SP"]
[null,null,"料筒选择-料筒2",null,"无","L5KYPJL_YL_Tank2Select","Get",{"$nulls":3},"YT6022_VALUE_WQ2116_PID4_SP"]
[null,null,"要料信息下发-料筒1",null,"料液重量、料液代码、批次号","L5KYPJL_YL_Tank1Info_Set(object info)","Post",{"$nulls":3},"YT6022_C_WQ2126_PREHEAT_STOP"]
[null,null,"要料信息下发-料筒2",null,"料液重量、料液代码、批次号","L5KYPJL_YL_Tank2Info_Set(object info)","Post",{"$nulls":3},"YT6022_C_SJ2116_PREHEAT_STOP"]
[null,null,"取消要料-料筒1",null,"无","L5KYPJL_YL_Tank1Cancel","Get",{"$nulls":3},"YT6022_TASK1_R09（真空））"]
[null,null,"取消要料-料筒2",null,"无","L5KYPJL_YL_Tank2Cancel","Get",{"$nulls":3},"YT6022_TASK1_R06（薄片）"]
[null,"组合启动","工单信息下发",null,"工单号、批次号、牌号","L5KYPJL_ZHStart_GDInfoSet(string YPGno,string BatchNo,string BrandNo）JSON格式","Post",{"$nulls":3},"YT6022_TASK1_R09（真空）"]
[null,null,"批开始",null,"无","L5KYPJL_ZHStart_BatchStart","Get",{"$nulls":3},"YT6022_TASK1_R06（薄片）"]
[null,null,"出预配柜条件验证及路径下发",null,"柜号","L5KYPJL_ZHStart_OutYPGCheck(string YPGno）","Post",{"$nulls":3},"YT6022_MIXENTRYID（工单）/YT6022_MIXBATCHNO（批次）/YT6022_MIXBRAND（牌号）"]
[null,null,"出预配柜路径取消",null,"柜号","L5KYPJL_ZHStart_OutYPGCancel(string YPGno）","Post",{"$nulls":3},"YT6022_TASK1_BSTART"]
[null,null,"出预配柜信息下发",null,"柜号","L5KYPJL_ZHStart_OutPGInfoSet(string YPGno）","Post",{"$nulls":3},"JK_YT6022_TANK1_TAG"]
[null,null,"进叶柜条件验证及路径下发",null,"柜号","L5KYPJL_ZHStart_InYGCheck(string YPGno）","Post",{"$nulls":3},"JK_YT6022_TANK1_TAG"]
[null,null,"进叶柜路径取消",null,"柜号",null,"Post",{"$nulls":3},"JK_YT6022_TASK1_A04（YP04）/JK_YT6022_TASK1_A03（YP05）/JK_YT6022_TASK1_A02（YP06）/JK_YT6022_TASK1_A01（YP07）","JK_YT6022_YP04_INT_UNITERR\n/JK_YT6022_YP05_INT_UNITERR\n/JK_YT6022_YP06_INT_UNITERR\n/JK_YT6022_YP07_INT_UNITERR"]
[null,null,"进叶柜信息下发",null,"柜号、批次号、牌号","L5KYPJL_ZHStart_InYgInfoSet(string YPGno,string BatchNo,string BrandNo）JSON格式","Post",{"$nulls":3},"JK_YT6022_TASK1_A04（YP04）/JK_YT6022_TASK1_A03（YP05）/JK_YT6022_TASK1_A02（YP06）/JK_YT6022_TASK1_A01（YP07）"]
[null,null,"设备组合启动",null,"无","L5KYPJL_ZHStart_Start","Get",{"$nulls":3},"YT6022_GP_2139R_JOB(YP04批次)\n/YT6022_GP_2139R_BRAND（牌号）"]
[null,"生产提升","生产提升",null,"无","L5KYPJL_TS_TSStart","Get",{"$nulls":3},"YT6022_GP_2139L_JOB(YP05批次)\n/YT6022_GP_2139L_BRAND（牌号）"]
[null,null,"强制提升",null,"无","L5KYPJL_TS_TSForceStart","Get",{"$nulls":3},"YT6022_GP_2138R_JOB(YP06批次)\n/YT6022_GP_2138R_BRAND（牌号）"]
[null,null,"强制停止提升",null,"无","L5KYPJL_TS_TSForceStop","Get",{"$nulls":3},"YT6022_GP_2138L_JOB(YP07批次)\n/YT6022_GP_2138L_BRAND（牌号）"]
[null,"组合停止","批结束",null,"无","L5KYPJL_ZHStop_BatchEnd","Get",{"$nulls":3},"YT6022_IN_TASK1_START"]
[null,null,"余料回收","管路余料回到料筒","无","L5KYPJL_ZHStopRec_Pipe_InTank","Get",{"$nulls":3},"YT6022_WPL3373_ASEND"]
[{"$nulls":3},"回料到料房-料筒1","无","L5KYPJL_ZHStopRec_Tank1_InMRoom","Get",{"$nulls":3},"YT6022_WPL3373_FORCEASEND"]
[{"$nulls":3},"回料到料房-料筒2","无","L5KYPJL_ZHStopRec_Tank2_InMRoom","Get",{"$nulls":3},"YT6022_WPL3373_FORCESTOP"]
[{"$nulls":3},"管路清洗","无","L5KYPJL_ZHStopRec_Pipe_Clear","Get",{"$nulls":3},"YT6022_WPL2122_ASEND"]
[{"$nulls":3},"料筒清洗-料筒1","无","L5KYPJL_ZHStopRec_Tank1_Clear","Get",{"$nulls":3},"YT6022_WPL2122_FORCEASEND"]
[{"$nulls":3},"料筒清洗-料筒2","无","L5KYPJL_ZHStopRec_Tank2_Clear","Get",{"$nulls":3},"YT6022_WPL2122_FORCESTOP"]
[null,null,"信息清零","任务结束","无","L5KYPJL_ZHStopInfoClear_TankClear","Get",{"$nulls":3},"YT6022_TASK1_BSTOP"]
[{"$nulls":3},"批次清零","无","L5KYPJL_ZHStopInfoClear_BatchClear","Get",{"$nulls":3},"YT6022_IN_TASK1_FINISH"]
[{"$nulls":3},"生产清零","无","L5KYPJL_ZHStopInfoClear_ProdClear","Get",{"$nulls":3},"JK_YT6022_MIXENTPC_CLEAR","JK_YT6022_MIXENTPC_UNITERR"]
[{"$nulls":3},"出预配柜路径清零","无","L5KYPJL_ZHStopInfoClear_OutYPG_PathClear","Get",{"$nulls":3},"JK_YT6022_MIXENTSC_CLEAR","JK_YT6022_MIXENTSC_UNITERR"]
[{"$nulls":3},"出预配柜柜号清零","无","L5KYPJL_ZHStopInfoClear_OutYPG_InfoClear","Get",{"$nulls":3},"YT6022_TASK1_NODEA\n"]
[{"$nulls":3},"进叶柜路径清零","无","L5KYPJL_ZHStopInfoClear_InYG_PathClear","Get"]
[{"$nulls":3},"进叶柜柜号清零","无","L5KYPJL_ZHStopInfoClear_InYG_InfoClear","Get",{"$nulls":3},"YT6022_IN_TASK1_STOP"]
[null,null,"设备组合停止",null,"无","L5KYPJL_ZHStop_Stop","Get"]
[null,"辅助操作","单机/联机",null,"段号","L5KYPJL_FK_DeviceLink(string DeviceName,Bool Bsel)","Post",{"$nulls":3},"YT6022_CONTROL_YT6022_RESET"]
[null,null,"故障复位",null,"无","L5KYPJL_FK_AlarmReset","Get"]
[{"$nulls":10},"YT6022_WQ2_SEL"]
["3千一次加料","设备预热","预热启动",null,"无","L3KYPJL1_SBYR_START","Get"]
[null,null,"预热温度值设定",null,"温度值","L3KYPJL1_SBYR_YRWDSET(float Temp)","Post"]
[null,null,"预热生产温度值设定",null,"温度值","L3KYPJL1_SBYR_YXWDSET(float Temp)","Post"]
[null,null,"预热结束",null,"无","L3KYPJL1_SBYR_CLOSE","Get"]
[null,"要料","料筒选择-料筒1",null,"无","L3KYPJL1_YL_Tank1Select","Get"]
[null,null,"料筒选择-料筒2",null,"无","L3KYPJL1_YL_Tank2Select","Get"]
[null,null,"要料信息下发-料筒1",null,"料液重量、料液代码、批次号","L3KYPJL1_YL_Tank1Info_Set(object info)","Post"]
[null,null,"要料信息下发-料筒2",null,"料液重量、料液代码、批次号","L3KYPJL1_YL_Tank2Info_Set(object info)","Post"]
[null,null,"取消要料-料筒1",null,"无","L3KYPJL1_YL_Tank1Cancel","Get"]
[null,null,"取消要料-料筒2",null,"无","L3KYPJL1_YL_Tank2Cancel","Get"]
[null,"组合启动","设备组合启动",null,"无","L3KYPJL1_ZHStart_GDInfoSet","Get"]
[null,"生产提升","生产提升",null,"无","L3KYPJL1_TS_TSStart","Get"]
[null,null,"强制提升",null,"无","L3KYPJL1_TS_TSForceStart","Get"]
[null,null,"强制停止提升",null,"无","L3KYPJL1_TS_TSForceStop","Get"]
[null,"组合停止","余料回收","管路余料回到料筒","无","L3KYPJL1_ZHStopRec_Pipe_InTank","Get"]
[{"$nulls":3},"料筒清洗-料筒1","无","L3KYPJL1_ZHStopRec_Tank1_InMRoom","Get"]
[{"$nulls":3},"料筒清洗-料筒2","无","L3KYPJL1_ZHStopRec_Tank2_InMRoom","Get"]
[null,null,"设备组合停止",null,"无","L3KYPJL1_ZHSTOP_STOP","Get"]
[null,"辅助操作","单机/联机",null,"段号","L3KYPJL1_FK_DeviceLink(string DeviceName,Bool Bsel)","Post"]
[null,null,"故障复位",null,"无","L3KYPJL1_FK_AlarmReset","Get"]
[]
["3千二次加料","设备预热","预热启动",null,"无","L3KYPJL2_SBYR_START","Get"]
[null,null,"预热温度值设定",null,"温度值","L3KYPJL2_SBYR_YRWDSET(float Temp)","Post"]
[null,null,"预热生产温度值设定",null,"温度值","L3KYPJL2_SBYR_YXWDSET(float Temp)","Post"]
[null,null,"预热结束",null,"无","L3KYPJL2_SBYR_CLOSE","Get"]
[null,"要料","料筒选择-料筒1",null,"无","L3KYPJL2_YL_Tank1Select","Get"]
[null,null,"料筒选择-料筒2",null,"无","L3KYPJL2_YL_Tank2Select","Get"]
[null,null,"要料信息下发-料筒1",null,"料液重量、料液代码、批次号","L3KYPJL2_YL_Tank1Info_Set(object info)","Post"]
[null,null,"要料信息下发-料筒2",null,"料液重量、料液代码、批次号","L3KYPJL2_YL_Tank2Info_Set(object info)","Post"]
[null,null,"取消要料-料筒1",null,"无","L3KYPJL2_YL_Tank1Cancel","Get"]
[null,null,"取消要料-料筒2",null,"无","L3KYPJL2_YL_Tank2Cancel","Get"]
[null,"组合启动","工单信息下发",null,"工单号、批次号、牌号","L3KYPJL2_ZHStart_GDInfoSet","Post"]
[null,null,"批开始",null,"无","L3KYPJL2_ZHStart_BatchStart","Get"]
[null,null,"出预配柜条件验证及路径下发",null,"柜号","L3KYPJL2_ZHStart_OutYPGCheck(string YPGno）","Post"]
[null,null,"出预配柜路径取消",null,"柜号","L3KYPJL2_ZHStart_OutYPGcancel(string YPGno）","Post"]
[null,null,"出预配柜信息下发",null,"柜号","L3KYPJL2_ZHStart_OutPGInfoSet(string YPGno）","Post"]
[null,null,"进配叶柜条件验证及路径下发",null,"柜号","L3KYPJL2_ZHStart_InYGCheck(string YPGno）","Post"]
[null,null,"进配叶柜路径取消",null,"柜号","L3KYPJL2_ZHStart_InYGCancel(string YPGno）","Post"]
[null,null,"进配叶柜信息下发",null,"柜号、批次号、牌号","L3KYPJL2_ZHStart_InYgInfoSet(string YPGno）","Post"]
[null,null,"设备组合启动",null,"无","L3KYPJL2_ZHStart_Start","Get"]
[null,"生产提升","生产提升",null,"无","L3KYPJL2_TS_TSStart","Get"]
[null,null,"强制提升",null,"无","L3KYPJL2_TS_TSForceStart","Get"]
[null,null,"强制停止提升",null,"无","L3KYPJL2_TS_TSForceStop","Get"]
[null,"组合停止","批结束",null,"无","L3KYPJL2_ZHStop_BatchEnd","Get"]
[null,null,"余料回收","管路余料回到料筒","无","L3KYPJL2_ZHStopRec_Pipe_InTank","Get"]
[{"$nulls":3},"管路清洗","无","L3KYPJL2_ZHStopRec_Pipe_Clear","Get"]
[{"$nulls":3},"料筒清洗-料筒1","无","L3KYPJL2_ZHStopRec_Tank1_InMRoom","Get"]
[{"$nulls":3},"料筒清洗-料筒2","无","L3KYPJL2_ZHStopRec_Tank2_InMRoom","Get"]
[null,null,"信息清零","任务结束","无","L3KYPJL2_ZHSTOP_TASK_END","Get"]
[{"$nulls":3},"批次清零","无","L3KYPJL2_ZHSTOP_CLEAR_BATCH","Get"]
[{"$nulls":3},"生产清零","无","L3KYPJL2_ZHSTOP_CLEAR_PRODINFO","Get"]
[{"$nulls":3},"出预配柜路径清零","无","L3KYPJL2_ZHStopInfoClear_OutYPG_PathClear","Get"]
[{"$nulls":3},"出预配柜柜号清零","无","L3KYPJL2_ZHStopInfoClear_OutYPG_InfoClear","Get"]
[{"$nulls":3},"进配叶柜路径清零","无","L3KYPJL2_ZHStopInfoClear_InYG_PathClear","Get"]
[{"$nulls":3},"进配叶柜柜号清零","无","L3KYPJL2_ZHStopInfoClear_InYG_InfoClear","Get"]
[null,null,"设备组合停止",null,"无","L3KYPJL2_ZHStop_Stop","Get"]
[null,"辅助操作","单机/联机",null,"段号","L3KYPJL2_FK_DeviceLink(string DeviceName,Bool Bsel)","Post"]
[null,null,"故障复位",null,"无","L3KYPJL2_FK_AlarmReset","Get"]
[]
["9千加料","设备预热","预热启动",null,"无"]
[null,null,"预热温度值设定",null,"温度值"]
[null,null,"预热生产温度值设定",null,"温度值"]
[null,null,"预热结束",null,"无"]
[null,"要料","料筒选择-料筒1",null,"无"]
[null,null,"料筒选择-料筒2",null,"无"]
[null,null,"要料信息下发-料筒1",null,"料液重量、料液代码、批次号"]
[null,null,"要料信息下发-料筒2",null,"料液重量、料液代码、批次号"]
[null,null,"取消要料-料筒1",null,"无"]
[null,null,"取消要料-料筒2",null,"无"]
[null,"组合启动","工单信息下发",null,"工单号、批次号、牌号"]
[null,null,"批开始",null,"无"]
[null,null,"出预配柜条件验证及路径下发",null,"柜号"]
[null,null,"出预配柜路径取消",null,"柜号"]
[null,null,"出预配柜信息下发",null,"柜号"]
[null,null,"进叶柜条件验证及路径下发",null,"柜号"]
[null,null,"进叶柜路径取消",null,"柜号"]
[null,null,"进叶柜信息下发",null,"柜号、批次号、牌号"]
[null,null,"设备组合启动",null,"无"]
[null,"生产提升","生产提升",null,"无"]
[null,null,"强制提升",null,"无"]
[null,null,"强制停止提升",null,"无"]
[null,"组合停止","批结束",null,"无"]
[null,null,"余料回收","管路余料回到料筒","无"]
[{"$nulls":3},"回料到料房-料筒1","无"]
[{"$nulls":3},"回料到料房-料筒2","无"]
[{"$nulls":3},"料筒清洗-料筒1","无"]
[{"$nulls":3},"料筒清洗-料筒2","无"]
[null,null,"信息清零","任务结束","无"]
[{"$nulls":3},"批次清零","无"]
[{"$nulls":3},"生产清零","无"]
[{"$nulls":3},"出预配柜路径清零","无"]
[{"$nulls":3},"出预配柜柜号清零","无"]
[{"$nulls":3},"进叶柜路径清零","无"]
[{"$nulls":3},"进叶柜柜号清零","无"]
[null,null,"设备组合停止",null,"无"]
[null,"辅助操作","单机/联机",null,"段号"]
[null,null,"故障复位",null,"无"]

{"sheet":"加料——001","index":5,"n_rows":52,"n_cols":14,"rows_kept":52,"merged":[[1,0,51,0],[1,1,4,1],[5,1,12,1],[13,1,23,1],[24,1,26,1],[27,1,49,1],[28,2,38,2],[40,2,48,2],[50,1,51,1]],"flags":["formulas_cached_only"]}
["工序","操作按钮","组件封装","业务说明","参数说明","API接口名","API请求方式","API传入参数","API接口检查点位","API接口写入点","触发脚本","备注","API状态","IFIX点位"]
["5千加料","设备预热","预热启动",null,"无","L5KYPJL_SBYR_START","get",null,null,"FIX.YT6022_C_SJ2147_PREHEAT_START.F_CV 1\nFIX.YT6022_C_SJ2147_PREHEAT_STOP.F_CV 0","      Fix32.THISNODE.YT6022_C_SJ2147_PREHEAT_START.F_CV = 1\n      Fix32.THISNODE.YT6022_C_SJ2147_PREHEAT_STOP.F_CV = 0",null,null,"YT6022_C_SJ2147_PREHEAT_START\n"]
[null,null,"预热温度值设定",null,"温度值","L5KYPJL_SBYR_YRWDSET(float Temp)","post",36.5,null,"FIX.YT6022_VALUE_SJ2147_P_SET_1.F_CV 输出","Fix32.THISNODE.YT6022_VALUE_SJ2147_P_SET_1.F_CV",null,null,"YT6022_VALUE_SJ2147_P_SET_1"]
[null,null,"预热生产温度值设定",null,"温度值","L5KYPJL_SBYR_YXWDSET(float Temp)","post",36.5,null,"FIX.YT6022_VALUE_SJ2147_PID1_SP.F_CV 输出","Fix32.THISNODE.YT6022_VALUE_SJ2147_PID1_SP.F_CV",null,null,"YT6022_VALUE_SJ2147_PID1_SP"]
[null,null,"预热结束",null,"无","L5KYPJL_SBYR_CLOSE","get",null,null,"FIX.YT6022_C_SJ2147_PREHEAT_START.F_CV 0\nFIX.YT6022_C_SJ2147_PREHEAT_STOP.F_CV 1","       Fix32.THISNODE.YT6022_C_SJ2147_PREHEAT_START.F_CV = 0\n       Fix32.THISNODE.YT6022_C_SJ2147_PREHEAT_STOP.F_CV = 1",null,null,"\nYT6022_C_SJ2147_PREHEAT_STOP"]
[null,"要料","料筒选择-料筒1",null,"无","L5KYPJL_YL_Tank1Select","get",null,null,"FIX.YT6022_SJ2147_TANK1_SEL.F_CV 1\nFIX.YT6022_SJ2147_TANK2_SEL.F_CV 0","\n       Fix32.THISNODE.YT6022_SJ2147_TANK1_SEL.F_CV = 1\n       Fix32.THISNODE.YT6022_SJ2147_TANK2_SEL.F_CV = 0",null,null,"YT6022_SJ2147_TANK1_SEL\n        "]
[null,null,"料筒选择-料筒2",null,"无","L5KYPJL_YL_Tank2Select","get",null,null,"FIX.YT6022_SJ2147_TANK2_SEL.F_CV 1\nFIX.YT6022_SJ2147_TANK1_SEL.F_CV 0","       Fix32.THISNODE.YT6022_SJ2147_TANK2_SEL.F_CV = 1\n       Fix32.THISNODE.YT6022_SJ2147_TANK1_SEL.F_CV = 0",null,null,"YT6022_SJ2147_TANK2_SEL\n         "]
[null,null,"要料信息下发-料筒1",null,"料液重量、料液代码、批次号","L5KYPJL_YL_Tank1Info_Set(object info)","post","{\"Weight\":1200,\"BrandNo\":\"sdfsf\",BatchNo:\"sfsdfsdf\"}",null,"FIX.YT6022_SJ2147Tank1AskQty.F_CV （重量）\nFIX.YT6022_SJ2147Tank1AskBrand.A_CV （代码）YT6022_SJ2147Tank1AskBatch.A_CV （批次）",{"$nulls":3},"YT6022_SJ2147Tank1AskQty（重量）\n/YT6022_SJ2147Tank1AskBrand（代码）\n/YT6022_SJ2147Tank1AskBatch（批次）"]
[null,null,"要料信息下发-料筒2",null,"料液重量、料液代码、批次号","L5KYPJL_YL_Tank2Info_Set(object info)","post","{\"Weight\":1200,\"BrandNo\":\"sdfsf\",BatchNo:\"sfsdfsdf\"}",null,"FIX.YT6022_SJ2147Tank2AskQty.F_CV（重量）\nFIX.YT6022_SJ2147Tank2AskBrand.A_CV（代码）\nFIX.YT6022_SJ2147Tank2AskBatch.A_CV（批次）",{"$nulls":3},"YT6022_SJ2147Tank2AskQty（重量）\n/YT6022_SJ2147Tank2AskBrand（代码）\n/YT6022_SJ2147Tank2AskBatch（批次）"]
[null,null,"要料请求-料筒1",null,"无","L5KYPJL_YL_Tank1_Set","get",null,null,"FIX.YT6022_SJ2147_TANK1_REQUEST.F_CV 1","if Fix32.THISNODE.YT6022_SJ2147_TANK1_REUSING.F_CV = 0 and Fix32.THISNODE.YT6022_SJ2147_TANK1_CLEARING.F_CV = 0 and Fix32.THISNODE.YT6022_SJ2147_PIPE1_BACK.F_CV = 0  then\nif  Fix32.THISNODE.YT6022_SJ2147Tank1AskBrand.A_CV <> \"\"\n   Fix32.THISNODE.YT6022_SJ2147Tank1AskBatch.A_CV = ComboBox1.Text\n   Fix32.THISNODE.YT6022_SJ2147Tank1AskBrand.A_CV = ComboBox2.Text\n   Fix32.THISNODE.YT6022_SJ2147Tank1AskQty.f_cv = TextBox1.Text\n   Fix32.THISNODE.YT6022_SJ2147_TANK1_REQUEST.f_cv = 1",null,null,"YT6022_SJ2147_TANK1_REQUEST"]
[null,null,"要料请求-料筒2",null,"无","L5KYPJL_YL_Tank2_Set","get",null,null,"FIX.YT6022_SJ2147_TANK2_REQUEST.F_CV  1","if  Fix32.THISNODE.YT6022_SA2224_PIPE2_SPAYING.F_CV = 0 and Fix32.THISNODE.YT6022_SA2224_TANK2_CLEARING.F_CV = 0 and Fix32.THISNODE.YT6022_SA2224_PIPE2_BACK.F_CV = 0  then\n if    Fix32.THISNODE.YT6022_SJ2147Tank2AskBatch.A_CV = ComboBox3.Text\n   Fix32.THISNODE.YT6022_SJ2147Tank2AskBrand.A_CV = ComboBox4.Text\n   Fix32.THISNODE.YT6022_SJ2147Tank2AskQty.f_cv = TextBox2.Text\n   Fix32.THISNODE.YT6022_SJ2147_TANK2_REQUEST.f_cv = 1",null,null,"YT6022_SJ2147_TANK2_REQUEST"]
[null,null,"取消要料-料筒1",null,"无","L5KYPJL_YL_Tank1Cancel","get",null,null,"FIX.YT6022_SJ2147_TANK1_REQUEST.F_CV 0","FIX.YT6022_SJ2147_TANK1_REQUEST.F_CV 0",null,null,"YT6022_SJ2147_TANK1_REQUEST"]
[null,null,"取消要料-料筒2",null,"无","L5KYPJL_YL_Tank2Cancel","get",null,null,"FIX.YT6022_SJ2147_TANK2_REQUEST.F_CV 0","FIX.YT6022_SJ2147_TANK2_REQUEST.F_CV 0",null,null,"YT6022_SJ2147_TANK2_REQUEST"]
[null,"组合启动","工单信息下发",null,"工单号、批次号、牌号","L5KYPJL_ZHStart_GDInfoSet(string YPno,string BatchNo,string BrandNo)","post","{\"YPNo\":1200,\"BatchNo\":\"sdfsf\",BrandNo:\"sfsdfsdf\"}",null,"FIX.YT6022_LeafEntryID.A_CV （工单）\nFIX.YT6022_LeafBatchNo.A_CV （批次）\nFIX.YT6022_LeafBrand.A_CV （牌号）",{"$nulls":3},"YT6022_LeafEntryID（工单）\n/YT6022_LeafBatchNo（批次）\n/YT6022_LeafBrand（牌号）"]
[null,null,"批开始",null,"无","L5KYPJL_ZHStart_BatchStart","get",null,null,"FIX.YT6022_TASK2_bSTART.F_CV  1\nFIX.YT6022_TASK2_bSTOP.F_CV  0","     Fix32.THISNODE.YT6022_TASK2_bSTART.F_CV = 1\n     Fix32.THISNODE.YT6022_TASK2_bSTOP.F_CV = 0",null,null,"YT6022_TASK2_bSTART\n  "]
[null,null,"出预配柜条件验证",null,"柜号","L5KYPJL_ZHStart_OutYPGCheck(string YPGno)","post","YP04/YP05/YP06/YP07","JK_YT6022_YP04_OUT_UNITERR\nJK_YT6022_YP05_OUT_UNITERR\nJK_YT6022_YP06_OUT_UNITERR\nJK_YT6022_YP07_OUT_UNITERR","FIX.JK_YT6022_TASK1_B04.F_CV 1\nFIX.JK_YT6022_TASK1_B03.F_CV 1\nFIX.JK_YT6022_TASK1_B02.F_CV 1\nFIX.JK_YT6022_TASK1_B01.F_CV 1",{"$nulls":3},"YP04/JK_YT6022_TASK1_B04\nYP05/JK_YT6022_TASK1_B03\nYP06/JK_YT6022_TASK1_B02\nYP07/JK_YT6022_TASK1_B01"]
[null,null,"出预配柜取消",null,"柜号","L5KYPJL_ZHStart_OutYPGCancel(string YPno)","post","YP04/YP05/YP06/YP07",null,"FIX.YT6022_task2_B04.F_CV   0\nFIX.YT6022_task2_B03.F_CV   0\nFIX.YT6022_task2_B02.F_CV   0\nFIX.YT6022_task2_B01.F_CV   0","YP07/writevalue 0, \"Fix32.THISNODE.YT6022_task2_B01.F_CV\", 1\nYP06/writevalue 0, \"Fix32.THISNODE.YT6022_task2_B02.F_CV\", 1\nYP05/writevalue 0, \"Fix32.THISNODE.YT6022_task2_B03.F_CV\", 1\nYP04/writevalue 0, \"Fix32.THISNODE.YT6022_task2_B04.F_CV\", 1\n",null,null,"YP07/YT6022_task2_B01\nYP06/YT6022_task2_B02\nYP05/YT6022_task2_B03\nYP04/YT6022_task2_B04"]
[null,null,"出预配柜信息下发（待定）",null,"柜号","L5KYPJL_ZHStart_OutPGInfoSet(string YPGno)","post","YP04/YP05/YP06/YP07",null,"YT6022_GP_2139R_JOB(YP04批次)\n/YT6022_GP_2139R_BRAND（牌号）\nYT6022_GP_2139L_JOB(YP05批次)\n/YT6022_GP_2139L_BRAND（牌号）\nYT6022_GP_2138R_JOB(YP06批次)\n/YT6022_GP_2138R_BRAND（牌号）\nYT6022_GP_2138L_JOB(YP07批次)\n/YT6022_GP_2138L_BRAND（牌号）",{"$nulls":3},"YT6022_GP_2139R_JOB(YP04批次)\n/YT6022_GP_2139R_BRAND（牌号）\nYT6022_GP_2139L_JOB(YP05批次)\n/YT6022_GP_2139L_BRAND（牌号）\nYT6022_GP_2138R_JOB(YP06批次)\n/YT6022_GP_2138R_BRAND（牌号）\nYT6022_GP_2138L_JOB(YP07批次)\n/YT6022_GP_2138L_BRAND（牌号）"]
[null,null,"启用生产关联",null,"无","L5KYPJL_REF_START","get",null,null,"FIX.YT630_IN_TASK2_LINK.F_CV  1   ",{"$nulls":3},"  YT630_IN_TASK2_LINK"]
[null,null,"取消生产关联",null,"无","L5KYPJL_REF_CANCEL","get",null,null,"FIX.YT630_IN_TASK2_LINK.F_CV  0",{"$nulls":3},"  YT630_IN_TASK2_LINK"]
[null,null,"进叶柜条件验证",null,"柜号","L5KYPJL_ZHStart_InYGCheck(string YGno）","post","YG01~YG24","JK_YT630_A1_IN_UnitErr  读1正常\nJK_YT630_A2_IN_UnitErr\nJK_YT630_A3_IN_UnitErr\nJK_YT630_A4_IN_UnitErr\nJK_YT630_A5_IN_UnitErr\nJK_YT630_A6_IN_UnitErr\nJK_YT630_A7_IN_UnitErr\nJK_YT630_A8_IN_UnitErr\nJK_YT630_A9_IN_UnitErr\nJK_YT630_A10_IN_UnitErr\nJK_YT630_A11_IN_UnitErr\nJK_YT630_A12_IN_UnitErr\nJK_YT630_A13_IN_UnitErr\nJK_YT630_A14_IN_UnitErr\nJK_YT630_A15_IN_UnitErr\nJK_YT630_A16_IN_UnitErr\nJK_YT630_A17_IN_UnitErr\nJK_YT630_A18_IN_UnitErr\nJK_YT630_A19_IN_UnitErr\nJK_YT630_A20_IN_UnitErr\n","Fix32.THISNODE.JK_YT630_IN_TASK2.F_CV",{"$nulls":3},"YG02/JK_YT630_IN_task2_A01 （写1）\nYG04/JK_YT630_IN_task2_A02\nYG06/JK_YT630_IN_task2_A03\nYG08/JK_YT630_IN_task2_A04\nYG10/JK_YT630_IN_task2_A05\nYG12/JK_YT630_IN_task2_A06\nYG14/JK_YT630_IN_task2_A07\nYG16/JK_YT630_IN_task2_A08\nYG01/JK_YT630_IN_task2_A09\nYG03/JK_YT630_IN_task2_A10\nYG05/JK_YT630_IN_task2_A11\nYG07/JK_YT630_IN_task2_A12\nYG09/JK_YT630_IN_task2_A13\nYG11/JK_YT630_IN_task2_A14\nYG13/JK_YT630_IN_task2_A15\nYG15/JK_YT630_IN_task2_A16\nYG18/JK_YT630_IN_task2_A17\nYG20/JK_YT630_IN_task2_A18\nYG22/JK_YT630_IN_task2_A19\nYG24/JK_YT630_IN_task2_A20"]
[null,null,"进页柜取消",null,"柜号","L5KYPJL_ZHStart_InYGCancel(string YGno）","post","YG01~YG24",null,"YG02/YT630_IN_task2_A01.F_CV （写0）\nYG04/YT630_IN_task2_A02\nYG06/YT630_IN_task2_A03\nYG08/YT630_IN_task2_A04\nYG10/YT630_IN_task2_A05\nYG12/YT630_IN_task2_A06\nYG14/YT630_IN_task2_A07\nYG16/YT630_IN_task2_A08\nYG01/YT630_IN_task2_A09\nYG03/YT630_IN_task2_A10\nYG05/YT630_IN_task2_A11\nYG07/YT630_IN_task2_A12\nYG09/YT630_IN_task2_A13\nYG11/YT630_IN_task2_A14\nYG13/YT630_IN_task2_A15\nYG15/YT630_IN_task2_A16\nYG18/YT630_IN_task2_A17\nYG20/YT630_IN_task2_A18\nYG22/YT630_IN_task2_A19\nYG24/YT630_IN_task2_A20",{"$nulls":3},"YG02/JK_YT630_IN_task2_A01 （写0）\nYG04/JK_YT630_IN_task2_A02\nYG06/JK_YT630_IN_task2_A03\nYG08/JK_YT630_IN_task2_A04\nYG10/JK_YT630_IN_task2_A05\nYG12/JK_YT630_IN_task2_A06\nYG14/JK_YT630_IN_task2_A07\nYG16/JK_YT630_IN_task2_A08\nYG01/JK_YT630_IN_task2_A09\nYG03/JK_YT630_IN_task2_A10\nYG05/JK_YT630_IN_task2_A11\nYG07/JK_YT630_IN_task2_A12\nYG09/JK_YT630_IN_task2_A13\nYG11/JK_YT630_IN_task2_A14\nYG13/JK_YT630_IN_task2_A15\nYG15/JK_YT630_IN_task2_A16\nYG18/JK_YT630_IN_task2_A17\nYG20/JK_YT630_IN_task2_A18\nYG22/JK_YT630_IN_task2_A19\nYG24/JK_YT630_IN_task2_A20"]
[null,null,"进叶柜信息下发",null,"柜号、批次号、牌号","L5KYPJL_ZHStart_InYgInfoSet(string YGNo,string BatchNo,string BrandNo)","post","{\"YGNo\":\"YG01\",\"BatchNo\":\"sdfsf\",BrandNo:\"sfsdfsdf\"}",null,"YG01/YT630_1129A_JOB.A_CV（批次）/YT630_1129A_BRAND（牌号）（A_CV）\nYG02/YT630_1129_JOB/YT630_1129_BRAND\nYG03/YT630_1129_1A_JOB/YT630_1129_1A_BRAND\nYG04/YT630_1129_1_JOB/YT630_1129_1_BRAND\nYG05/YT630_1129_2A_JOB/YT630_1129_2A_BRAND\nYG06/YT630_1129_2_JOB/YT630_1129_2_BRAND\nYG07/YT630_1129_3A_JOB/YT630_1129_3A_BRAND\nYG08/YT630_1129_3_JOB/YT630_1129_3_BRAND\nYG09/YT630_1129_4A_JOB/YT630_1129_4A_BRAND\nYG10/YT630_1129_4_JOB/YT630_1129_4_BRAND\nYG11/YT630_1129_5A_JOB/YT630_1129_5A_BRAND\nYG12/YT630_1129_5_JOB/YT630_1129_5_BRAND\nYG13/YT630_1129_6A_JOB/YT630_1129_6A_BRAND\nYG14/YT630_1129_6_JOB/YT630_1129_6_BRAND\nYG15/YT630_1129_7A_JOB/YT630_1129_7A_BRAND\nYG16/YT630_1129_7_JOB/YT630_1129_7_BRAND\nYG18/YT630_1153_JOB/YT630_1153_BRAND\nYG20/YT630_1153_1_JOB/YT630_1153_1_BRAND\nYG22/YT630_1153_2_JOB/YT630_1153_2_BRAND\nYG24/YT630_1153_3_JOB/YT630_1153_3_BRAND",{"$nulls":3},"YG01/YT630_1129A_JOB（批次）/YT630_1129A_BRAND（牌号）\nYG02/YT630_1129_JOB/YT630_1129_BRAND\nYG03/YT630_1129_1A_JOB/YT630_1129_1A_BRAND\nYG04/YT630_1129_1_JOB/YT630_1129_1_BRAND\nYG05/YT630_1129_2A_JOB/YT630_1129_2A_BRAND\nYG06/YT630_1129_2_JOB/YT630_1129_2_BRAND\nYG07/YT630_1129_3A_JOB/YT630_1129_3A_BRAND\nYG08/YT630_1129_3_JOB/YT630_1129_3_BRAND\nYG09/YT630_1129_4A_JOB/YT630_1129_4A_BRAND\nYG10/YT630_1129_4_JOB/YT630_1129_4_BRAND\nYG11/YT630_1129_5A_JOB/YT630_1129_5A_BRAND\nYG12/YT630_1129_5_JOB/YT630_1129_5_BRAND\nYG13/YT630_1129_6A_JOB/YT630_1129_6A_BRAND\nYG14/YT630_1129_6_JOB/YT630_1129_6_BRAND\nYG15/YT630_1129_7A_JOB/YT630_1129_7A_BRAND\nYG16/YT630_1129_7_JOB/YT630_1129_7_BRAND\nYG18/YT630_1153_JOB/YT630_1153_BRAND\nYG20/YT630_1153_1_JOB/YT630_1153_1_BRAND\nYG22/YT630_1153_2_JOB/YT630_1153_2_BRAND\nYG24/YT630_1153_3_JOB/YT630_1153_3_BRAND"]
[null,null,"设备组合启动",null,"无","L5KYPJL_ZHStart_Start","get",null,null,"FIX.YT630_IN_TASK2_START.F_CV  1\nFIX.YT6022_IN_TASK2_START.F_CV  1","      Fix32.THISNODE.YT630_IN_TASK2_START.F_CV = 1\n       Fix32.THISNODE.YT6022_IN_TASK2_START.F_CV = 1",null,null,"    YT630_IN_TASK2_START\n    YT6022_IN_TASK2_START"]
[null,"生产提升","生产提升",null,"无","L5KYPJL_TS_TSStart","get",null,null,"FIX.YT6022_WPL2141_ASEND.F_CV  1",{"$nulls":3},"YT6022_WPL2141_ASEND"]
[null,null,"强制提升",null,"无","L5KYPJL_TS_TSForceStart","get",null,null,"FIX.YT6022_WPL2141_FORCEASEND.F_CV  1",{"$nulls":3},"YT6022_WPL2141_FORCEASEND"]
[null,null,"强制停止提升",null,"无","L5KYPJL_TS_TSForceStop","get",null,null,"FIX.YT6022_WPL2141_FORCESTOP.F_CV  1",{"$nulls":3},"YT6022_WPL2141_FORCESTOP"]
[null,"组合停止","批结束",null,"无","L5KYPJL_ZHStop_BatchEnd","get",null,null,"FIX.YT6022_TASK2_bSTOP.F_CV  1\nFIX.YT6022_TASK2_bSTART.F_CV  0","     Fix32.THISNODE.YT6022_TASK2_bSTOP.F_CV = 1\n     Fix32.THISNODE.YT6022_TASK2_bSTART.F_CV = 0",null,null,"  YT6022_TASK2_bSTOP\n  YT6022_TASK2_bSTART"]
[null,null,"余料回收","管路余料回到料筒","无","L5KYPJL_ZHStopRec_Pipe_InTank","get",null,null,"FIX.YT6022_SJ2147_PIPE_CLEAR.F_CV  0\nFIX.YT6022_SJ2147_PIPE_REUSE.F_CV  1","if  Fix32.THISNODE.YT6022_STATE_SJ2147_PREFILL.F_CV = 0 and Fix32.THISNODE.YT6022_STATE_SJ2147_WORK.F_CV = 0 and Fix32.THISNODE.YT6022_SA2224_TANK2_CLEA.F_CV = 0 and Fix32.THISNODE.YT6022_SA2224_TANK2_SPA.F_CV = 0  then\nFix32.THISNODE.YT6022_SJ2147_PIPE_CLEAR.f_cv = 0\n     Fix32.THISNODE.YT6022_SJ2147_PIPE_REUSE.f_cv = 1",null,null,"YT6022_SJ2147_PIPE_REUSE"]
[{"$nulls":3},"管路余料取消回到料筒","无","L5KYPJL_ZHStopRec_Pipe_InTankCANCEL","get",null,null,"FIX.YT6022_SJ2147_PIPE_CLEAR.F_CV  0\nFIX.YT6022_SJ2147_PIPE_REUSE.F_CV  0","     Fix32.THISNODE.YT6022_SJ2147_PIPE_CLEAR.f_cv = 0\n     Fix32.THISNODE.YT6022_SJ2147_PIPE_REUSE.f_cv = 0",null,null,"YT6022_SJ2147_PIPE_REUSE"]
[{"$nulls":3},"回料到料房-料筒1","无","L5KYPJL_ZHStopRec_Tank1_InMRoom","get",null,null,"FIX.YT6022_SJ2147_TANK1_REQUEST.F_CV  0\nFIX.YT6022_SJ2147_TANK1_CLEAR_S.F_CV  0\nFIX.YT6022_SJ2147_TANK1_REUSE.F_CV  1","     Fix32.THISNODE.YT6022_SJ2147_TANK1_REQUEST.f_cv = 0\n     Fix32.THISNODE.YT6022_SJ2147_TANK1_CLEAR_S.f_cv = 0\n     Fix32.THISNODE.YT6022_SJ2147_TANK1_REUSE.f_cv = 1","(取消回料？)",null,"YT6022_SJ2147_TANK1_REUSE"]
[{"$nulls":3},"取消回料到料房-料筒1",null,"L5KYPJL_ZHStopRec_Tank1_InMRoomCANCEL","get",null,null,"FIX.YT6022_SJ2147_TANK1_REQUEST.F_CV  0\nFIX.YT6022_SJ2147_TANK1_CLEAR_S.F_CV  0\nFIX.YT6022_SJ2147_TANK1_REUSE.F_CV  0","     Fix32.THISNODE.YT6022_SJ2147_TANK1_REQUEST.f_cv = 0\n     Fix32.THISNODE.YT6022_SJ2147_TANK1_CLEAR_S.f_cv = 0\n     Fix32.THISNODE.YT6022_SJ2147_TANK1_REUSE.f_cv = 0",null,null,"YT6022_SJ2147_TANK1_REUSE"]
[{"$nulls":3},"回料到料房-料筒2","无","L5KYPJL_ZHStopRec_Tank2_InMRoom","get",null,null,"FIX.YT6022_SJ2147_TANK2_REQUEST.F_CV  0\nFIX.YT6022_SJ2147_TANK2_CLEAR_S.F_CV  0\nFIX.YT6022_SJ2147_TANK2_REUSE.F_CV  1","Fix32.THISNODE.YT6022_SA2224_TANK2_ALLOW_IN.F_CV = 0 and Fix32.THISNODE.YT6022_SA2224_TANK2_CLEARING.F_CV = 0 and Fix32.THISNODE.YT6022_SA2224_PIPE2_BACK.F_CV = 0\n If Fix32.THISNODE.YT6022_SJ2147_TANK2_REUSE.f_cv = 1 Then\n   If MsgBox(\"确定要取消料桶2回料吗？\", vbYesNo, \"回料\") = vbYes Then\n     Fix32.THISNODE.YT6022_SJ2147_TANK2_REQUEST.f_cv = 0\n     Fix32.THISNODE.YT6022_SJ2147_TANK2_CLEAR_S.f_cv = 0\n     Fix32.THISNODE.YT6022_SJ2147_TANK2_REUSE.f_cv = 0\n     Call Modlogin.Oplog((0), (0), (1), \"取消料桶2回料\")\n   End If\n Else\n   If MsgBox(\"确定要料桶2回料吗？\", vbYesNo, \"回余料\") = vbYes Then\n     Fix32.THISNODE.YT6022_SJ2147_TANK2_REQUEST.f_cv = 0\n     Fix32.THISNODE.YT6022_SJ2147_TANK2_CLEAR_S.f_cv = 0\n     Fix32.THISNODE.YT6022_SJ2147_TANK2_REUSE.f_cv = 1\n   End If\n   Call Modlogin.Oplog((0), (0), (1), \"料桶2回料\")\n End If",null,null,"YT6022_SJ2147_TANK2_REUSE"]
[{"$nulls":3},"取消回料到料房-料筒2","无","L5KYPJL_ZHStopRec_Tank2_InMRoomCANCEL","get",null,null,"FIX.YT6022_SJ2147_TANK2_REQUEST.F_CV  0\nFIX.YT6022_SJ2147_TANK2_CLEAR_S.F_CV  0\nFIX.YT6022_SJ2147_TANK2_REUSE.F_CV  0",{"$nulls":3},"YT6022_SJ2147_TANK2_REUSE"]
[{"$nulls":3},"管路清洗","无","L5KYPJL_ZHStopRec_Pipe_Clear","get",null,null,"FIX.YT6022_SJ2147_PIPE_REUSE.F_CV  0\nFIX.YT6022_SJ2147_PIPE_CLEAR.F_CV  1","Fix32.THISNODE.YT6022_SA2224_TANK2_SPA.F_CV = 0\nIf Fix32.THISNODE.YT6022_SJ2147_PIPE_CLEAR.f_cv = 1 Then\n    If MsgBox(\"确定要取消清洗管路吗？\", vbYesNo, \"清洗管路\") = vbYes Then\n     Fix32.THISNODE.YT6022_SJ2147_PIPE_REUSE.f_cv = 0\n     Fix32.THISNODE.YT6022_SJ2147_PIPE_CLEAR.f_cv = 0\n     Call Modlogin.Oplog((0), (0), (1), \"取消清洗管路\")\n    End If\n  Else\n    If MsgBox(\"确定要清洗管路吗？\", vbYesNo, \"清洗管路\") = vbYes Then\n     Fix32.THISNODE.YT6022_SJ2147_PIPE_REUSE.f_cv = 0\n     Fix32.THISNODE.YT6022_SJ2147_PIPE_CLEAR.f_cv = 1\n     Call Modlogin.Oplog((0), (0), (1), \"清洗管路\")\n    End If\n  End If",null,null,"YT6022_SJ2147_PIPE_CLEAR"]
[{"$nulls":3},"取消管路清洗","无","L5KYPJL_ZHStopRec_Pipe_ClearCANCEL","get",null,null,"FIX.YT6022_SJ2147_PIPE_REUSE.F_CV  0\nFIX.YT6022_SJ2147_PIPE_CLEAR.F_CV  0",{"$nulls":3},"YT6022_SJ2147_PIPE_CLEAR"]
[{"$nulls":3},"料筒清洗-料筒1","无","L5KYPJL_ZHStopRec_Tank1_Clear","get",null,null,"FIX.YT6022_SJ2147_TANK1_REQUEST.F_CV  0\nFIX.YT6022_SJ2147_TANK1_REUSE.F_CV 0\nFIX.YT6022_SJ2147_TANK1_CLEAR_S.F_CV  1\nFIX.YT6022_SJ2147Tank1Brand.A_CV 0 \nFIX.YT6022_SJ2147Tank1LotID2.A_CV 0\nFIX.YT6022_SJ2147Tank1LotID1.A_CV 0  ","Fix32.THISNODE.YT6022_SJ2147_TANK1_REUSING.F_CV = 0 and Fix32.THISNODE.YT6022_SJ2147_TANK1_ALLOW_IN.F_CV = 0 and Fix32.THISNODE.YT6022_VALUE_SJ2147_P_CUR_16.F_CV < 10\n If Fix32.THISNODE.YT6022_SJ2147_TANK1_CLEAR_S.f_cv = 1 Then\n    If MsgBox(\"确定要取消清洗料桶吗？\", vbYesNo, \"清洗料桶\") = vbYes Then\n     Fix32.THISNODE.YT6022_SJ2147_TANK1_REQUEST.f_cv = 0\n     Fix32.THISNODE.YT6022_SJ2147_TANK1_REUSE.f_cv = 0\n     Fix32.THISNODE.YT6022_SJ2147_TANK1_CLEAR_S.f_cv = 0\n     Call Modlogin.Oplog((0), (0), (1), \"取消清洗料桶\")\n    End If\n  Else\n    If MsgBox(\"确定要清洗料桶吗？\", vbYesNo, \"清洗料桶\") = vbYes Then\n     Fix32.THISNODE.YT6022_SJ2147_TANK1_REQUEST.f_cv = 0\n     Fix32.THISNODE.YT6022_SJ2147_TANK1_REUSE.f_cv = 0\n     Fix32.THISNODE.YT6022_SJ2147_TANK1_CLEAR_S.f_cv = 1\n     Fix32.THISNODE.YT6022_SJ2147Tank1Brand.A_CV = \"\"\n     Fix32.THISNODE.YT6022_SJ2147Tank1LotID2.A_CV = \"\"\n     Fix32.THISNODE.YT6022_SJ2147Tank1LotID1.A_CV = \"\"\n     Call Modlogin.Oplog((0), (0), (1), \"清洗料桶\")\n    End If\n  End If",null,null,"YT6022_SJ2147_TANK1_CLEAR_S"]
[{"$nulls":3},"料筒清洗取消-料筒1","无","L5KYPJL_ZHStopRec_Tank1_ClearCANCEL","get",null,null,"FIX.YT6022_SJ2147_TANK1_REQUEST.F_CV  0\nFIX.YT6022_SJ2147_TANK1_REUSE.F_CV  0\nFIX.YT6022_SJ2147_TANK1_CLEAR_S.F_CV  0",{"$nulls":3},"YT6022_SJ2147_TANK1_CLEAR_S"]
[{"$nulls":3},"料筒清洗-料筒2","无","L5KYPJL_ZHStopRec_Tank2_Clear","get",null,null,"FIX.YT6022_SJ2147_TANK2_REQUEST.F_CV  0\nFIX.YT6022_SJ2147_TANK2_REUSE.F_CV  0\nFIX.YT6022_SJ2147_TANK2_CLEAR_S.F_CV  1\nFIX.YT6022_SJ2147Tank2Brand.A_CV 0\nFIX.YT6022_SJ2147Tank2LotID1.A_CV 0\nFIX.YT6022_SJ2147Tank2LotID2.A_CV 0 ","Fix32.THISNODE.YT6022_SA2224_TANK2_ALLOW_IN.F_CV = 0 and Fix32.THISNODE.YT6022_SA2224_PIPE2_SPAYING.F_CV = 0 and Fix32.THISNODE.YT6022_SA2224_PIPE2_CLEARING.F_CV = 0 and Fix32.THISNODE.YT6022_VALUE_SJ2147_P_CUR_17.F_CV < 10\n If Fix32.THISNODE.YT6022_SJ2147_TANK2_CLEAR_S.f_cv = 1 Then\n    If MsgBox(\"确定要取消清洗料桶吗？\", vbYesNo, \"清洗料桶\") = vbYes Then\n     Fix32.THISNODE.YT6022_SJ2147_TANK2_REQUEST.f_cv = 0\n     Fix32.THISNODE.YT6022_SJ2147_TANK2_REUSE.f_cv = 0\n     Fix32.THISNODE.YT6022_SJ2147_TANK2_CLEAR_S.f_cv = 0\n     Call Modlogin.Oplog((0), (0), (1), \"取消清洗料桶\")\n    End If\n  Else\n    If MsgBox(\"确定要清洗料桶吗？\", vbYesNo, \"清洗料桶\") = vbYes Then\n     Fix32.THISNODE.YT6022_SJ2147_TANK2_REQUEST.f_cv = 0\n     Fix32.THISNODE.YT6022_SJ2147_TANK2_REUSE.f_cv = 0\n     Fix32.THISNODE.YT6022_SJ2147_TANK2_CLEAR_S.f_cv = 1\n     Fix32.THISNODE.YT6022_SJ2147Tank2Brand.A_CV = \"\"\n     Fix32.THISNODE.YT6022_SJ2147Tank2LotID1.A_CV = \"\"\n     Fix32.THISNODE.YT6022_SJ2147Tank2LotID2.A_CV = \"\"\n     Call Modlogin.Oplog((0), (0), (1), \"清洗料桶\")\n    End If",null,null,"YT6022_SJ2147_TANK2_CLEAR_S"]
[{"$nulls":3},"料筒清洗取消-料筒2","无","L5KYPJL_ZHStopRec_Tank2_ClearCANCEL","get",null,null,"FIX.YT6022_SJ2147_TANK2_REQUEST.F_CV  0\nFIX.YT6022_SJ2147_TANK2_REUSE.F_CV  0\nFIX.YT6022_SJ2147_TANK2_CLEAR_S.F_CV  0",{"$nulls":3},"YT6022_SJ2147_TANK2_CLEAR_S"]
[null,null,"信息清零","批结束","无","L5KYPJL_ZHStopInfoClear_BatchEnd","get",null,null,"FIX.YT6022_TASK2_bSTOP.F_CV  1\nFIX.YT6022_TASK2_bSTART.F_CV  0","     Fix32.THISNODE.YT6022_TASK2_bSTOP.F_CV = 1\n     Fix32.THISNODE.YT6022_TASK2_bSTART.F_CV = 0\n  Fix32.THISNODE.YT6022_YSTJ.F_CV = Fix32.THISNODE.YT6022_YSTJ.F_CV + Fix32.THISNODE.YT6022_VALUE_SJ2147_W_P4.F_CV\n    ",null,null,"YT6022_TASK2_bSTOP"]
[{"$nulls":3},"任务结束加料段","无","L5KYPJL_ZHStopInfoClear_TankClear","get",null,null,"FIX.YT6022_IN_TASK2_FINISH.F_CV 1\nFIX.YT6022_task2_NODEB.F_CV 1\nFIX.YT6022_task2_ROUTE.F_CV 1","\nwritevalue 1, \"Fix32.THISNODE.YT6022_IN_TASK2_FINISH.F_CV\", 1\nwritevalue 0, \"Fix32.THISNODE.YT6022_task2_NODEB.F_CV\", 1\nwritevalue 0, \"Fix32.THISNODE.YT6022_task2_ROUTE.F_CV\", 1",null,null,"YT6022_IN_TASK2_FINISH"]
[{"$nulls":3},"进柜段任务结束","无","L5KYPJL_ZHStopInfoClear_TankEND","get",null,"FIX.JK_YT630_IN_TASK2_FINISH_OK.F_CV 1","FIX.JK_YT630_IN_TASK2_FINISH.F_CV 1","If MsgBox(\"是否任务结束？\", vbOKCancel + vbQuestion) = vbOK Then\n\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_A03.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_A01.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_A02.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_A04.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_A05.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_A06.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_A07.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_A08.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_A09.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_A10.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_A11.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_A12.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_A13.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_A14.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_A15.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_A16.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_A17.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_A18.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_A19.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_A20.F_CV\"\n\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_R04.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_R05.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_R06.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_R07.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_R08.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_R09.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_R10.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_R11.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK2_R14.F_CV\"\n\n\nEnd If\nCall Modlogin.Oplog((1), (0), (1), \"叶片进柜任务2—5000任务结束 \")\n",null,null,"FIX.YT630_IN_TASK2_A03.F_CV  0\nFIX.YT630_IN_TASK2_A01.F_CV\nFIX.YT630_IN_TASK2_A02.F_CV\nFIX.YT630_IN_TASK2_A04.F_CV\nFIX.YT630_IN_TASK2_A05.F_CV\nFIX.YT630_IN_TASK2_A06.F_CV\nFIX.YT630_IN_TASK2_A07.F_CV\nFIX.YT630_IN_TASK2_A08.F_CV\nFIX.YT630_IN_TASK2_A09.F_CV\nFIX.YT630_IN_TASK2_A10.F_CV\nFIX.YT630_IN_TASK2_A11.F_CV\nFIX.YT630_IN_TASK2_A12.F_CV\nFIX.YT630_IN_TASK2_A13.F_CV\nFIX.YT630_IN_TASK2_A14.F_CV\nFIX.YT630_IN_TASK2_A15.F_CV\nFIX.YT630_IN_TASK2_A16.F_CV\nFIX.YT630_IN_TASK2_A17.F_CV\nFIX.YT630_IN_TASK2_A18.F_CV\nFIX.YT630_IN_TASK2_A19.F_CV\nFIX.YT630_IN_TASK2_A20.F_CV\n"]
[{"$nulls":3},"批次清零","无","L5KYPJL_ZHStopInfoClear_BatchClear","get",null,"FIX.JK_YT6022_LEAFBPC_CLEAR_OK.F_CV 1","FIX.JK_YT6022_LEAFBPC_CLEAR.F_CV 1","\nFix32.THISNODE.YT6022_C_SJ2147_WATER_CLEAR.F_CV=1/累计加水量清零\n\nFix32.THISNODE.YT6022_2143_CLEAR.F_CV = 1/称2143清零\nFix32.THISNODE.YT6022_C_SJ2147_STUFF_CL1.F_CV = 1/加料机2147加料量累计清零",null,null,"JK_YT6022_LEAFBPC_CLEAR"]
[{"$nulls":3},"生产清零","无","L5KYPJL_ZHStopInfoClear_ProdClear","get",null,"FIX.JK_YT6022_LEAFBSC_CLEAR_OK.F_CV 1","FIX.JK_YT6022_LEAFBSC_CLEAR.F_CV 1","WriteValue \"\", \"FIX32.THISNODE.YT6022_LEAFBATCHNO.A_CV\", 2 /叶片段当前批次号\nWriteValue \"0\", \"FIX32.THISNODE.YT6022_LEAFBATCHSEQ.F_CV\", 2 /批次顺序\nWriteValue \"\", \"FIX32.THISNODE.YT6022_LEAFBRAND.A_CV\", 2  /叶片段当前牌号\nWriteValue \"\", \"FIX32.THISNODE.YT6022_LEAFENTRYID.A_CV\", 2 /EntryID\nWriteValue \"\", \"FIX32.THISNODE.YT6022_LEAFINGP1.A_CV\", 2 /预计入柜号1\nWriteValue \"0\", \"FIX32.THISNODE.YT6022_LEAFINGP1AMOUNT.F_CV\", 2/入1柜料量\nWriteValue \"\", \"FIX32.THISNODE.YT6022_LEAFINGP2.A_CV\", 2/预计入柜号2\nWriteValue \"0\", \"FIX32.THISNODE.YT6022_LEAFINGP2AMOUNT.F_CV\", 2/入2柜料量\nWriteValue \"\", \"FIX32.THISNODE.YT6022_LEAFINGP3.A_CV\", 2/预计入柜号3\nWriteValue \"0\", \"FIX32.THISNODE.YT6022_LEAFINGP3AMOUNT.F_CV\", 2/入3柜料量\nWriteValue \"0\", \"FIX32.THISNODE.YT6022_LEAFINGPQTY.F_CV\", 2/生成物料入的柜子数量\nWriteValue \"\", \"FIX32.THISNODE.YT6022_LEAFJHJSSJ.A_CV\", 2/叶片段计划结束时间\nWriteValue \"\", \"FIX32.THISNODE.YT6022_LEAFJHKSSJ.A_CV\", 2/叶片段计划开始时间\nWriteValue \"\", \"FIX32.THISNODE.YT6022_LEAFOUTGP.A_CV\", 2/预混柜出柜号\nWriteValue \"0\", \"FIX32.THISNODE.YT6022_LEAFPRODMIX.F_CV\", 2/产出物是否汇集\nWriteValue \"0\", \"FIX32.THISNODE.YT6022_LEAFROAD.F_CV\", 2/生产工艺路线\nWriteValue \"\", \"FIX32.THISNODE.YT6022_LEAFSTUFFBRAND.A_CV\", 2/叶片段当前料液牌号\nWriteValue \"0\", \"FIX32.THISNODE.YT6022_LEAFWEIGHT.F_CV\", 2/叶片段当前重量",null,null,"JK_YT6022_LEAFBSC_CLEAR"]
[{"$nulls":3},"出预配柜路径清零","柜号","L5KYPJL_ZHStopInfoClear_OutYPG_PathClear(string YPNo)","post","YP04/YP05/YP06/YP07",null,"YT6022_TASK2_B04\n/YT6022_TASK2_B03\n/YT6022_TASK2_B02\n/YT6022_TASK2_B01",{"$nulls":3},"YT6022_TASK2_B04\n/YT6022_TASK2_B03\n/YT6022_TASK2_B02\n/YT6022_TASK2_B01"]
[{"$nulls":3},"出预配柜信息清零","柜号","L5KYPJL_ZHStopInfoClear_OutYPG_InfoClear(string YPNo)","post","YP04/YP05/YP06/YP07",null,"YT6022_GP_2139R_JOB(YP04批次)\n/YT6022_GP_2139R_BRAND（牌号）\nYT6022_GP_2139L_JOB(YP05批次)\n/YT6022_GP_2139L_BRAND（牌号）\nYT6022_GP_2138R_JOB(YP06批次)\n/YT6022_GP_2138R_BRAND（牌号）\nYT6022_GP_2138L_JOB(YP07批次)\n/YT6022_GP_2138L_BRAND（牌号）",{"$nulls":3},"YT6022_GP_2139R_JOB(YP04批次)\n/YT6022_GP_2139R_BRAND（牌号）\nYT6022_GP_2139L_JOB(YP05批次)\n/YT6022_GP_2139L_BRAND（牌号）\nYT6022_GP_2138R_JOB(YP06批次)\n/YT6022_GP_2138R_BRAND（牌号）\nYT6022_GP_2138L_JOB(YP07批次)\n/YT6022_GP_2138L_BRAND（牌号）"]
[{"$nulls":3},"进叶柜路径清零","进叶柜号","L5KYPJL_ZHStopInfoClear_InYG_PathClear(string YGNo)","post","YG01~YG24",null,"YG02/JK_YT630_IN_task2_A01 （写0）\nYG04/JK_YT630_IN_task2_A02\nYG06/JK_YT630_IN_task2_A03\nYG08/JK_YT630_IN_task2_A04\nYG10/JK_YT630_IN_task2_A05\nYG12/JK_YT630_IN_task2_A06\nYG14/JK_YT630_IN_task2_A07\nYG16/JK_YT630_IN_task2_A08\nYG01/JK_YT630_IN_task2_A09\nYG03/JK_YT630_IN_task2_A10\nYG05/JK_YT630_IN_task2_A11\nYG07/JK_YT630_IN_task2_A12\nYG09/JK_YT630_IN_task2_A13\nYG11/JK_YT630_IN_task2_A14\nYG13/JK_YT630_IN_task2_A15\nYG15/JK_YT630_IN_task2_A16\nYG18/JK_YT630_IN_task2_A17\nYG20/JK_YT630_IN_task2_A18\nYG22/JK_YT630_IN_task2_A19\nYG24/JK_YT630_IN_task2_A20",{"$nulls":3},"YG02/JK_YT630_IN_task2_A01 （写0）\nYG04/JK_YT630_IN_task2_A02\nYG06/JK_YT630_IN_task2_A03\nYG08/JK_YT630_IN_task2_A04\nYG10/JK_YT630_IN_task2_A05\nYG12/JK_YT630_IN_task2_A06\nYG14/JK_YT630_IN_task2_A07\nYG16/JK_YT630_IN_task2_A08\nYG01/JK_YT630_IN_task2_A09\nYG03/JK_YT630_IN_task2_A10\nYG05/JK_YT630_IN_task2_A11\nYG07/JK_YT630_IN_task2_A12\nYG09/JK_YT630_IN_task2_A13\nYG11/JK_YT630_IN_task2_A14\nYG13/JK_YT630_IN_task2_A15\nYG15/JK_YT630_IN_task2_A16\nYG18/JK_YT630_IN_task2_A17\nYG20/JK_YT630_IN_task2_A18\nYG22/JK_YT630_IN_task2_A19\nYG24/JK_YT630_IN_task2_A20"]
[{"$nulls":3},"进叶柜信息清零（单机操作）","进叶柜号","L5KYPJL_ZHStopInfoClear_InYG_InfoClear(string YGNo)","post","YG01~YG24",null,"YG01/YT630_1129A_JOB（批次）/YT630_1129A_BRAND（牌号）\nYG02/YT630_1129_JOB/YT630_1129_BRAND\nYG03/YT630_1129_1A_JOB/YT630_1129_1A_BRAND\nYG04/YT630_1129_1_JOB/YT630_1129_1_BRAND\nYG05/YT630_1129_2A_JOB/YT630_1129_2A_BRAND\nYG06/YT630_1129_2_JOB/YT630_1129_2_BRAND\nYG07/YT630_1129_3A_JOB/YT630_1129_3A_BRAND\nYG08/YT630_1129_3_JOB/YT630_1129_3_BRAND\nYG09/YT630_1129_4A_JOB/YT630_1129_4A_BRAND\nYG10/YT630_1129_4_JOB/YT630_1129_4_BRAND\nYG11/YT630_1129_5A_JOB/YT630_1129_5A_BRAND\nYG12/YT630_1129_5_JOB/YT630_1129_5_BRAND\nYG13/YT630_1129_6A_JOB/YT630_1129_6A_BRAND\nYG14/YT630_1129_6_JOB/YT630_1129_6_BRAND\nYG15/YT630_1129_7A_JOB/YT630_1129_7A_BRAND\nYG16/YT630_1129_7_JOB/YT630_1129_7_BRAND\nYG18/YT630_1153_JOB/YT630_1153_BRAND\nYG20/YT630_1153_1_JOB/YT630_1153_1_BRAND\nYG22/YT630_1153_2_JOB/YT630_1153_2_BRAND\nYG24/YT630_1153_3_JOB/YT630_1153_3_BRAND",{"$nulls":3},"YG01/YT630_1129A_JOB（批次）/YT630_1129A_BRAND（牌号）\nYG02/YT630_1129_JOB/YT630_1129_BRAND\nYG03/YT630_1129_1A_JOB/YT630_1129_1A_BRAND\nYG04/YT630_1129_1_JOB/YT630_1129_1_BRAND\nYG05/YT630_1129_2A_JOB/YT630_1129_2A_BRAND\nYG06/YT630_1129_2_JOB/YT630_1129_2_BRAND\nYG07/YT630_1129_3A_JOB/YT630_1129_3A_BRAND\nYG08/YT630_1129_3_JOB/YT630_1129_3_BRAND\nYG09/YT630_1129_4A_JOB/YT630_1129_4A_BRAND\nYG10/YT630_1129_4_JOB/YT630_1129_4_BRAND\nYG11/YT630_1129_5A_JOB/YT630_1129_5A_BRAND\nYG12/YT630_1129_5_JOB/YT630_1129_5_BRAND\nYG13/YT630_1129_6A_JOB/YT630_1129_6A_BRAND\nYG14/YT630_1129_6_JOB/YT630_1129_6_BRAND\nYG15/YT630_1129_7A_JOB/YT630_1129_7A_BRAND\nYG16/YT630_1129_7_JOB/YT630_1129_7_BRAND\nYG18/YT630_1153_JOB/YT630_1153_BRAND\nYG20/YT630_1153_1_JOB/YT630_1153_1_BRAND\nYG22/YT630_1153_2_JOB/YT630_1153_2_BRAND\nYG24/YT630_1153_3_JOB/YT630_1153_3_BRAND"]
[null,null,"设备组合停止",null,"无","L5KYPJL_ZHStop_Stop","get",null,null,"FIX.YT630_IN_TASK2_STop.F_CV  1\nFIX.YT6022_IN_TASK2_STOP.F_CV  1","       Fix32.THISNODE.YT630_IN_TASK2_STop.F_CV = 1\n       Fix32.THISNODE.YT6022_IN_TASK2_STOP.F_CV = 1",null,null,"YT6022_IN_TASK2_STOP"]
[null,"辅助操作","单机/联机",null,"段号","L5KYPJL_FK_DeviceLink(string DeviceName,Bool Bsel)"]
[null,null,"故障复位（两个复位，一起）",null,"无","L5KYPJL_FK_AlarmReset","get",null,null,"FIX.YT6022_CONTROL_YT6022_RESET.F_CV  1",{"$nulls":3},"YT6022_CONTROL_YT6022_RESET"]

{"sheet":"Sheet6","index":6,"n_rows":15,"n_cols":4,"rows_kept":15,"flags":["formulas_cached_only"]}
["public","string","工序","{get;set;}"]
["public","string","操作按钮","{get;set;}"]
["public","string","组件封装","{get;set;}"]
["public","string","业务说明","{get;set;}"]
["public","string","参数说明","{get;set;}"]
["public","string","API接口名","{get;set;}"]
["public","string","API请求方式","{get;set;}"]
["public","string",null,"{get;set;}"]
["public","string","API传入参数","{get;set;}"]
["public","string","API接口检查点位","{get;set;}"]
["public","string","API接口写入点","{get;set;}"]
["public","string","触发脚本","{get;set;}"]
["public","string","备注","{get;set;}"]
["public","string","API状态","{get;set;}"]
["public","string","IFIX点位","{get;set;}"]

{"sheet":"Sheet1","index":7,"n_rows":21,"n_cols":7,"rows_kept":21,"flags":["formulas_cached_only"]}
["apiName","param","InputName","WriteTagName","CheckTagName","StrValue","DelayTime"]
["L5KYPJL_ZHStart_InYGCancel","YG02",null,"FIX.YT630_IN_task2_A01.F_CV","FIX.YT630_IN_task2_A01.F_CV",0,1500]
["L5KYPJL_ZHStart_InYGCancel","YG04",null,"FIX.YT630_IN_task2_A02.F_CV","FIX.YT630_IN_task2_A02.F_CV",0,1500]
["L5KYPJL_ZHStart_InYGCancel","YG06",null,"FIX.YT630_IN_task2_A03.F_CV","FIX.YT630_IN_task2_A03.F_CV",0,1500]
["L5KYPJL_ZHStart_InYGCancel","YG08",null,"FIX.YT630_IN_task2_A04.F_CV","FIX.YT630_IN_task2_A04.F_CV",0,1500]
["L5KYPJL_ZHStart_InYGCancel","YG10",null,"FIX.YT630_IN_task2_A05.F_CV","FIX.YT630_IN_task2_A05.F_CV",0,1500]
["L5KYPJL_ZHStart_InYGCancel","YG12",null,"FIX.YT630_IN_task2_A06.F_CV","FIX.YT630_IN_task2_A06.F_CV",0,1500]
["L5KYPJL_ZHStart_InYGCancel","YG14",null,"FIX.YT630_IN_task2_A07.F_CV","FIX.YT630_IN_task2_A07.F_CV",0,1500]
["L5KYPJL_ZHStart_InYGCancel","YG16",null,"FIX.YT630_IN_task2_A08.F_CV","FIX.YT630_IN_task2_A08.F_CV",0,1500]
["L5KYPJL_ZHStart_InYGCancel","YG01",null,"FIX.YT630_IN_task2_A09.F_CV","FIX.YT630_IN_task2_A09.F_CV",0,1500]
["L5KYPJL_ZHStart_InYGCancel","YG03",null,"FIX.YT630_IN_task2_A10.F_CV","FIX.YT630_IN_task2_A10.F_CV",0,1500]
["L5KYPJL_ZHStart_InYGCancel","YG05",null,"FIX.YT630_IN_task2_A11.F_CV","FIX.YT630_IN_task2_A11.F_CV",0,1500]
["L5KYPJL_ZHStart_InYGCancel","YG07",null,"FIX.YT630_IN_task2_A12.F_CV","FIX.YT630_IN_task2_A12.F_CV",0,1500]
["L5KYPJL_ZHStart_InYGCancel","YG09",null,"FIX.YT630_IN_task2_A13.F_CV","FIX.YT630_IN_task2_A13.F_CV",0,1500]
["L5KYPJL_ZHStart_InYGCancel","YG11",null,"FIX.YT630_IN_task2_A14.F_CV","FIX.YT630_IN_task2_A14.F_CV",0,1500]
["L5KYPJL_ZHStart_InYGCancel","YG13",null,"FIX.YT630_IN_task2_A15.F_CV","FIX.YT630_IN_task2_A15.F_CV",0,1500]
["L5KYPJL_ZHStart_InYGCancel","YG15",null,"FIX.YT630_IN_task2_A16.F_CV","FIX.YT630_IN_task2_A16.F_CV",0,1500]
["L5KYPJL_ZHStart_InYGCancel","YG18",null,"FIX.YT630_IN_task2_A17.F_CV","FIX.YT630_IN_task2_A17.F_CV",0,1500]
["L5KYPJL_ZHStart_InYGCancel","YG20",null,"FIX.YT630_IN_task2_A18.F_CV","FIX.YT630_IN_task2_A18.F_CV",0,1500]
["L5KYPJL_ZHStart_InYGCancel","YG22",null,"FIX.YT630_IN_task2_A19.F_CV","FIX.YT630_IN_task2_A19.F_CV",0,1500]
["L5KYPJL_ZHStart_InYGCancel","YG24",null,"FIX.YT630_IN_task2_A20.F_CV","FIX.YT630_IN_task2_A20.F_CV",0,1500]

{"sheet":"进叶柜","index":8,"n_rows":26,"n_cols":18,"rows_kept":26,"merged":[[1,0,25,0],[1,1,11,1],[12,1,23,1],[13,2,22,2],[20,3,22,3],[24,1,25,1]],"flags":["formulas_cached_only"]}
["工序","操作按钮","组件封装","业务说明","参数说明","API接口名",null,"API方式","API传入参数","API接口检查点位","API接口写入点","触发脚本","备注","API状态","IFIX点位","代码生成","配置文件","代码标记"]
["3000配叶柜\n进叶柜","组合启动","工单信息下发",null,"工单号、批次号、牌号","L3KYPYG_ZHStart_GDInfoSet(json) 示例：string GDNum,string BatchNum,string BrandNum","L3KYPYG_ZHStart_GDInfoSet","Post",null,null,"THISNODE.YT6023C_EntryID.A_CV\nTHISNODE.YT6023C_BatchNo.A_CV\nTHISNODE.YT6023C_Brand.A_CV"]
[null,null,"启用生产关联","启用生产关联","无","L3KYPYG_ZHStart_DevLinkEnable","L3KYPYG_ZHStart_DevLinkEnable","Get",null,null,"THISNODE.YT630_IN_TASK3_LINK.F_CV 1",{"$nulls":4},"case 'api/L3KYPYG_ZHStart_DevLinkEnable':   //启用生产关联\n                    rlt = AppUtil.WriteAndCheckListComm(AppUtil.GetConfig(ModuleEnum.L3_JYG), 'L3KYPYG_ZHStart_DevLinkEnable'); break;"]
[null,null,"取消生产关联","取消生产关联","无","L3KYPYG_ZHStart_DevLinkDisable","L3KYPYG_ZHStart_DevLinkDisable","Get",null,null,"THISNODE.YT630_IN_TASK3_LINK.F_CV 0",{"$nulls":4},"case 'api/L3KYPYG_ZHStart_DevLinkDisable':   //取消生产关联\n                    rlt = AppUtil.WriteAndCheckListComm(AppUtil.GetConfig(ModuleEnum.L3_JYG), 'L3KYPYG_ZHStart_DevLinkDisable'); break;"]
[null,null,"任务开始","任务开始","无","L3KYPYG_ZHStart_TaskStart","L3KYPYG_ZHStart_TaskStart","Get",null,null,"thisnode.YT630_IN_TASK3_START.F_CV 1\nthisnode.YT630_IN_TASK3_STop.F_CV 0",{"$nulls":4},"case 'api/L3KYPYG_ZHStart_TaskStart':   //任务开始\n                    rlt = AppUtil.WriteAndCheckListComm(AppUtil.GetConfig(ModuleEnum.L3_JYG), 'L3KYPYG_ZHStart_TaskStart'); break;"]
[null,null,"批开始","批开始","无","L3KYPYG_ZHStart_BatchStart","L3KYPYG_ZHStart_BatchStart","Get",null,null,"THISNODE.YT6023_TASK3_bSTART.F_CV 1\nTHISNODE.YT6023_TASK3_bSTOP.F_CV 0",{"$nulls":4},"case 'api/L3KYPYG_ZHStart_BatchStart':   //批开始\n                    rlt = AppUtil.WriteAndCheckListComm(AppUtil.GetConfig(ModuleEnum.L3_JYG), 'L3KYPYG_ZHStart_BatchStart'); break;"]
[null,null,"出配叶柜验证","设备组合启动","柜号","L3KYPYG_ZHStart_OutPYGCheck(string GPno)","L3KYPYG_ZHStart_OutPYGCheck","Post","YP01/YP02","THISNODE.JK_YT6023_TASK3_OUT_0_OK.F_CV\nTHISNODE.JK_YT6023_TASK3_OUT_02_OK.F_CV","THISNODE.JK_YT6023_TASK3_OUT_01.F_CV  1\nTHISNODE.JK_YT6023_TASK3_OUT_02.F_CV   1",null,"If READvalue(\"Fix32.THISNODE.YT6023_TASK2_NODE_IN_01.F_CV\", 1) = 1 Then\n   MsgBox \"切片任务中此柜被选做进柜，不能同时进柜，请确认后操作！\", vbOKOnly + vbCritical, \"单元选择冲突\"\n   Exit Sub\nEnd If\nIf READvalue(\"Fix32.THISNODE.YT6023_TASK2_NODE_FIRST_01.F_CV\", 1) = 1 Then\n   MsgBox \"切片任务中此柜被选做进柜，不能同时进柜，请确认后操作！\", vbOKOnly + vbCritical, \"单元选择冲突\"\n   Exit Sub\nEnd If\nIf READvalue(\"Fix32.THISNODE.YT6023_TASK2_NODE_SECOND_01.F_CV\", 1) = 1 Then\n   MsgBox \"切片任务中此柜被选做进柜，不能同时进柜，请确认后操作！\", vbOKOnly + vbCritical, \"单元选择冲突\"\n   Exit Sub\nEnd If\nIf READvalue(\"Fix32.THISNODE.YT6023_TASK2_NODE_THIRD_01.F_CV\", 1) = 1 Then\n   MsgBox \"切片任务中此柜被选做进柜，不能同时进柜，请确认后操作！\", vbOKOnly + vbCritical, \"单元选择冲突\"\n   Exit Sub\nEnd If\n\nwritevalue 1, \"Fix32.THISNODE.YT6023_TASK3_NODE_OUT_01.F_CV\", 1\nIf User.YT6023_TASK3_LINK.CurrentValue = True Then\n   writevalue 1, \"Fix32.THISNODE.YT6023_TASK3_R15.F_CV\", 1\nEnd If"]
[null,null,"出配叶柜取消","批结束","柜号","L3KYPYG_ZHStart_OutPYGCancel(string GPno)","L3KYPYG_ZHStart_OutPYGCancel","Post","YP01/YP02","THISNODE.JK_YT6023_TASK3_OUT_CLEAR_OK.F_CV \nTHISNODE.JK_YT6023_TASK3_OUT2_CLEAR_OK.F_CV ","THISNODE.JK_YT6023_TASK3_OUT1_CLEAR.F_CV  1\nTHISNODE.JK_YT6023_TASK3_OUT2_CLEAR.F_CV   1"]
[null,null,"进叶柜条件验证及路径下发",null,"柜号","L3KYPYG_ZHStart_InYPGPathSet(string GPno)","L3KYPYG_ZHStart_InYPGPathSet","Post",null,"YG8/THISNODE.JK_YT630_IN_TASK3_A7_OK.F_CV\nYG20/THISNODE.JK_YT630_IN_TASK3_A8_OK.F_CV\nYG22/THISNODE.JK_YT630_IN_TASK3_A9_OK.F_CV \nYG24/THISNODE.JK_YT630_IN_TASK3_A20_OK.F_CV \nYG7/THISNODE.JK_YT630_IN_TASK3_A2_OK.F_CV \nYG9/THISNODE.JK_YT630_IN_TASK3_A22_OK.F_CV \nYG2/THISNODE.JK_YT630_IN_TASK3_A23_OK.F_CV \nYG23/THISNODE.JK_YT630_IN_TASK3_A24_OK.F_CV \n","YG18/THISNODE.JK_YT630_IN_TASK3_A17.F_CV 1\nYG20/THISNODE.JK_YT630_IN_TASK3_A18.F_CV 1\nYG22/THISNODE.JK_YT630_IN_TASK3_A19.F_CV 1\nYG24/THISNODE.JK_YT630_IN_TASK3_A20.F_CV 1\nYG17/THISNODE.JK_YT630_IN_TASK3_A21.F_CV 1 \nYG19/THISNODE.JK_YT630_IN_TASK3_A22.F_CV 1\nYG21/THISNODE.JK_YT630_IN_TASK3_A23.F_CV 1\nYG23/THISNODE.JK_YT630_IN_TASK3_A24.F_CV 1\n",null,"writevalue \"1\", \"Fix32.THISNODE.YT630_IN_task3_A17.F_CV\"\n\nwritevalue \"0\", \"Fix32.THISNODE.YT630_IN_task3_A18.F_CV\"\nwritevalue \"0\", \"Fix32.THISNODE.YT630_IN_task3_A19.F_CV\"\nwritevalue \"0\", \"Fix32.THISNODE.YT630_IN_task3_A20.F_CV\"\nwritevalue \"0\", \"Fix32.THISNODE.YT630_IN_task3_A21.F_CV\"\nwritevalue \"0\", \"Fix32.THISNODE.YT630_IN_task3_A22.F_CV\"\nwritevalue \"0\", \"Fix32.THISNODE.YT630_IN_task3_A23.F_CV\"\nwritevalue \"0\", \"Fix32.THISNODE.YT630_IN_task3_A24.F_CV\""]
[null,null,"进叶柜路径取消",null,"柜号","L3KYPYG_ZHStart_InYPGPathCancel(string GPno)","L3KYPYG_ZHStart_InYPGPathCancel","Post",null,null,"YG18/THISNODE.YT630_IN_TASK3_A17.F_CV 0\nYG20/THISNODE.YT630_IN_TASK3_A18.F_CV 0\nYG22/THISNODE.YT630_IN_TASK3_A19.F_CV 0\nYG24/THISNODE.YT630_IN_TASK3_A20.F_CV 0\nYG17/THISNODE.YT630_IN_TASK3_A21.F_CV 0\nYG19/THISNODE.YT630_IN_TASK3_A22.F_CV 0\nYG21/THISNODE.YT630_IN_TASK3_A23.F_CV 0\nYG23/THISNODE.YT630_IN_TASK3_A24.F_CV 0\n"]
[null,null,"进叶柜信息下发",null,"柜号、批次号、牌号","L3KYPYG_ZHStart_InYPGInfoSet(string GPno)","L3KYPYG_ZHStart_InYPGInfoSet","Post",null,null,"YG18/THISNODE.YT630_1153_JOB.A_CV/THISNODE.YT630_1153_BRAND.A_CV\nYG20/THISNODE.YT630_1153_1_JOB.A_CV/THISNODE.YT630_1153_1_BRAND.A_CV\nYG22/THISNODE.YT630_1153_2_JOB.A_CV/THISNODE.YT630_1153_2_BRAND.A_CV\nYG24/THISNODE.YT630_1153_3_JOB.A_CV/THISNODE.YT630_1153_3_BRAND.A_CV\nYG17/THISNODE.YT630_1153A_JOB.A_CV/THISNODE.YT630_1153A_BRAND.A_CV\nYG19/THISNODE.YT630_1153_1A_JOB.A_CV/THISNODE.YT630_1153_1A_BRAND.A_CV\nYG21/THISNODE.YT630_1153_2A_JOB.A_CV/THISNODE.YT630_1153_2A_BRAND.A_CV\nYG23/THISNODE.YT630_1153_3A_JOB.A_CV/THISNODE.YT630_1153_3A_BRAND.A_CV\n"]
[null,null,"设备组合启动","设备组合启动","无","L3KYPYG_ZHStart_Start",null,"Get",null,"THISNODE.JK_YT6023_TASK3_START_OK.F_CV ","THISNODE.JK_YT6023_TASK3_START.F_CV 1","THISNODE.YT6023_TASK3_START.F_CV = 1\n THISNODE.YT630_IN_TASK3_START.F_CV =1\nFix32.THISNODE.YT630_IN_TASK3_STop.F_CV =0",{"$nulls":3},"case 'api/L3KYPYG_ZHStart_Start':   //设备组合启动\n                    rlt = AppUtil.WriteAndCheckListComm(AppUtil.GetConfig(ModuleEnum.L3_JYG), 'L3KYPYG_ZHStart_Start'); break;"]
[null,"组合停止","批结束","批结束","无","L3KYPYG_ZHStop_BatchEnd",null,"Get",null,null,"THISNODE.YT6023_TASK3_bSTOP.F_CV 1\nTHISNODE.YT6023_TASK3_bSTART.F_CV 0\n  ",{"$nulls":4},"case 'api/L3KYPYG_ZHStop_BatchEnd':   //批结束\n                    rlt = AppUtil.WriteAndCheckListComm(AppUtil.GetConfig(ModuleEnum.L3_JYG), 'L3KYPYG_ZHStop_BatchEnd'); break;"]
[null,null,"信息清零","任务停止","无","L3KYPYG_ZHStopInfoClear_TaskStop",null,"Get",null,null,"thisnode.YT630_IN_TASK3_STop.F_CV 1\nthisnode.YT630_IN_TASK3_START.F_CV 0",{"$nulls":4},"case 'api/L3KYPYG_ZHStopInfoClear_TaskStop':   //任务停止\n                    rlt = AppUtil.WriteAndCheckListComm(AppUtil.GetConfig(ModuleEnum.L3_JYG), 'L3KYPYG_ZHStopInfoClear_TaskStop'); break;"]
[{"$nulls":3},"任务结束","无","L3KYPYG_ZHStopInfoClear_TaskEnd",null,"Get",null,null,"thisnode.YT630_IN_TASK3_A17.F_CV 0\nthisnode.YT630_IN_TASK3_A18.F_CV 0\nthisnode.YT630_IN_TASK3_A19.F_CV 0\nthisnode.YT630_IN_TASK3_A20.F_CV 0\nthisnode.YT630_IN_TASK3_A21.F_CV 0\nthisnode.YT630_IN_TASK3_A22.F_CV 0\nthisnode.YT630_IN_TASK3_A23.F_CV 0\nthisnode.YT630_IN_TASK3_A24.F_CV 0\nthisnode.YT630_IN_TASK3_R12.F_CV 0\nthisnode.YT630_IN_TASK3_R13.F_CV 0\nthisnode.YT630_IN_TASK3_R14.F_CV 0\nthisnode.YT630_IN_TASK3_R15.F_CV 0\n",{"$nulls":4},"case 'api/L3KYPYG_ZHStopInfoClear_TaskEnd':   //任务结束\n                    rlt = AppUtil.WriteAndCheckListComm(AppUtil.GetConfig(ModuleEnum.L3_JYG), 'L3KYPYG_ZHStopInfoClear_TaskEnd'); break;"]
[{"$nulls":3},"批次清零","无","L3KYPYG_ZHStopInfoClear_BatchClear",null,"Get",null,null,"THISNODE.YT630_3000_OUT_BATCH_STOP.F_CV 1",{"$nulls":4},"case 'api/L3KYPYG_ZHStopInfoClear_BatchClear':   //批次清零\n                    rlt = AppUtil.WriteAndCheckListComm(AppUtil.GetConfig(ModuleEnum.L3_JYG), 'L3KYPYG_ZHStopInfoClear_BatchClear'); break;"]
[{"$nulls":3},"生产清零","无","L3KYPYG_ZHStopInfoClear_ProdClear",null,"Get",null," THISNODE.JK_YT6023_LAMINASC_CLEAR_OK.F_CV","THISNODE.JK_YT6023_LAMINASC_CLEAR.F_CV 1",null,"writevalue 0, \"\"Fix32.THISNODE.YT6023C_BATCHSEQ.F_CV\"\", 1  '批次顺序\nwritevalue 0, \"\"Fix32.THISNODE.YT6023C_INGP1AMOUNT.F_CV\"\", 1  '入1柜料量\nwritevalue 0, \"\"Fix32.THISNODE.YT6023C_INGP2AMOUNT.F_CV\"\", 1  '入2柜料量\nwritevalue 0, \"\"Fix32.THISNODE.YT6023C_INGP3AMOUNT.F_CV\"\", 1  '入3柜料量\nwritevalue 0, \"\"Fix32.THISNODE.YT6023C_INGPQTY.F_CV\"\", 1  '生成物料入的柜子数量\n\nWriteValue \"\"\"\", \"\"FIX32.THISNODE.YT6023C_BATCHNO.A_CV\"\", 2 '/3k线配叶出柜段当前批次号\n\nWriteValue \"\"\"\", \"\"FIX32.THISNODE.YT6023C_BRAND.A_CV\"\", 2 ' /3k线配叶出柜段当前牌号\nWriteValue \"\"\"\", \"\"FIX32.THISNODE.YT6023C_ENTRYID.A_CV\"\", 2 '/EntryID\nWriteValue \"\"\"\", \"\"FIX32.THISNODE.YT6023C_INGP1.A_CV\"\", 2' /预计入柜号1\nWriteValue \"\"\"\", \"\"FIX32.THISNODE.YT6023C_INGP2.A_CV\"\", 2'/预计入柜号2\nWriteValue \"\"\"\", \"\"FIX32.THISNODE.YT6023C_INGP3.A_CV\"\", 2'/预计入柜号3\nWriteValue \"\"\"\", \"\"FIX32.THISNODE.YT6023C_JHJSSJ.A_CV\"\", 2'/3k线配叶出柜段计划结束时间\nWriteValue \"\"\"\", \"\"FIX32.THISNODE.YT6023C_JHKSSJ.A_CV\"\", 2'/3k线配叶出柜段计划开始时间\nWriteValue \"\"\"\", \"\"FIX32.THISNODE.YT6023C_OUTGP.A_CV\"\", 2'/3k线配叶出柜段出柜号\nWriteValue \"\"0\"\", \"\"FIX32.THISNODE.YT6023C_PRODMIX.F_CV\"\", 2'/产出物是否汇集\nWriteValue \"\"0\"\", \"\"FIX32.THISNODE.YT6023C_ROAD.F_CV\"\", 2'/生产工艺路线\nWriteValue \"\"\"\", \"\"FIX32.THISNODEY.YT6023C_STUFFBRAND.A_CV\"\", 2'/3k线配叶出柜段当前料液牌号\nWriteValue \"\"0\"\", \"\"FIX32.THISNODE.YT6023C_WEIGHT.F_CV\"\", 2'/3k线配叶出柜段当前重量\n",null,null,"case 'api/L3KYPYG_ZHStopInfoClear_ProdClear':   //生产清零\n                    rlt = AppUtil.WriteAndCheckListComm(AppUtil.GetConfig(ModuleEnum.L3_JYG), 'L3KYPYG_ZHStopInfoClear_ProdClear'); break;"]
[{"$nulls":3},"进叶柜路径清零","无","L3KYPYG_ZHStopInfoClear_InYPGPathClear",null,"Get",null,null,"YG18/THISNODE.JK_YT630_IN_TASK3_A17.F_CV 0\nYG20/THISNODE.JK_YT630_IN_TASK3_A18.F_CV 0\nYG22/THISNODE.JK_YT630_IN_TASK3_A19.F_CV 0\nYG24/THISNODE.JK_YT630_IN_TASK3_A20.F_CV 0\nYG17/THISNODE.JK_YT630_IN_TASK3_A21.F_CV 0\nYG19/THISNODE.JK_YT630_IN_TASK3_A22.F_CV 0\nYG21/THISNODE.JK_YT630_IN_TASK3_A23.F_CV 0\nYG23/THISNODE.JK_YT630_IN_TASK3_A24.F_CV 0\n",{"$nulls":4},"case 'api/L3KYPYG_ZHStopInfoClear_InYPGPathClear':   //进叶柜路径清零\n                    rlt = AppUtil.WriteAndCheckListComm(AppUtil.GetConfig(ModuleEnum.L3_JYG), 'L3KYPYG_ZHStopInfoClear_InYPGPathClear'); break;"]
[{"$nulls":3},"出配叶柜路径清零","无","L3KYPYG_ZHStopInfoClear_OutPYGPathClear",null,"Get",null,null,"THISNODE.YT6023_TASK3_NODE_OUT.F_CV  0\nTHISNODE.YT6023_TASK1_ROUTE.F_CV   0",{"$nulls":4},"case 'api/L3KYPYG_ZHStopInfoClear_OutPYGPathClear':   //出配叶柜路径清零\n                    rlt = AppUtil.WriteAndCheckListComm(AppUtil.GetConfig(ModuleEnum.L3_JYG), 'L3KYPYG_ZHStopInfoClear_OutPYGPathClear'); break;"]
[{"$nulls":3},"进叶柜柜号清零","无","L3KYPYG_ZHStopInfoClear_InYPGInfoClear",{"$nulls":9},"case 'api/L3KYPYG_ZHStopInfoClear_InYPGInfoClear':   //进叶柜柜号清零\n                    rlt = AppUtil.WriteAndCheckListComm(AppUtil.GetConfig(ModuleEnum.L3_JYG), 'L3KYPYG_ZHStopInfoClear_InYPGInfoClear'); break;"]
[{"$nulls":3},"配丝柜信息清零","第1选柜(单柜号、批次号、牌号)\n"]
[{"$nulls":4},"第2选柜(单柜号、批次号、牌号)"]
[{"$nulls":4},"第3选柜(单柜号、批次号、牌号)"]
[null,null,"设备组合停止",null,"无","L3KYPYG_ZHStop_DevZHStop",null,"Get",null,null,"THISNODE.YT6023_TASK3_STOP.F_CV 1\n THISNODE.YT630_IN_TASK3_STop.F_CV 1\nTHISNODE.YT630_IN_TASK3_START.F_CV 0",{"$nulls":4},"case 'api/L3KYPYG_ZHStop_DevZHStop':   //\n                    rlt = AppUtil.WriteAndCheckListComm(AppUtil.GetConfig(ModuleEnum.L3_JYG), 'L3KYPYG_ZHStop_DevZHStop'); break;"]
[null,"辅助操作","单机/联机",null,"段号"]
[null,null,"故障复位",null,"无","L3KYPYG_FK_AlarmReset",null,"Get",null,null,"thisnode.YT630_CONTROL_YT630_RESET.F_CV 1",{"$nulls":4},"case 'api/L3KYPYG_FK_AlarmReset':   //\n                    rlt = AppUtil.WriteAndCheckListComm(AppUtil.GetConfig(ModuleEnum.L3_JYG), 'L3KYPYG_FK_AlarmReset'); break;"]