{"text_format":"3","workbook":"xls","n_sheets":9,"sheets":["9000回潮","9000加料","3000进叶柜加料","真空回潮","Sheet6","API封装需求","300加料","白肋烟","Sheet1"],"not_rendered":{"external_links":1,"defined_names":3},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"9000回潮","index":0,"n_rows":36,"n_cols":21,"rows_kept":36,"merged":[[1,0,35,0],[1,1,8,1],[9,1,23,1],[19,2,21,2],[24,1,26,1],[27,1,32,1],[28,2,31,2],[34,1,35,1]],"flags":["formulas_cached_only"]}
["工序","操作按钮","组件封装","业务说明","参数说明","API接口名1","是否验证","生成类型","选写多值","API接口名","写入点位","测试方法","检查点位","测试状态","测试输入","测试输出","测试点位变化","备注","API状态","按键逻辑","逻辑代码"]
["9千回潮","设备预热","预热启动-松散回潮",null,"无","L9KYPHC_YRSTART_HC",{"$nulls":3},"L9KYPHC_YRSTART_HC","THISNODE.K2_Z5TB1StartHeat_FK.F_CV=1\n","get",null,"\n   Fix32.THISNODE.K2_Z5TB1StartHeat_FK.F_CV = 1\n"]
[null,null,"预热启动-薄片",null,"无","L9KYPHC_YRSTART_BP",{"$nulls":3},"L9KYPHC_YRSTART_BP","THISNODE.YT6024_WQ3154_PREHEAT_START.F_CV=1\nTHISNODE.YT6024_WQ3154_PREHEAT_STOP.F_CV=0","get",null,"Fix32.THISNODE.YT6024_WQ3154_PREHEAT_START.F_CV = 1\nFix32.THISNODE.YT6024_WQ3154_PREHEAT_STOP.F_CV = 0"]
[null,null,"松散预热温度值设定",null,"温度值","L9KYPHC_YRHC_YRWDSET",null,"单写","20\n25\n30\n40","L9KYPHC_YRHC_YRWDSET(float tmp)","THISNODE.K2_Z5L1CurrRec_P_23.F_CV=","post",null,"无"]
[null,null,"薄片预热温度值设定",null,"温度值","L9KYPHC_YRPB_YRWDSET",null,"单写","20\n25\n30\n40","L9KYPHC_YRPB_YRWDSET(float tmp)","THISNODE.YT6024_WQ3154_SP1.F_CV=","post",null,"Fix32.THISNODE.YT6024_WQ3154_SP1.F_CV"]
[null,null,"松散预热生产温度值设定",null,"温度值","L9KYPHC_YRHC_YXWDSET",null,"单写","20\n25\n30\n40","L9KYPHC_YRHC_YXWDSET(float tmp)","THISNODE.K2_Z5L1CurrRec_P_23.F_CV=","post",null,"Fix32.THISNODE.K2_Z5L1CurrRec_P_23.F_CV"]
[null,null,"薄片预热生产温度值设定",null,"温度值","L9KYPHC_YRPB_YXWDSET",null,"单写",null,"L9KYPHC_YRPB_YXWDSET(float tmp)","THISNODE.YT6024_WQ3154_SP15.F_CV=","get",null,"Fix32.THISNODE.YT6024_WQ3154_SP15.F_CV"]
[null,null,"预热结束-松散回潮",null,"无","L9KYPHC_YRCLOSE_HC",{"$nulls":3},"L9KYPHC_YRCLOSE_HC","THISNODE.K2_Z5TB1StopHeat_FK.F_CV=1","get",null,"Fix32.THISNODE.K2_Z5TB1StopHeat_FK.F_CV = 1"]
[null,null,"预热结束-薄片",null,"无","L9KYPHC_YRCLOSE_BP",{"$nulls":3},"L9KYPHC_YRCLOSE_BP","THISNODE.YT6024_WQ3154_PREHEAT_START.F_CV=0\nTHISNODE.YT6024_WQ3154_PREHEAT_STOP.F_CV=1","get",null,"Fix32.THISNODE.YT6024_WQ3154_PREHEAT_START.F_CV = 0\nFix32.THISNODE.YT6024_WQ3154_PREHEAT_STOP.F_CV = 1"]
[null,"组合启动","生产路径选择","薄片旁线","无","L9KYPHC_ZHQD_PATHSelZK",{"$nulls":3},"L9KYPHC_ZHQD_PATHSelZK","THISNODE.YT602_TASK1_YT602_4_Sel.F_CV=1","get",null," Fix32.THISNODE.YT602_TASK1_YT602_4_Sel.F_CV = 1"]
[{"$nulls":3},"薄片取消","无","L9KYPHC_ZHQD_PATHSelQP",{"$nulls":3},"L9KYPHC_ZHQD_PATHSelQP","THISNODE.YT602_TASK1_YT602_4_Sel.F_CV=0","get",null,"Fix32.THISNODE.YT602_TASK1_YT602_4_Sel.F_CV = 0"]
[{"$nulls":3},"选择切片","无","L9KYPHC_YCJL_PATHSELECT",{"$nulls":3},"L9KYPHC_YCJL_PATHSELECT","THISNODE.YT602_FT1105_Cut_No.F_CV=1","get",null,"Fix32.THISNODE.YT602_FT1105_Cut_No.F_CV = 1"]
[{"$nulls":3},"取消切片","无","L9KYPHC_YCJL_PATHCANCEL",{"$nulls":3},"L9KYPHC_YCJL_PATHCANCEL","THISNODE.YT602_FT1105_Cut_No.F_CV=0","get",null," Fix32.THISNODE.YT602_FT1105_Cut_No.F_CV = 0"]
[{"$nulls":3},"进白肋烟","无","L9KYPHC_BPPX_PATHSELECT",{"$nulls":3},"L9KYPHC_BPPX_PATHSELECT","THISNODE.YT602_TASK1_YT612_Sel.F_CV=1","get",null,"Fix32.THISNODE.YT602_TASK1_YT612_Sel.F_CV = 1"]
[{"$nulls":3},"取消白肋烟","无","L9KYPHC_BPPX_PATHCANCEL",{"$nulls":3},"L9KYPHC_BPPX_PATHCANCEL","THISNODE.YT602_TASK1_YT612_Sel.F_CV=0","get",null," Fix32.THISNODE.YT602_TASK1_YT612_Sel.F_CV = 0"]
[null,null,"工单信息下发",null,"工单号、批次号、牌号","L9KYPHC_PathSel_DirectIn",null,"多写2",null,"L9KYPHC_PathSel_DirectIn","THISNODE.PreMixEntryID.A_CV\nTHISNODE.PreMixBatchNo.A_CV\nTHISNODE.PreMixBrand.A_CV","post",null,"Fix32.THISNODE.PreMixEntryID.A_CV\n/Fix32.THISNODE.PreMixBatchNo.A_CV\n/Fix32.THISNODE.PreMixBrand.A_CV"]
[null,null,"批开始",null,"无","L9KYPHC_PathSel_DirectInCancel",{"$nulls":3},"L9KYPHC_PathSel_DirectInCancel","THISNODE.YT602PreMixBatchStart.F_CV=1\nTHISNODE.YT602PREMIXBATCHEND.F_CV=0","get",null,"Fix32.THISNODE.YT602PreMixBatchStart.F_CV = 1\n       Fix32.THISNODE.YT602PREMIXBATCHEND.F_CV = 0"]
[null,null,"进预配柜条件验证",null,"柜号(单柜号)","L9KYPHC_ZHQD_GDMSGWRITE",null,"选单写","YP01,YP02,YP03","L9KYPHC_ZHQD_GDMSGWRITE(string GDNum) JSON方式","THISNODE.YT602_R03_START.F_CV=1\nTHISNODE.YT602_R04_START.F_CV=1\nTHISNODE.YT602_R05_START.F_CV=1","post",null,"YP01/Fix32.THISNODE.YT602_R03_START.F_CV   1\nYP02/Fix32.THISNODE.YT602_R04_START.F_CV  1\nYP03/Fix32.THISNODE.YT602_R05_START.F_CV  1"]
[null,null,"进预配柜条件取消",null,null,"L9KYPHC_ZHQD_GDMSGWRITE_Cancel",null,"选单写","YP01,YP02,YP03","L9KYPHC_ZHQD_GDMSGWRITE_Cancel(string GDNum,string BatchNum,string BrandNum) JSON方式","THISNODE.YT602_R03_START.F_CV=0\nTHISNODE.YT602_R04_START.F_CV=0\nTHISNODE.YT602_R05_START.F_CV=0","post",null,"YP01/Fix32.THISNODE.YT602_R03_START.F_CV   0\nYP02/Fix32.THISNODE.YT602_R04_START.F_CV  0\nYP03/Fix32.THISNODE.YT602_R05_START.F_CV  0"]
[null,null,"进预配柜信息下发",null,"柜号(多个柜以逗号分割)、批次号、牌号","L9KYPHC_ZHQD_YPGSelno1_InfoSet",null,"选多写","YP01,YP02,YP03","L9KYPHC_ZHQD_YPGSelno1_InfoSet(string GPNum,string BatchNum,string BrandNum) JSON方式\n","THISNODE.YT602_GP1112_JOB1.A_CV,THISNODE.YT602_GP1112_BRAND1.A_CV\nTHISNODE.YT602_GP1112_1_JOB1.A_CV,THISNODE.YT602_GP1112_1_BRAND1.A_CV\nTHISNODE.YT602_GP1112_2_JOB1.A_CV,THISNODE.YT602_GP1112_2_BRAND1.A_CV","post",null,"YP01/YT602_GP1112_JOB1/YT602_GP1112_BRAND1\n     /YT602_GP1112_JOB2/YT602_GP1112_BRAND2\n      /YT602_GP1112_JOB3/YT602_GP1112_BRAND3\nYP02/YT602_GP1112_1_JOB1\n\n\nYP03/\n\n\n\n"]
[{"$nulls":4},"柜号(多个柜以逗号分割)、批次号、牌号","L9KYPHC_ZHQD_YPGSelno2_InfoSet",null,"选多写","YP01,YP02,YP03","L9KYPHC_ZHQD_YPGSelno2_InfoSet(string GPNum,string BatchNum,string BrandNum) JSON方式\n","THISNODE.YT602_GP1112_JOB2.A_CV,THISNODE.YT602_GP1112_BRAND2.A_CV\nTHISNODE.YT602_GP1112_1_JOB2.A_CV,THISNODE.YT602_GP1112_1_BRAND2.A_CV\nTHISNODE.YT602_GP1112_2_JOB2.A_CV,THISNODE.YT602_GP1112_2_BRAND2.A_CV"]
[{"$nulls":4},"柜号(多个柜以逗号分割)、批次号、牌号","L9KYPHC_ZHQD_YPGSelno3_InfoSet",null,"选多写","YP01,YP02,YP03","L9KYPHC_ZHQD_YPGSelno3_InfoSet(string GPNum,string BatchNum,string BrandNum) JSON方式\n","THISNODE.YT602_GP1112_JOB3.A_CV,THISNODE.YT602_GP1112_BRAND3.A_CV\nTHISNODE.YT602_GP1112_1_JOB3.A_CV,THISNODE.YT602_GP1112_1_BRAND3.A_CV\nTHISNODE.YT602_GP1112_2_JOB3.A_CV,THISNODE.YT602_GP1112_2_BRAND3.A_CV"]
[null,null,"薄片旁线组合启动",null,"无","L9KYPHC_BPPXZHQD_Start",{"$nulls":3},"L9KYPHC_BPPXZHQD_Start","THISNODE.YT6024_START.F_CV=1","get",null,"Fix32.THISNODE.YT6024_START.F_CV = 1"]
[null,null,"设备组合启动",null,"无","L9KYPHC_ZHQD_Start",{"$nulls":3},"L9KYPHC_ZHQD_Start","THISNODE.JK_YT602_TASK1_START.F_CV=1","get","THISNODE.JK_YT602_TASK1_START_OK.F_CV=1","If judgeRole(\"操作员\", \"YT602\") = -1 Then Exit Sub\n  If MsgBox(\"确定要组合启动吗？\", vbYesNo, \"组合启动\") = vbYes Then\n    'Fix32.ThISNODE.YT602PreMixGStart.F_CV = 1\n    Fix32.THISNODE.YT602_TASK1_START.F_CV = 1\n    Fix32.THISNODE.K2_Z5Grp1Start_FK.F_CV = 1\n    Call modlogin.Oplog((1), (0), (1), \"预混段组合启动操作\")\n    'If Fix32.ThISNODE.WQ3204Sel.F_CV = 1\n    If Fix32.THISNODE.YT602_TASK1_YT602_4_Sel.F_CV = 1 Then\n       Fix32.THISNODE.YT6024_START.F_CV = 1\n       Call modlogin.Oplog((1), (0), (1), \"薄片旁线组合启动操作\")\n    End If\n'    Call modlogin.OpLogGS(\"TS602A\")\n  End If\n","  If MsgBox(\"确定要组合启动吗？\", vbOkCancle, \"组合启动\") = vbOK Then\n    Fix32.THISNODE.YT602PreMixGStart.f_cv = 1\n    Call modlogin.Oplog((1), (0), (1), \"YT602预混段组合启动操作\")\n    If Fix32.THISNODE.WQ3204Sel.f_cv = 1 Then\n       Fix32.THISNODE.YT6024_START.f_cv = 1\n       Call modlogin.Oplog((1), (0), (1), \"薄片旁线组合启动操作\")\n    End If\n  End If"]
[null,"生产提升","生产提升-薄片",null,"无","L9KYPHC_TS_BPHCSTART",{"$nulls":3},"L9KYPHC_TS_BPHCSTART","Thisnode.YT6024_WP3151_CONTROL1.f_CV=1","get",null,"Fix32.Thisnode.YT6024_WP3151_CONTROL1.f_cv = 1"]
[null,null,"强制提升-薄片",null,"无","L9KYPHC_TS_BPHCFORCE",{"$nulls":3},"L9KYPHC_TS_BPHCFORCE","Thisnode.YT6024_WP3151_CONTROL2.f_CV=1","get",null," Fix32.Thisnode.YT6024_WP3151_CONTROL2.f_cv = 1"]
[null,null,"强制停止提升-薄片",null,"无","L9KYPHC_TS_BPHCSTOP",{"$nulls":3},"L9KYPHC_TS_BPHCSTOP","Thisnode.YT6024_WP3151_CONTROL3.f_CV=1","get",null,"       Fix32.Thisnode.YT6024_WP3151_CONTROL3.f_cv = 1"]
[null,"组合停止","批结束",null,"无","L9KYPHC_ZHSTOP_BATCH_END",{"$nulls":3},"L9KYPHC_ZHSTOP_BATCH_END","THISNODE.YT602PreMixBatchStart.F_CV=0\nTHISNODE.YT602PREMIXBATCHEND.F_CV=1\n","get",null,"  Fix32.THISNODE.YT602PreMixBatchStart.F_CV = 0\n       Fix32.THISNODE.YT602PREMIXBATCHEND.F_CV = 1\n       "]
[null,null,"信息清零","任务结束","无","L9KYPHC_ZHSTOP_TASK_END",{"$nulls":3},"L9KYPHC_ZHSTOP_TASK_END","THISNODE.YT602_TASK1_END.F_CV=1\nTHISNODE.YT602_R03_START.F_CV=0\nTHISNODE.YT602_R04_START.F_CV=0\nTHISNODE.YT602_R05_START.F_CV=0","get",null,"writevalue 1, \"Fix32.THISNODE.YT602_TASK1_STOP.F_CV\", 1"]
[{"$nulls":3},"批次清零","无","L9KYPHC_ZHSTOP_CLEAR_BATCH",{"$nulls":3},"L9KYPHC_ZHSTOP_CLEAR_BATCH","THISNODE.K2_Z5Grp1ResTot_FK.F_CV=1\nTHISNODE.YT6024_WQ3154_STUFF_CL1.F_CV=0\nTHISNODE.YT6024_CK3152_CLEAR.F_CV=0\n","get"]
[{"$nulls":3},"生产清零","无","L9KYPHC_ZHSTOP_CLEAR_PRODINFO",{"$nulls":3},"L9KYPHC_ZHSTOP_CLEAR_PRODINFO","THISNODE.JK_YT602_MIXENTSC_CLEAR.f_CV=1\n","get","THISNODE.JK_YT602_MIXENTSC_CLEAR_ok.f_CV=1","THISNODE.K2_Z5L1CurrRec_P_38.F_CV = 0\nTHISNODE.CK1107AAccmFlowDB.F_CV = 0\nTHISNODE.K2_Z5L1CurrRec_P_21.F_CV = 0\nTHISNODE.CK3202AccmFlowDB.F_CV = 0\nTHISNODE.CK3202FlowSet.F_CV = 0\nTHISNODE.YT602_R03_START.F_CV = 0\nTHISNODE.YT602_R04_START.F_CV = 0\nTHISNODE.YT602_R05_START.F_CV = 0\nTHISNODE.LAPTOTALACCUMDB.F_CV = 0\nTHISNODE.K2_Z5L1CurrRec_P_24.F_CV = 0\nTHISNODE.YT602_TASK1_SEL.F_CV = 0\nTHISNODE.WQ3204AccmWaterDB.F_CV = 0\nTHISNODE.WQ3204InMoistSet.F_CV = 0\nTHISNODE.WQ3204RollPreHeatTemSet.F_CV = 0\nTHISNODE.WQ3204RollWorkTemSet.F_CV = 0\nTHISNODE.YT602_TASK1_YT602_4_Sel.F_CV = 0\nTHISNODE.GP3104InSelCur.F_CV = 0\nTHISNODE.GP3104_1InSelCur.F_CV = 0\nTHISNODE.K2_Z5L1CurrRec_P_23.F_CV = 0\nTHISNODE.YT602_TASK1_YT612_Sel.F_CV = 0\nTHISNODE.K2_Z5L1CurrRec_P_26.F_CV = 0\nTHISNODE.K2_Z5L1CurrRec_P_28.F_CV = 0\nTHISNODE.K2_Z5L1CurrRec_P_29.F_CV = 0\nTHISNODE.K2_Z5L1CurrRec_P_30.F_CV = 0\nTHISNODE.K2_Z5L1CurrRec_P_31.F_CV = 0\nTHISNODE.K2_Z5L1CurrRec_P_36.F_CV = 0\nTHISNODE.K2_Z5L1CurrRec_P_37.F_CV = 0\nTHISNODE.PREMIXBATCHSEQ.F_CV = 0\nTHISNODE.PREMIXINGP1AMOUNT.F_CV = 0\nTHISNODE.PREMIXINGP2AMOUNT.F_CV = 0\nTHISNODE.PREMIXINGP3AMOUNT.F_CV = 0\nTHISNODE.PREMIXINGPQTY.F_CV = 0\nTHISNODE.PREMIXPRODMIX.F_CV = 0\nTHISNODE.YT602_TASK2_BATCHEND.F_CV = 0\nTHISNODE.PREMIXWEIGHT.F_CV = 0\nTHISNODE.K2_Z5L1CurrRec_P_23.F_CV = 0\nTHISNODE.YT6024_WQ3154_SP15.F_CV = 0\nTHISNODE.WQ1118StuffRatioset.F_CV = 0\nTHISNODE.PREMIXBATCHNO.A_CV = \"\"\nTHISNODE.PREMIXBRAND = \"\"\nTHISNODE.PREMIXENTRYID.A_CV = \"\"\n\nTHISNODE.PREMIXOUTGP.A_CV = \"\"\nTHISNODE.PREMIXINGP1.A_CV = \"\"\nTHISNODE.PREMIXINGP2.A_CV = \"\"\nTHISNODE.PREMIXINGP3.A_CV = \"\"\nTHISNODE.PREMIXJHJSSJ.A_CV = \"\"\nTHISNODE.PREMIXJHKSSJ.A_CV = \"\"\n","THISNODE.K2_Z5L1CurrRec_P_38.F_CV = 0\nTHISNODE.CK1107AAccmFlowDB.F_CV = 0\nTHISNODE.K2_Z5L1CurrRec_P_21.F_CV = 0\nTHISNODE.CK3202AccmFlowDB.F_CV = 0\nTHISNODE.CK3202FlowSet.F_CV = 0\nTHISNODE.YT602_R03_START.F_CV = 0\nTHISNODE.YT602_R04_START.F_CV = 0\nTHISNODE.YT602_R05_START.F_CV = 0\nTHISNODE.LAPTOTALACCUMDB.F_CV = 0\nTHISNODE.K2_Z5L1CurrRec_P_24.F_CV = 0\nTHISNODE.YT602_TASK1_SEL.F_CV = 0\nTHISNODE.WQ3204AccmWaterDB.F_CV = 0\nTHISNODE.WQ3204InMoistSet.F_CV = 0\nTHISNODE.WQ3204RollPreHeatTemSet.F_CV = 0\nTHISNODE.WQ3204RollWorkTemSet.F_CV = 0\nTHISNODE.YT602_TASK1_YT602_4_Sel.F_CV = 0\nTHISNODE.GP3104InSelCur.F_CV = 0\nTHISNODE.GP3104_1InSelCur.F_CV = 0\nTHISNODE.K2_Z5L1CurrRec_P_23.F_CV = 0\nTHISNODE.YT602_TASK1_YT612_Sel.F_CV = 0\nTHISNODE.K2_Z5L1CurrRec_P_26.F_CV = 0\nTHISNODE.K2_Z5L1CurrRec_P_28.F_CV = 0\nTHISNODE.K2_Z5L1CurrRec_P_29.F_CV = 0\nTHISNODE.K2_Z5L1CurrRec_P_30.F_CV = 0\nTHISNODE.K2_Z5L1CurrRec_P_31.F_CV = 0\nTHISNODE.K2_Z5L1CurrRec_P_36.F_CV = 0\nTHISNODE.K2_Z5L1CurrRec_P_37.F_CV = 0\nTHISNODE.PREMIXBATCHSEQ.F_CV = 0\nTHISNODE.PREMIXINGP1AMOUNT.F_CV = 0\nTHISNODE.PREMIXINGP2AMOUNT.F_CV = 0\nTHISNODE.PREMIXINGP3AMOUNT.F_CV = 0\nTHISNODE.PREMIXINGPQTY.F_CV = 0\nTHISNODE.PREMIXPRODMIX.F_CV = 0\nTHISNODE.YT602_TASK2_BATCHEND.F_CV = 0\nTHISNODE.PREMIXWEIGHT.F_CV = 0\nTHISNODE.K2_Z5L1CurrRec_P_23.F_CV = 0\nTHISNODE.YT6024_WQ3154_SP15.F_CV = 0\nTHISNODE.WQ1118StuffRatioset.F_CV = 0\nTHISNODE.PREMIXBATCHNO.A_CV = \"\"\nTHISNODE.PREMIXBRAND = \"\"\nTHISNODE.PREMIXENTRYID.A_CV = \"\"\n\nTHISNODE.PREMIXOUTGP.A_CV = \"\"\nTHISNODE.PREMIXINGP1.A_CV = \"\"\nTHISNODE.PREMIXINGP2.A_CV = \"\"\nTHISNODE.PREMIXINGP3.A_CV = \"\"\nTHISNODE.PREMIXJHJSSJ.A_CV = \"\"\nTHISNODE.PREMIXJHKSSJ.A_CV = \"\"\n"]
[{"$nulls":3},"预配柜柜号清零","无","L9KYPHC_ZHSTOP_CLEAR_YPGnoINFO",{"$nulls":3},"L9KYPHC_ZHSTOP_CLEAR_YPGnoINFO"]
[null,null,"设备组合停止",null,"无","L9KYPHC_ZHSTOP_STOP",{"$nulls":3},"L9KYPHC_ZHSTOP_STOP","THISNODE.JK_YT602_TASK1_STOP.f_CV=1\n","get","THISNODE.JK_YT602_TASK1_STOP_OK.f_CV=1","    If MsgBox(\"确定要组合停止吗？\", vbYesNo, \"组合停止\") = vbYes Then\n       Fix32.THISNODE.YT602PreMixGStop.f_cv = 1\n       Call modlogin.Oplog((1), (0), (1), \"YT602预混段组合停止操作\")\n       If Fix32.THISNODE.WQ3204Sel.f_cv = 1 Then   'WQ3204当前选中\n          Fix32.THISNODE.YT6024_STOP.f_cv = 1\n       Call modlogin.Oplog((1), (0), (1), \"薄片旁线组合停止操作\")\n     End If\n    End If"]
[null,null,"薄片旁线组合停止",null,"无","L9KYPHC_PXBPZHSTOP_STOP",{"$nulls":3},"L9KYPHC_PXBPZHSTOP_STOP","THISNODE.YT6024_STOP.F_CV=1","get",null,"  Fix32.THISNODE.YT6024_STOP.F_CV = 1"]
[null,"辅助操作","单机/联机",null,"段号"]
[null,null,"故障复位",null,"无","L9KYPHC_FK_Alarm_ALLReset",{"$nulls":3},"L9KYPHC_FK_Alarm_ALLReset","THISNODE.K2_Z5Grp1ResTot_FK.F_CV=1\n","get",null,"If Fix32.THISNODE.K2_Z5Grp1CntrMode.F_CV = 4 Then\nIf MsgBox(\"是否确定全部复位？\", vbOKCancel, \"操作提示\") = vbOK Then\n   Fix32.THISNODE.K2_Z5Grp1ResTot_FK.F_CV = 1\n   Call Modlogin.Oplog((1), \"0\", \"1\", (\"回潮段全部复位\"))\n   End If\n\nElse\nMsgBox \"控制模式不是远程自动，操作无效！\", vbOKOnly, \"操作提示\"\nEnd If"]

{"sheet":"9000加料","index":1,"n_rows":66,"n_cols":22,"rows_kept":66,"merged":[[1,0,65,0],[1,1,4,1],[5,1,14,1],[17,1,30,1],[31,1,33,1],[35,1,63,1],[36,2,53,2],[54,2,62,2],[64,1,65,1]],"flags":["formulas_cached_only"]}
["工序","操作按钮","组件封装","业务说明","参数说明","API接口名","API接口名1","是否验证","生成类型","选写多值","测试方法","API传入参数","API测试结果","检查点位","写入点位","触发脚本","备注","API状态","IFIX点位","代码生成","配置文件","代码标记"]
["9千加料","设备预热","预热启动",null,"无","L9KYPJL_SBYR_START","L9KYPJL_SBYR_START",{"$nulls":3},"get",{"$nulls":3},"THISNODE.K3_Z6ST1_StartHeat_FK.F_CV = 1"," Fix32.THISNODE.K3_Z6ST1_StartHeat_FK.F_CV = 1"]
[null,null,"预热温度值设定",null,"温度值","L9KYPJL_SBYR_YRWDSET(float Temp)","L9KYPJL_SBYR_YRWDSET",null,"单写",null,"Post","15\n20\n30\n50",null,null,"THISNODE.K3_Z6L1CurrRec_P_1.F_CV"]
[null,null,"预热生产温度值设定",null,"温度值","L9KYPJL_SBYR_YXWDSET(float Temp)","L9KYPJL_SBYR_YXWDSET",{"$nulls":3},"Post","15\n20\n30\n50",null,null,"THISNODE.K3_Z6L1CurrRec_P_1.F_CV"]
[null,null,"预热结束",null,"无","L9KYPJL_SBYR_CLOSE","L9KYPJL_SBYR_CLOSE",{"$nulls":3},"Get",{"$nulls":3},"THISNODE.K3_Z6ST1_StopHeat_FK.F_CV = 1"]
[null,"要料","料筒选择-料筒1",null,"无","L9KYPJL_YL_Tank1Select","L9KYPJL_YL_Tank1Select",{"$nulls":3},"Get",{"$nulls":3},"THISNODE.K3_Z6L1CurrConf_P_3.F_CV = 1"]
[null,null,"料筒选择-料筒不选",null,"无","L9KYPJL_YL_TankNoSelect","L9KYPJL_YL_TankNoSelect",{"$nulls":3},"Get",{"$nulls":3},"THISNODE.K3_Z6L1CurrConf_P_3.F_CV = 0"]
[null,null,"料筒选择-料筒2",null,"无","L9KYPJL_YL_Tank2Select","L9KYPJL_YL_Tank2Select",{"$nulls":3},"Get",{"$nulls":3},"THISNODE.K3_Z6L1CurrConf_P_3.F_CV = 2"]
[null,null,"自动选择料筒",null,null,"L9KYPJL_YL_TankAutoSelect","L9KYPJL_YL_TankAutoSelect",{"$nulls":3},"Get",null,null,"THISNODE.JK_K3_Z6L1CurrConf_P_3_OK.F_CV=1 ","THISNODE.JK_K3_Z6L1CurrConf_P_3.F_CV =1","If Fix32.THISNODE.K3_Z6L1CurrConf_P_3.F_CV = 99 Then\n   Fix32.THISNODE.K3_Z6L1CurrConf_P_3.F_CV = 0\nElse\n   Fix32.THISNODE.K3_Z6L1CurrConf_P_3.F_CV = 99\nEnd If"]
[null,null,"要料信息下发-料筒1",null,"料液重量、料液代码、批次号","L9KYPJL_YL_Tank1Info_Set(object info)","L9KYPJL_YL_Tank1Info_Set",null,"多写1",null,"POST","{\"Weight\":123,\"BatchNum\":\"abdj\",\"BrandNum\":\"123akdk\"}",null,null,"THISNODE.WQ1108Tank1AskQty.F_CV\nTHISNODE.WQ1108Tank1AskBatch.A_CV\nTHISNODE.WQ1108Tank1AskBrand.A_CV\n"]
[null,null,"要料信息下发-料筒2",null,"料液重量、料液代码、批次号","L9KYPJL_YL_Tank2Info_Set(object info)","L9KYPJL_YL_Tank2Info_Set",null,"多写1",null,"POST","{\"Weight\":123,\"BatchNum\":\"abdj\",\"BrandNum\":\"123akdk\"}",null,null,"THISNODE.WQ1108Tank2AskQty.F_CV \nTHISNODE.WQ1108Tank2AskBatch.A_CV \nTHISNODE.WQ1108Tank2AskBrand.A_CV  "]
[null,null,"要料请求-料筒1",null,null,"L9KYPJL_YL_Tank1Req","L9KYPJL_YL_Tank1Req",{"$nulls":3},"Get",{"$nulls":3},"THISNODE.WQ1108Tank1Request.F_CV = 1","THISNODE.K3_Z6KA1AskStuff_FK.F_CV = 1"]
[null,null,"取消要料-料筒1",null,null,"L9KYPJL_YL_Tank1Cancel","L9KYPJL_YL_Tank1Cancel",{"$nulls":3},"Get",{"$nulls":3},"THISNODE.WQ1108Tank1Request.F_CV = 0","THISNODE.K3_Z6KA1AskStuffEnd_FK.F_CV = 1"]
[null,null,"要料请求-料筒2",null,"无","L9KYPJL_YL_Tank2Req","L9KYPJL_YL_Tank2Req",{"$nulls":3},"Get",{"$nulls":3},"  THISNODE.WQ1108Tank2Request.F_CV = 1","THISNODE.K3_Z6KA2AskStuff_FK.F_CV = 1"]
[null,null,"取消要料-料筒2",null,"无","L9KYPJL_YL_Tank2Cancel","L9KYPJL_YL_Tank2Cancel",{"$nulls":3},"Get",{"$nulls":3},"  THISNODE.WQ1108Tank2Request.F_CV = 0","THISNODE.K3_Z6KA2AskStuffEnd_FK.F_CV = 1"]
[null,null,"选择白肋烟掺兑",null,null,"L9KYPJL_YL_BLYBlend","L9KYPJL_YL_BLYBlend",{"$nulls":3},"Get",{"$nulls":3},"THISNODE.YT602_TASK2_YT612_Sel.F_CV = 1"]
[null,null,"取消白肋烟掺兑",null,null,"L9KYPJL_YL_BLYBlendCancel","L9KYPJL_YL_BLYBlendCancel",{"$nulls":3},"Get",{"$nulls":3},"THISNODE.YT602_TASK2_YT612_Sel.F_CV = 0"]
[null,"组合启动","工单信息下发",null,"工单号、批次号、牌号","L9KYPJL_ZHStart_GDInfoSet","L9KYPJL_ZHStart_GDInfoSet",null,"多写2",null,"POST","{\"GDNum\":\"abddd\",\"BatchNum\":\"23432\",\"BrandNum\":\"uutu3333\"}",null,null,"THISNODE.LeafInYGEntryID.A_CV\nTHISNODE.LeafInYGBatchNo.A_CV\nTHISNODE.LeafInYGBrand.A_CV"]
[null,null,"批开始",null,"无","L9KYPJL_ZHStart_BatchStart","L9KYPJL_ZHStart_BatchStart",{"$nulls":3},"Get",{"$nulls":3},"THISNODE.YT602InGPBatchStart.F_CV = 1\nTHISNODE.YT602INGPBATCHEND.F_CV = 0"]
[null,null,"叶片段任务2选择",null,null,"L9KYPJL_ZHStart_TASK2Sel","L9KYPJL_ZHStart_TASK2Sel",{"$nulls":3},"Get",{"$nulls":3},"THISNODE.YT602_TASK2_SEL.F_CV =1"]
[null,null,"叶片段任务2取消选择",null,null,"L9KYPJL_ZHStart_TASK2SelCancel","L9KYPJL_ZHStart_TASK2SelCancel",{"$nulls":3},"Get",{"$nulls":3},"THISNODE.YT602_TASK2_SEL.F_CV =0"]
[null,null,"叶片线叶片段任务2结束",null,null,"L9KYPJL_ZHStart_TASK2FINISH","L9KYPJL_ZHStart_TASK2FINISH",{"$nulls":3},"Get",{"$nulls":3},"THISNODE.YT602_TASK2_END.F_CV= 1"]
[null,null,"出预配柜任务启动",null,null,"L9KYPJL_ZHStart_OutYPGStart","L9KYPJL_ZHStart_OutYPGStart",{"$nulls":3},"Get",{"$nulls":3},"THISNODE.YT602_TASK2_START.F_CV= 1"]
[null,null,"进页柜任务启动",null,null,"L9KYPJL_ZHStart_INYPGStart","L9KYPJL_ZHStart_INYPGStart",{"$nulls":3},"Get",{"$nulls":3},"thisnode.YT630_IN_TASK1_START.F_CV =1\nthisnode.YT630_IN_TASK1_STop.F_CV =0"]
[null,null,"出预配柜条件验证及路径下发",null,"柜号R06/R07/R08","L9KYPJL_ZHStart_OutPGCheck(string Slotno）","L9KYPJL_ZHStart_OutPGCheck",null,"选单写","R06,R07,R08","Post",{"$nulls":3},"THISNODE.YT602_R06_START.F_CV=1\nTHISNODE.YT602_R07_START.F_CV=1\nTHISNODE.YT602_R08_START.F_CV=1\n\n"]
[null,null,"出预配柜路径取消",null,"柜号R06/R07/R09","L9KYPJL_ZHStart_OutPGCancel(string Slotno）","L9KYPJL_ZHStart_OutPGCancel",null,"选单写","R06,R07,R08","Post",{"$nulls":3},"THISNODE.YT602_R06_START.F_CV=0\nTHISNODE.YT602_R07_START.F_CV=0\nTHISNODE.YT602_R08_START.F_CV=0\n\n"]
[null,null,"出预配柜信息下发",null,"柜号","L9KYPJL_ZHStart_OutPGInfoSet(string Slotno）","L9KYPJL_ZHStart_OutPGInfoSet",null,"选单写","R06,R07,R08"]
[null,null,"进叶柜条件验证及路径下发",null,"柜号","L9KYPJL_ZHStart_InYGPATHCheck(string Slotno）","L9KYPJL_ZHStart_InYGPATHCheck",null,"选单写","YG02,YG06,YG08,YG10,YG12,YG14,YG16,YG01,YG03,YG05,YG07,YG09,YG11,YG13,YG15","Post",null,null,"THISNODE.JK_YT630_IN_TASK1_A01_OK.F_CV=1\nTHISNODE.JK_YT630_IN_TASK1_A02_OK.F_CV=1\nTHISNODE.JK_YT630_IN_TASK1_A03_OK.F_CV=1\nTHISNODE.JK_YT630_IN_TASK1_A04_OK.F_CV=1\nTHISNODE.JK_YT630_IN_TASK1_A05_OK.F_CV=1\nTHISNODE.JK_YT630_IN_TASK1_A06_OK.F_CV=1\nTHISNODE.JK_YT630_IN_TASK1_A07_OK.F_CV=1\nTHISNODE.JK_YT630_IN_TASK1_A08_OK.F_CV=1\nTHISNODE.JK_YT630_IN_TASK1_A09_OK.F_CV=1\nTHISNODE.JK_YT630_IN_TASK1_A10_OK.F_CV=1\nTHISNODE.JK_YT630_IN_TASK1_A11_OK.F_CV=1\nTHISNODE.JK_YT630_IN_TASK1_A12_OK.F_CV=1\nTHISNODE.JK_YT630_IN_TASK1_A13_OK.F_CV=1\nTHISNODE.JK_YT630_IN_TASK1_A14_OK.F_CV=1\nTHISNODE.JK_YT630_IN_TASK1_A15_OK.F_CV=1\nTHISNODE.JK_YT630_IN_TASK1_A16_OK.F_CV=1","THISNODE.JK_YT630_IN_TASK1_A01.F_CV = 1\nTHISNODE.JK_YT630_IN_TASK1_A02.F_CV = 1\nTHISNODE.JK_YT630_IN_TASK1_A03.F_CV = 1\nTHISNODE.JK_YT630_IN_TASK1_A04.F_CV = 1\nTHISNODE.JK_YT630_IN_TASK1_A05.F_CV = 1\nTHISNODE.JK_YT630_IN_TASK1_A06.F_CV = 1\nTHISNODE.JK_YT630_IN_TASK1_A07.F_CV = 1\nTHISNODE.JK_YT630_IN_TASK1_A08.F_CV = 1\nTHISNODE.JK_YT630_IN_TASK1_A09.F_CV = 1\nTHISNODE.JK_YT630_IN_TASK1_A10.F_CV = 1\nTHISNODE.JK_YT630_IN_TASK1_A11.F_CV = 1\nTHISNODE.JK_YT630_IN_TASK1_A12.F_CV = 1\nTHISNODE.JK_YT630_IN_TASK1_A13.F_CV = 1\nTHISNODE.JK_YT630_IN_TASK1_A14.F_CV = 1\nTHISNODE.JK_YT630_IN_TASK1_A15.F_CV = 1\nTHISNODE.JK_YT630_IN_TASK1_A16.F_CV = 1",null,"YG02/THISNODE.JK_YT630_IN_TASK1_A01.F_CV （写1）\nYG04/THISNODE.JK_YT630_IN_TASK1_A02.F_CV\nYG06/THISNODE.JK_YT630_IN_TASK1_A03.F_CV\nYG08/THISNODE.JK_YT630_IN_TASK1_A04.F_CV\nYG10/THISNODE.JK_YT630_IN_TASK1_A05.F_CV\nYG12/THISNODE.JK_YT630_IN_TASK1_A06.F_CV\nYG14/THISNODE.JK_YT630_IN_TASK1_A07.F_CV\nYG16/THISNODE.JK_YT630_IN_TASK1_A08.F_CV\nYG01/THISNODE.JK_YT630_IN_TASK1_A09.F_CV\nYG03/THISNODE.JK_YT630_IN_TASK1_A10.F_CV\nYG05/THISNODE.JK_YT630_IN_TASK1_A11.F_CV\nYG07/THISNODE.JK_YT630_IN_TASK1_A12.F_CV\nYG09/THISNODE.JK_YT630_IN_TASK1_A13.F_CV\nYG11/THISNODE.JK_YT630_IN_TASK1_A14.F_CV\nYG13/THISNODE.JK_YT630_IN_TASK1_A15.F_CV\nYG15/THISNODE.JK_YT630_IN_TASK1_A16.F_CV\nYG18/THISNODE.JK_YT630_IN_TASK1_A17.F_CV\nYG20/THISNODE.JK_YT630_IN_TASK1_A18.F_CV\nYG22/THISNODE.JK_YT630_IN_TASK1_A19.F_CV\nYG24/THISNODE.JK_YT630_IN_TASK1_A20.F_CV"]
[null,null,"进叶柜路径取消",null,"柜号","L9KYPJL_ZHStart_InYGPATHCancel","L9KYPJL_ZHStart_InYGPATHCancel",null,"选单写","YG02,YG04,YG06,YG08,YG10,YG12,YG14,YG16,YG01,YG03,YG05,YG07,YG09,YG11,YG13,YG15","Post",{"$nulls":3},"THISNODE.YT630_IN_TASK1_A01.F_CV = 0\nTHISNODE.YT630_IN_TASK1_A02.F_CV = 0\nTHISNODE.YT630_IN_TASK1_A03.F_CV = 0\nTHISNODE.YT630_IN_TASK1_A04.F_CV = 0\nTHISNODE.YT630_IN_TASK1_A05.F_CV = 0\nTHISNODE.YT630_IN_TASK1_A06.F_CV = 0\nTHISNODE.YT630_IN_TASK1_A07.F_CV = 0\nTHISNODE.YT630_IN_TASK1_A08.F_CV = 0\nTHISNODE.YT630_IN_TASK1_A09.F_CV = 0\nTHISNODE.YT630_IN_TASK1_A10.F_CV = 0\nTHISNODE.YT630_IN_TASK1_A11.F_CV = 0\nTHISNODE.YT630_IN_TASK1_A12.F_CV = 0\nTHISNODE.YT630_IN_TASK1_A13.F_CV = 0\nTHISNODE.YT630_IN_TASK1_A14.F_CV = 0\nTHISNODE.YT630_IN_TASK1_A15.F_CV = 0\nTHISNODE.YT630_IN_TASK1_A16.F_CV = 0"]
[null,null,"进叶柜信息下发",null,"柜号、批次号、牌号","L9KYPJL_ZHStart_InPGInfoSet(string Slotno）","L9KYPJL_ZHStart_InPGInfoSet",null,"选多写","YG01 ,YG02 ,YG03 ,YG04 ,YG05 ,YG06 ,YG07,YG08 ,YG09 ,YG10 ,YG11,YG12 ,YG13 ,YG14 ,YG15 ","Post",{"$nulls":3},"THISNODE.YT630_1129A_JOB.A_CV,THISNODE. YT630_1129A_BRAND.A_CV\nTHISNODE.YT630_1129_JOB.A_CV ,THISNODE. YT630_1129_BRAND.A_CV\nTHISNODE.YT630_1129_1A_JOB.A_CV ,THISNODE. YT630_1129_1A_BRAND.A_CV\nTHISNODE.YT630_1129_1_JOB.A_CV ,THISNODE. YT630_1129_1_BRAND.A_CV\nTHISNODE.YT630_1129_2A_JOB.A_CV ,THISNODE. YT630_1129_2A_BRAND.A_CV\nTHISNODE.YT630_1129_2_JOB.A_CV ,THISNODE. YT630_1129_2_BRAND.A_CV\nTHISNODE.YT630_1129_3A_JOB.A_CV ,THISNODE. YT630_1129_3A_BRAND.A_CV\nTHISNODE.YT630_1129_3_JOB.A_CV ,THISNODE. YT630_1129_3_BRAND.A_CV\nTHISNODE.YT630_1129_4A_JOB.A_CV ,THISNODE. YT630_1129_4A_BRAND.A_CV\nTHISNODE.YT630_1129_4_JOB.A_CV ,THISNODE. YT630_1129_4_BRAND.A_CV\nTHISNODE.YT630_1129_5A_JOB.A_CV ,THISNODE. YT630_1129_5A_BRAND.A_CV\nTHISNODE.YT630_1129_5_JOB.A_CV ,THISNODE. YT630_1129_5_BRAND.A_CV\nTHISNODE.YT630_1129_6A_JOB.A_CV ,THISNODE. YT630_1129_6A_BRAND.A_CV\nTHISNODE.YT630_1129_6_JOB.A_CV ,THISNODE. YT630_1129_6_BRAND.A_CV\nTHISNODE.YT630_1129_7A_JOB.A_CV ,THISNODE. YT630_1129_7A_BRAND.A_CV"]
[null,null,"设备组合启动",null,"无","L9KYPJL_ZHStart_Start","L9KYPJL_ZHStart_Start",{"$nulls":3},"get",{"$nulls":3},"THISNODE.YT602_TASK2_START.F_CV = 1\n thisnode.YT630_IN_TASK1_START.F_CV =1\nthisnode.YT630_IN_TASK1_STop.F_CV = 0\nTHISNODE.K3_Z6L1_1Start_FK.F_CV = 1"]
[null,"生产提升","生产提升",null,"无","L9KYPJL_TS_TSStart","L9KYPJL_TS_TSStart",{"$nulls":3},"get",{"$nulls":3},"THISNODE.YT602_WP1115_PROTS.F_CV= 1"]
[null,null,"强制提升",null,"无","L9KYPJL_TS_TSForceStart","L9KYPJL_TS_TSForceStart",{"$nulls":3},"get",{"$nulls":3},"THISNODE.YT602_WP1115_ENTS.F_CV= 1"]
[null,null,"强制停止提升",null,"无","L9KYPJL_TS_TSForceStop","L9KYPJL_TS_TSForceStop",{"$nulls":3},"get",{"$nulls":3},"THISNODE.YT602_WP1115_ENSTOP.F_CV= 1"]
[null,null,"底带点动",null,null,"L9KYPJL_ZHStop_DDJog","L9KYPJL_ZHStop_DDJog",{"$nulls":3},"get",{"$nulls":3},"THISNODE.YT602_WP1115_DDSTART.F_CV= 1"]
[null,"组合停止","批结束",null,"无","L9KYPJL_ZHStop_BatchEnd","L9KYPJL_ZHStop_BatchEnd",{"$nulls":3},"get",{"$nulls":3},"THISNODE.YT602InGPBatchStart.F_CV = 0\nTHISNODE.YT602INGPBATCHEND.F_CV = 1"]
[{"$nulls":3},"回料到料房-料筒1","无","L9KYPJL_ZHStopRec_Tank1_InMRoom","L9KYPJL_ZHStopRec_Tank1_InMRoom",{"$nulls":3},"get",{"$nulls":3},"THISNODE.K3_Z6KA1BackStuff_FK.F_CV = 1"]
[{"$nulls":3},"回料到料房-料筒2","无","L9KYPJL_ZHStopRec_Tank2_InMRoom","L9KYPJL_ZHStopRec_Tank2_InMRoom",{"$nulls":3},"get",{"$nulls":3},"THISNODE.K3_Z6KA2BackStuff_FK.F_CV = 1"]
[{"$nulls":3},"ST1 清洁",null,"L9KYPJL_ZHStopRec_ST1_Clear","L9KYPJL_ZHStopRec_ST1_Clear",{"$nulls":3},"get",{"$nulls":3},"THISNODE.K3_Z6ST1_StartClean_FK.F_CV = 1"]
[{"$nulls":3},"ST1 清洁停止",null,"L9KYPJL_ZHStopRec_ST1_StopClear","L9KYPJL_ZHStopRec_ST1_StopClear",{"$nulls":3},"get",{"$nulls":3},"THISNODE.K3_Z6ST1_StopClean_FK.F_CV = 1"]
[{"$nulls":3},"KA 泵预加料",null,"L9KYPJL_ZHStop_Pump_Start","L9KYPJL_ZHStop_Pump_Start",{"$nulls":3},"get",{"$nulls":3},"THISNODE.K3_Z6KA1_PumpStartPreFill_FK.F_CV = 1"]
[{"$nulls":3},"KA 泵预加料停止",null,"L9KYPJL_ZHStop_Pump_Stop","L9KYPJL_ZHStop_Pump_Stop",{"$nulls":3},"get",{"$nulls":3},"THISNODE.K3_Z6KA1_PumpStopPreFill_FK.F_CV = 1"]
[{"$nulls":3},"KA 泵回送料",null,"L9KYPJL_ZHStop_Pipe_InTank","L9KYPJL_ZHStop_Pipe_InTank",{"$nulls":3},"get",{"$nulls":3}," THISNODE.K3_Z6KA1_PumpStartFeedBack_FK.F_CV = 1"]
[{"$nulls":3},"KA 泵回送料停止",null,"L9KYPJL_ZHStop_StopPipe_InTank","L9KYPJL_ZHStop_StopPipe_InTank",{"$nulls":3},"get",{"$nulls":3},"THISNODE.K3_Z6KA1_PumpStopFeedBack_FK.F_CV = 1"]
[{"$nulls":3},"泵清洁管路和喷嘴",null,"L9KYPJL_ZHStop_Pipe_Clear","L9KYPJL_ZHStop_Pipe_Clear",{"$nulls":3},"get",{"$nulls":3},"THISNODE.K3_Z6KA1_PumpStartCP_N_FK.F_CV = 1"]
[{"$nulls":3},"泵清洁管路和喷嘴停止",null,"L9KYPJL_ZHStop_StopPipe_Clear","L9KYPJL_ZHStop_StopPipe_Clear",{"$nulls":3},"get",{"$nulls":3},"THISNODE.K1_Z7TT1StopCoolDown_FK.F_CV = 1"]
[{"$nulls":3},"泵清洁管路",null,"L9KYPJL_ZHStop_Nozzle_Clear","L9KYPJL_ZHStop_Nozzle_Clear",{"$nulls":3},"get",{"$nulls":3}," THISNODE.K3_Z6KA1_PumpStartCleaningP_FK.F_CV = 1"]
[{"$nulls":3},"泵清洁管路停止",null,"L9KYPJL_ZHStop_StopNozzle_Clear","L9KYPJL_ZHStop_StopNozzle_Clear",{"$nulls":3},"get",{"$nulls":3}," THISNODE.K3_Z6KA1_PumpStopCleaningP_FK.F_CV = 1"]
[{"$nulls":3},"KA1清洁料罐",null,"L9KYPJL_ZHStop_Tank1_WashStart","L9KYPJL_ZHStop_Tank1_WashStart",{"$nulls":3},"get",{"$nulls":3}," THISNODE.K3_Z6KA1_StartCleaningTank_FK.F_CV = 1"]
[{"$nulls":3},"KA1清洁料罐停止",null,"L9KYPJL_ZHStop_Tank1_WashStop","L9KYPJL_ZHStop_Tank1_WashStop",{"$nulls":3},"get",{"$nulls":3},"THISNODE.K3_Z6KA1_StopCleaningTank_FK.F_CV = 1"]
[{"$nulls":3},"KA2清洁料罐",null,"L9KYPJL_ZHStop_Tank2_WashStart","L9KYPJL_ZHStop_Tank2_WashStart",{"$nulls":3},"get",{"$nulls":3},"  THISNODE.K3_Z6KA2_StartCleaningTank_FK.F_CV = 1"]
[{"$nulls":3},"KA2清洁料罐停止",null,"L9KYPJL_ZHStop_Tank2_WashStop","L9KYPJL_ZHStop_Tank2_WashStop",{"$nulls":3},"get",{"$nulls":3},"THISNODE.K3_Z6KA2_StopCleaningTank_FK.F_CV = 1"]
[{"$nulls":3},"KA1 手动加热",null,"L9KYPJL_ZHStop_Tank1_SDHeadStart","L9KYPJL_ZHStop_Tank1_SDHeadStart",{"$nulls":3},"get",{"$nulls":3},"THISNODE.K3_Z6KA1ManualHeat_FK.F_CV = 1"]
[{"$nulls":3},"KA2 手动加热",null,"L9KYPJL_ZHStop_Tank2_SDHeadStop","L9KYPJL_ZHStop_Tank2_SDHeadStop",{"$nulls":3},"get",{"$nulls":3},"THISNODE.K3_Z6KA2ManualHeat_FK.F_CV = 1"]
[null,null,"信息清零","任务结束","无","L9KYPJL_ZHStopInfoClear_TaskStop_Stop","L9KYPJL_ZHStopInfoClear_TaskStop_Stop",{"$nulls":3},"get",{"$nulls":3},"THISNODE.YT602_TASK2_END.F_CV= 1\n\n"]
[{"$nulls":3},"进页柜任务结束",null,"L9KYPJL_ZHStopInfoClear_InYGTask_End","L9KYPJL_ZHStopInfoClear_InYGTask_End",{"$nulls":3},"get",null,null,"THISNODE.JK_YT602_IN_TASK2_FINISH_OK.F_CV=1 ","  THISNODE.JK_YT602_IN_TASK2_FINISH.F_CV =1","thisnode.YT630_IN_TASK1_A03.F_CV=0\nthisnode.YT630_IN_TASK1_A01.F_CV=0\nthisnode.YT630_IN_TASK1_A02.F_CV=0\nthisnode.YT630_IN_TASK1_A04.F_CV=0\nthisnode.YT630_IN_TASK1_A05.F_CV=0\nthisnode.YT630_IN_TASK1_A06.F_CV=0\nthisnode.YT630_IN_TASK1_A07.F_CV=0\nthisnode.YT630_IN_TASK1_A08.F_CV=0\nthisnode.YT630_IN_TASK1_A09.F_CV=0\nthisnode.YT630_IN_TASK1_A10.F_CV=0\nthisnode.YT630_IN_TASK1_A11.F_CV=0\nthisnode.YT630_IN_TASK1_A12.F_CV=0\nthisnode.YT630_IN_TASK1_A13.F_CV=0\nthisnode.YT630_IN_TASK1_A14.F_CV=0\nthisnode.YT630_IN_TASK1_A15.F_CV=0\nthisnode.YT630_IN_TASK1_A16.F_CV=0\nthisnode.YT630_IN_TASK1_R01.F_CV=0\nthisnode.YT630_IN_TASK1_R02.F_CV=0\nthisnode.YT630_IN_TASK1_R03.F_CV=0\nthisnode.YT630_IN_TASK1_R09.F_CV=0\nthisnode.YT630_IN_TASK1_R10.F_CV=0","\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK1_A03.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK1_A01.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK1_A02.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK1_A04.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK1_A05.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK1_A06.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK1_A07.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK1_A08.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK1_A09.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK1_A10.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK1_A11.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK1_A12.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK1_A13.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK1_A14.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK1_A15.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK1_A16.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK1_R01.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK1_R02.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK1_R03.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK1_R09.F_CV\"\nwritevalue \"0\", \"Fix32.thisnode.YT630_IN_TASK1_R10.F_CV\""]
[{"$nulls":3},"批次清零","无","L9KYPJL_ZHStopInfoClear_InfoClear_PathClear","L9KYPJL_ZHStopInfoClear_InfoClear_PathClear",{"$nulls":3},"get",{"$nulls":3},"THISNODE.K3_Z6_CK1116_ACCU_CLEAR.F_CV =1\nTHISNODE.K3_Z6L1_1RESTOTAL_FK.F_CV =1"]
[{"$nulls":3},"生产清零","无","L9KYPJL_ZHStopInfoClear_OutYPG_InfoClear","L9KYPJL_ZHStopInfoClear_OutYPG_InfoClear",{"$nulls":3},"get",null,null,"THISNODE.JK_YT602_LEAFBSC_CLEAR_OK.F_CV=1 ","THISNODE.JK_YT602_LEAFBSC_CLEAR.F_CV =1"]
[{"$nulls":3},"出预配柜柜号清零",null,"L9KYPJL_ZHStopInfoClear_OutYG_Clear","L9KYPJL_ZHStopInfoClear_OutYG_Clear"]
[{"$nulls":3},"出预配柜信息清零","柜号(多个柜以逗号分割)、批次号、牌号","L9KYPHC_ZHQD_YPGSelno1_InfoSet(string GPNum,string BatchNum,string BrandNum) JSON方式\n","L9KYPHC_ZHQD_YPGSelno1_InfoSet",null,"选多写",{"$nulls":4},"\n\n\n\n"]
[{"$nulls":5},"L9KYPHC_ZHQD_YPGSelno2_InfoSet(string GPNum,string BatchNum,string BrandNum) JSON方式\n","L9KYPHC_ZHQD_YPGSelno2_InfoSet",null,"选多写","R06,R07,R08"]
[{"$nulls":5},"L9KYPHC_ZHQD_YPGSelno3_InfoSet(string GPNum,string BatchNum,string BrandNum) JSON方式\n","L9KYPHC_ZHQD_YPGSelno3_InfoSet",null,"选多写","R06,R07,R08"]
[{"$nulls":3},"进叶柜柜号清零","无","L9KYPJL_ZHStopInfoClear_InYG_InfoClear","L9KYPJL_ZHStopInfoClear_InYG_InfoClear"]
[null,null,"设备组合停止",null,"无","L9KYPJL_ZHStop_Stop","L9KYPJL_ZHStop_Stop",{"$nulls":3},"get",{"$nulls":3},"THISNODE.YT602_TASK2_STOP.F_CV = 1\nthisnode.YT630_IN_TASK1_STop.F_CV  =1\nthisnode.YT630_IN_TASK1_START.F_CV =0\nTHISNODE.K3_Z6L1_1ProdPaus_FK.F_CV = 1"]
[null,"辅助操作","单机/联机",null,"段号"]
[null,null,"故障复位",null,"无","L3KYPYG_FK_AlarmReset","L3KYPYG_FK_AlarmReset",{"$nulls":3},"get",{"$nulls":3},"THISNODE.YT602_RESET.F_CV = 1\nTHISNODE.YT6024_CONTROL_RESET.F_CV = 1\n thisnode.YT630_CONTROL_YT630_RESET.F_CV=1\nTHISNODE.K2_Z5Grp1AcknA_FK.F_CV = 1\n  THISNODE.K3_Z6L1_AcknA_FK.F_CV = 1"]

{"sheet":"3000进叶柜加料","index":2,"n_rows":25,"n_cols":22,"rows_kept":25,"merged":[[1,0,24,0],[1,1,11,1],[12,1,22,1],[13,2,21,2],[19,3,21,3],[23,1,24,1]],"flags":["formulas_cached_only"]}
["工序","操作按钮","组件封装","业务说明","参数说明","API接口名","API接口名1","是否验证","生成类型","选写多值","测试方法","API传入参数","API测试结果","检查点位","写入点位","触发脚本","备注","API状态","IFIX点位","代码生成","配置文件","代码标记"]
["3000配叶柜\n进叶柜","组合启动","工单信息下发",null,"工单号、批次号、牌号","L3KYPYG_ZHStart_GDInfoSet(json) 示例：string GDNum,string BatchNum,string BrandNum","L3KYPYG_ZHStart_GDInfoSet",null,"多写2",null,"Post",{"$nulls":3},"THISNODE.YT6023C_EntryID.A_CV\nTHISNODE.YT6023C_BatchNo.A_CV\nTHISNODE.YT6023C_Brand.A_CV"]
[null,null,"启用生产关联",null,"无","L3KYPYG_ZHStart_DevLinkEnable","L3KYPYG_ZHStart_DevLinkEnable",{"$nulls":3},"Get",{"$nulls":3},"THISNODE.YT630_IN_TASK3_LINK.F_CV=1"]
[null,null,"取消生产关联",null,"无","L3KYPYG_ZHStart_DevLinkDisable","L3KYPYG_ZHStart_DevLinkDisable",{"$nulls":3},"Get",{"$nulls":3},"THISNODE.YT630_IN_TASK3_LINK.F_CV=0"]
[null,null,"任务开始",null,"无","L3KYPYG_ZHStart_TaskStart","L3KYPYG_ZHStart_TaskStart",{"$nulls":3},"Get",{"$nulls":3},"thisnode.YT630_IN_TASK3_START.F_CV=1\nthisnode.YT630_IN_TASK3_STop.F_CV=0"]
[null,null,"批开始",null,"无","L3KYPYG_ZHStart_BatchStart","L3KYPYG_ZHStart_BatchStart",{"$nulls":3},"Get",{"$nulls":3},"THISNODE.YT6023_TASK3_bSTART.F_CV=1\nTHISNODE.YT6023_TASK3_bSTOP.F_CV=0"]
[null,null,"出配叶柜验证",null,"柜号","L3KYPYG_ZHStart_OutPYGCheck(string GPno)","L3KYPYG_ZHStart_OutPYGCheck",null,"选单写","YP01,YP02","Post","YP01/YP02",null,"THISNODE.JK_YT6023_TASK3_OUT_01_OK.F_CV=1\nTHISNODE.JK_YT6023_TASK3_OUT_02_OK.F_CV=1","THISNODE.JK_YT6023_TASK3_OUT_01.F_CV=1\nTHISNODE.JK_YT6023_TASK3_OUT_02.F_CV=1",null,"If READvalue(\"Fix32.THISNODE.YT6023_TASK2_NODE_IN_01.F_CV\", 1) = 1 Then\n   MsgBox \"切片任务中此柜被选做进柜，不能同时进柜，请确认后操作！\", vbOKOnly + vbCritical, \"单元选择冲突\"\n   Exit Sub\nEnd If\nIf READvalue(\"Fix32.THISNODE.YT6023_TASK2_NODE_FIRST_01.F_CV\", 1) = 1 Then\n   MsgBox \"切片任务中此柜被选做进柜，不能同时进柜，请确认后操作！\", vbOKOnly + vbCritical, \"单元选择冲突\"\n   Exit Sub\nEnd If\nIf READvalue(\"Fix32.THISNODE.YT6023_TASK2_NODE_SECOND_01.F_CV\", 1) = 1 Then\n   MsgBox \"切片任务中此柜被选做进柜，不能同时进柜，请确认后操作！\", vbOKOnly + vbCritical, \"单元选择冲突\"\n   Exit Sub\nEnd If\nIf READvalue(\"Fix32.THISNODE.YT6023_TASK2_NODE_THIRD_01.F_CV\", 1) = 1 Then\n   MsgBox \"切片任务中此柜被选做进柜，不能同时进柜，请确认后操作！\", vbOKOnly + vbCritical, \"单元选择冲突\"\n   Exit Sub\nEnd If\n\nwritevalue 1, \"Fix32.THISNODE.YT6023_TASK3_NODE_OUT_01.F_CV\", 1\nIf User.YT6023_TASK3_LINK.CurrentValue = True Then\n   writevalue 1, \"Fix32.THISNODE.YT6023_TASK3_R15.F_CV\", 1\nEnd If"]
[null,null,"出配叶柜取消",null,"柜号","L3KYPYG_ZHStart_OutPYGCancel(string GPno)","L3KYPYG_ZHStart_OutPYGCancel",null,"选单写","YP01,YP02","Post","YP01/YP02",null,"THISNODE.JK_YT6023_TASK3_OUT1_CLEAR_OK.F_CV=1\nTHISNODE.JK_YT6023_TASK3_OUT2_CLEAR_OK.F_CV=1","THISNODE.JK_YT6023_TASK3_OUT1_CLEAR.F_CV=1\nTHISNODE.JK_YT6023_TASK3_OUT2_CLEAR.F_CV=1"]
[null,null,"进叶柜条件验证及路径下发",null,"柜号","L3KYPYG_ZHStart_InYPGPathSet(string GPno)","L3KYPYG_ZHStart_InYPGPathSet",null,"选单写","YG18,YG20,YG22,YG24,YG17,YG19,YG21,YG23","Post",null,null,"THISNODE.JK_YT630_IN_TASK3_A17_OK.F_CV=1\nTHISNODE.JK_YT630_IN_TASK3_A18_OK.F_CV = 1\nTHISNODE.JK_YT630_IN_TASK3_A19_OK.F_CV = 1\nTHISNODE.JK_YT630_IN_TASK3_A20_OK.F_CV = 1\nTHISNODE.JK_YT630_IN_TASK3_A21_OK.F_CV = 1\nTHISNODE.JK_YT630_IN_TASK3_A22_OK.F_CV = 1\nTHISNODE.JK_YT630_IN_TASK3_A23_OK.F_CV = 1\nTHISNODE.JK_YT630_IN_TASK3_A24_OK.F_CV = 1","THISNODE.JK_YT630_IN_TASK3_A17.F_CV = 1\nTHISNODE.JK_YT630_IN_TASK3_A18.F_CV = 1\nTHISNODE.JK_YT630_IN_TASK3_A19.F_CV = 1\nTHISNODE.JK_YT630_IN_TASK3_A20.F_CV = 1\nTHISNODE.JK_YT630_IN_TASK3_A21.F_CV = 1 \nTHISNODE.JK_YT630_IN_TASK3_A22.F_CV = 1\nTHISNODE.JK_YT630_IN_TASK3_A23.F_CV = 1\nTHISNODE.JK_YT630_IN_TASK3_A24.F_CV = 1",null,"writevalue \"1\", \"Fix32.THISNODE.YT630_IN_task3_A17.F_CV\"\n\nwritevalue \"0\", \"Fix32.THISNODE.YT630_IN_task3_A18.F_CV\"\nwritevalue \"0\", \"Fix32.THISNODE.YT630_IN_task3_A19.F_CV\"\nwritevalue \"0\", \"Fix32.THISNODE.YT630_IN_task3_A20.F_CV\"\nwritevalue \"0\", \"Fix32.THISNODE.YT630_IN_task3_A21.F_CV\"\nwritevalue \"0\", \"Fix32.THISNODE.YT630_IN_task3_A22.F_CV\"\nwritevalue \"0\", \"Fix32.THISNODE.YT630_IN_task3_A23.F_CV\"\nwritevalue \"0\", \"Fix32.THISNODE.YT630_IN_task3_A24.F_CV\""]
[null,null,"进叶柜路径取消",null,"柜号","L3KYPYG_ZHStart_InYPGPathCancel(string GPno)","L3KYPYG_ZHStart_InYPGPathCancel",null,"选单写","YG18,YG20,YG22,YG24,YG17,YG19,YG21,YG23","Post",{"$nulls":3},"THISNODE.YT630_IN_TASK3_A17.F_CV = 0\nTHISNODE.YT630_IN_TASK3_A18.F_CV = 0\nTHISNODE.YT630_IN_TASK3_A19.F_CV = 0\nTHISNODE.YT630_IN_TASK3_A20.F_CV = 0\nTHISNODE.YT630_IN_TASK3_A21.F_CV = 0\nTHISNODE.YT630_IN_TASK3_A22.F_CV = 0\nTHISNODE.YT630_IN_TASK3_A23.F_CV = 0\nTHISNODE.YT630_IN_TASK3_A24.F_CV = 0"]
[null,null,"进叶柜信息下发",null,"柜号、批次号、牌号","L3KYPYG_ZHStart_InYPGInfoSet(string GPno)","L3KYPYG_ZHStart_InYPGInfoSet",null,"选多写","YG18,YG20,YG22,YG24,YG17,YG19,YG21,YG23","Post",{"$nulls":3},"THISNODE.YT630_1153_JOB.A_CV,THISNODE.YT630_1153_BRAND.A_CV\nTHISNODE.YT630_1153_1_JOB.A_CV,THISNODE.YT630_1153_1_BRAND.A_CV\nTHISNODE.YT630_1153_2_JOB.A_CV,THISNODE.YT630_1153_2_BRAND.A_CV\nTHISNODE.YT630_1153_3_JOB.A_CV,THISNODE.YT630_1153_3_BRAND.A_CV\nTHISNODE.YT630_1153A_JOB.A_CV,THISNODE.YT630_1153A_BRAND.A_CV\nTHISNODE.YT630_1153_1A_JOB.A_CV,THISNODE.YT630_1153_1A_BRAND.A_CV\nTHISNODE.YT630_1153_2A_JOB.A_CV,THISNODE.YT630_1153_2A_BRAND.A_CV\nTHISNODE.YT630_1153_3A_JOB.A_CV,THISNODE.YT630_1153_3A_BRAND.A_CV"]
[null,null,"设备组合启动",null,"无","L3KYPYG_ZHStart_Start","L3KYPYG_ZHStart_Start",{"$nulls":3},"Get",null,null,"THISNODE.JK_YT6023_TASK3_START_OK.F_CV=1","THISNODE.JK_YT6023_TASK3_START.F_CV=1","THISNODE.YT6023_TASK3_START.F_CV = 1\n THISNODE.YT630_IN_TASK3_START.F_CV =1\nFix32.THISNODE.YT630_IN_TASK3_STop.F_CV =0"]
[null,"组合停止","批结束",null,"无","L3KYPYG_ZHStop_BatchEnd","L3KYPYG_ZHStop_BatchEnd",{"$nulls":3},"Get",{"$nulls":3},"THISNODE.YT6023_TASK3_bSTOP.F_CV=1\nTHISNODE.YT6023_TASK3_bSTART.F_CV=0\n="]
[null,null,"信息清零","任务停止","无","L3KYPYG_ZHStopInfoClear_TaskStop","L3KYPYG_ZHStopInfoClear_TaskStop",{"$nulls":3},"Get",{"$nulls":3},"thisnode.YT630_IN_TASK3_STop.F_CV=1\nthisnode.YT630_IN_TASK3_START.F_CV=0"]
[{"$nulls":3},"任务结束","无","L3KYPYG_ZHStopInfoClear_TaskEnd","L3KYPYG_ZHStopInfoClear_TaskEnd",{"$nulls":3},"Get",{"$nulls":3},"thisnode.YT630_IN_TASK3_A17.F_CV=0\nthisnode.YT630_IN_TASK3_A18.F_CV=0\nthisnode.YT630_IN_TASK3_A19.F_CV=0\nthisnode.YT630_IN_TASK3_A20.F_CV=0\nthisnode.YT630_IN_TASK3_A21.F_CV=0\nthisnode.YT630_IN_TASK3_A22.F_CV=0\nthisnode.YT630_IN_TASK3_A23.F_CV=0\nthisnode.YT630_IN_TASK3_A24.F_CV=0\nthisnode.YT630_IN_TASK3_R12.F_CV=0\nthisnode.YT630_IN_TASK3_R13.F_CV=0\nthisnode.YT630_IN_TASK3_R14.F_CV=0\nthisnode.YT630_IN_TASK3_R15.F_CV=0\nTHISNODE.YT6023_TASK3_NODE_OUT.F_CV=0\nTHISNODE.YT6023_TASK3_ROUTE.F_CV=0"]
[{"$nulls":3},"批次清零","无","L3KYPYG_ZHStopInfoClear_BatchClear","L3KYPYG_ZHStopInfoClear_BatchClear",{"$nulls":3},"Get",{"$nulls":3},"THISNODE.YT630_3000_OUT_BATCH_STOP.F_CV=1"]
[{"$nulls":3},"生产清零","无","L3KYPYG_ZHStopInfoClear_ProdClear","L3KYPYG_ZHStopInfoClear_ProdClear",{"$nulls":3},"Get",null,null,"THISNODE.JK_YT6023_LAMINASC_CLEAR_OK.F_CV=1","THISNODE.JK_YT6023_LAMINASC_CLEAR.F_CV=1",null,"writevalue 0, \"\"Fix32.THISNODE.YT6023C_BATCHSEQ.F_CV\"\", 1  '批次顺序\nwritevalue 0, \"\"Fix32.THISNODE.YT6023C_INGP1AMOUNT.F_CV\"\", 1  '入1柜料量\nwritevalue 0, \"\"Fix32.THISNODE.YT6023C_INGP2AMOUNT.F_CV\"\", 1  '入2柜料量\nwritevalue 0, \"\"Fix32.THISNODE.YT6023C_INGP3AMOUNT.F_CV\"\", 1  '入3柜料量\nwritevalue 0, \"\"Fix32.THISNODE.YT6023C_INGPQTY.F_CV\"\", 1  '生成物料入的柜子数量\n\nWriteValue \"\"\"\", \"\"FIX32.THISNODE.YT6023C_BATCHNO.A_CV\"\", 2 '/3k线配叶出柜段当前批次号\n\nWriteValue \"\"\"\", \"\"FIX32.THISNODE.YT6023C_BRAND.A_CV\"\", 2 ' /3k线配叶出柜段当前牌号\nWriteValue \"\"\"\", \"\"FIX32.THISNODE.YT6023C_ENTRYID.A_CV\"\", 2 '/EntryID\nWriteValue \"\"\"\", \"\"FIX32.THISNODE.YT6023C_INGP1.A_CV\"\", 2' /预计入柜号1\nWriteValue \"\"\"\", \"\"FIX32.THISNODE.YT6023C_INGP2.A_CV\"\", 2'/预计入柜号2\nWriteValue \"\"\"\", \"\"FIX32.THISNODE.YT6023C_INGP3.A_CV\"\", 2'/预计入柜号3\nWriteValue \"\"\"\", \"\"FIX32.THISNODE.YT6023C_JHJSSJ.A_CV\"\", 2'/3k线配叶出柜段计划结束时间\nWriteValue \"\"\"\", \"\"FIX32.THISNODE.YT6023C_JHKSSJ.A_CV\"\", 2'/3k线配叶出柜段计划开始时间\nWriteValue \"\"\"\", \"\"FIX32.THISNODE.YT6023C_OUTGP.A_CV\"\", 2'/3k线配叶出柜段出柜号\nWriteValue \"\"0\"\", \"\"FIX32.THISNODE.YT6023C_PRODMIX.F_CV\"\", 2'/产出物是否汇集\nWriteValue \"\"0\"\", \"\"FIX32.THISNODE.YT6023C_ROAD.F_CV\"\", 2'/生产工艺路线\nWriteValue \"\"\"\", \"\"FIX32.THISNODEY.YT6023C_STUFFBRAND.A_CV\"\", 2'/3k线配叶出柜段当前料液牌号\nWriteValue \"\"0\"\", \"\"FIX32.THISNODE.YT6023C_WEIGHT.F_CV\"\", 2'/3k线配叶出柜段当前重量\n"]
[{"$nulls":3},"出配叶柜路径清零","无","L3KYPYG_ZHStopInfoClear_OutPYGPathClear","L3KYPYG_ZHStopInfoClear_OutPYGPathClear"]
[{"$nulls":3},"进叶柜柜号清零","无","L3KYPYG_ZHStopInfoClear_InYPGInfoClear","L3KYPYG_ZHStopInfoClear_InYPGInfoClear"]
[{"$nulls":3},"配叶柜信息清零","第1选柜(单柜号、批次号、牌号)\n","L3KYPYG_ZHQD_YPGno1INFOSET(string GDNum,string BatchNum,string BrandNum) JSON方式\nL3KYPYG_ZHQD_YPGno2INFOSET\nL3KYPYG_ZHQD_YPGno3INFOSET","L3KYPYG_ZHQD_YPGno1INFOSET(string GDNum,string BatchNum,string BrandNum) JSON方式\nL3KYPYG_ZHQD_YPGno2INFOSET\nL3KYPYG_ZHQD_YPGno3INFOSET"]
[{"$nulls":4},"第2选柜(单柜号、批次号、牌号)","L3KYPHC_ZHQD_YPGno2INFOSET(string GDNumNum,string BatchNum,string BrandNum) JSON方式","L3KYPHC_ZHQD_YPGno2INFOSET(string GDNumNum,string BatchNum,string BrandNum) JSON方式"]
[{"$nulls":4},"第3选柜(单柜号、批次号、牌号)","L3KYPHC_ZHQD_YPGno3INFOSET(string GDNum,string BatchNum,string BrandNum) JSON方式","L3KYPHC_ZHQD_YPGno3INFOSET(string GDNum,string BatchNum,string BrandNum) JSON方式"]
[null,null,"设备组合停止",null,"无","L3KYPYG_ZHStop_DevZHStop","L3KYPYG_ZHStop_DevZHStop",{"$nulls":3},"Get",{"$nulls":3},"THISNODE.YT6023_TASK3_STOP.F_CV=1\nTHISNODE.YT630_IN_TASK3_STop.F_CV=1\nTHISNODE.YT630_IN_TASK3_START.F_CV=0"]
[null,"辅助操作","单机/联机",null,"段号"]
[null,null,"故障复位",null,"无","L3KYPYG_FK_AlarmReset","L3KYPYG_FK_AlarmReset",{"$nulls":3},"Get",{"$nulls":3},"thisnode.YT630_CONTROL_YT630_RESET.F_CV=1"]

{"sheet":"真空回潮","index":3,"n_rows":92,"n_cols":13,"rows_kept":92,"merged":[[1,0,49,0],[1,1,16,1],[2,2,5,2],[8,2,12,2],[14,2,17,2],[18,1,23,1],[24,1,37,1],[38,1,47,1],[39,2,42,2],[43,2,47,2],[48,1,49,1]],"flags":["formulas_cached_only"]}
["工序","操作按钮","组件封装","业务说明","参数说明","API接口名",null,"测试状态","备注","API状态"]
["5K真空回潮","生产启动","工单信息下发",null,"工单号、批次号、牌号","L5KYPZK_Start_GDinfoSet(object obj) string GDH,string PCH,string PH","YT618A_BATCHNO（批次）\n/YT618A_ENTRYID(工单)\n/YT618A_BRAND(牌号)",{"$nulls":3},"YT618A_BATCHNO（批次）\n/YT618A_ENTRYID(工单)\n/YT618A_BRAND(牌号)"]
[null,null,"生产路径选择","3K回潮路径选择",null,"L5KYPZK_Start_PathSel3K(object obj)  string DevName=3K,bool BSel","       Fix32.THISNODE.YT618_WL3000_SELECT.F_CV = 1\n       Fix32.THISNODE.YT618_WL5000_SELECT.F_CV = 0",{"$nulls":3},"YT618_WL3000_SELECT",null,"\n    If (MsgBox(\"是否需要选择真空回潮3000线供料\", vbOKCancel, \"选择3000线供料\") = vbOK) Then\n       Fix32.THISNODE.YT618_WL3000_SELECT.F_CV = 1\n       Fix32.THISNODE.YT618_WL5000_SELECT.F_CV = 0\n       Call Modlogin.Oplog((1), (0), (1), \"YT618选择真空回潮3000线供料\")\n    End If\n Else\n   If (MsgBox(\"是否需要取消选择真空回潮3000线供料\", vbOKCancel, \"选择3000线供料\") = vbOK) Then\n      Fix32.THISNODE.YT618_WL3000_SELECT.F_CV = 0\n      Fix32.THISNODE.YT618_WL5000_SELECT.F_CV = 1\n      Call Modlogin.Oplog((1), (0), (1), \"YT618取消选择真空回潮3000线供料\")\n   End If\n End If"]
[{"$nulls":3},"3K回潮路径选择取消",null,null,"      Fix32.THISNODE.YT618_WL3000_SELECT.F_CV = 0\n      Fix32.THISNODE.YT618_WL5000_SELECT.F_CV = 1"]
[{"$nulls":3},"5K回潮路径选择",null,"L5KYPZK_Start_PathSel5K(object obj)  string DevName=5K,bool BSel","       Fix32.THISNODE.YT618_WL5000_SELECT.F_CV = 1\n       Fix32.THISNODE.YT618_WL3000_SELECT.F_CV = 0",{"$nulls":3},"YT618_WL5000_SELECT"]
[{"$nulls":3},"5K回潮路径选择取消",null,null,"      Fix32.THISNODE.YT618_WL5000_SELECT.F_CV = 0\n      Fix32.THISNODE.YT618_WL3000_SELECT.F_CV = 1"]
[]
[null,null,"批开始",null,null,"L5KYPZK_Start_BatchStart","     Fix32.thisnode.YT618_TASK1_BSTART.F_CV = 1\n     Fix32.thisnode.YT618_TASK1_BSTOP.F_CV = 0",{"$nulls":3},"YT618_TASK1_BSTART"]
[null,null,"设备打自动","设备1组打自动",null,"L5KYPZK_Start_SetAutoDev1","     Fix32.THISNODE.YT618_TASK1_MANUAL.F_CV = 0\n     Fix32.THISNODE.YT618_TASK1_LOCK.F_CV = 0\n     Fix32.THISNODE.YT618_TASK1_AUTO.F_CV = 1",{"$nulls":3},"YT618_TASK1_AUTO"]
[{"$nulls":3},"设备1组打单机",null,"L5KYPZK_Start_SetManualDev1","     Fix32.THISNODE.YT618_TASK1_MANUAL.F_CV = 1\n     Fix32.THISNODE.YT618_TASK1_LOCK.F_CV = 0\n     Fix32.THISNODE.YT618_TASK1_AUTO.F_CV = 0"]
[{"$nulls":3},"设备1组闭锁",null,"L5KYPZK_Start_LockDev1","     Fix32.THISNODE.YT618_TASK1_MANUAL.F_CV = 0\n     Fix32.THISNODE.YT618_TASK1_LOCK.F_CV = 1\n     Fix32.THISNODE.YT618_TASK1_AUTO.F_CV = 0"]
[{"$nulls":3},"设备2组打自动",null,"L5KYPZK_Start_SetAutoDev2","     Fix32.THISNODE.YT618_TASK2_MANUAL.F_CV = 0\n     Fix32.THISNODE.YT618_TASK2_LOCK.F_CV = 0\n     Fix32.THISNODE.YT618_TASK2_AUTO.F_CV = 1",{"$nulls":3},"YT618_TASK2_AUTO"]
[{"$nulls":3},"设备2组打单机",null,"L5KYPZK_Start_SetManualDev2","     Fix32.THISNODE.YT618_TASK2_MANUAL.F_CV = 1\n     Fix32.THISNODE.YT618_TASK2_LOCK.F_CV = 0\n     Fix32.THISNODE.YT618_TASK2_AUTO.F_CV = 0"]
[{"$nulls":3},"设备2组闭锁",null,"L5KYPZK_Start_LockDev2","     Fix32.THISNODE.YT618_TASK2_MANUAL.F_CV = 0\n     Fix32.THISNODE.YT618_TASK2_LOCK.F_CV = 1\n     Fix32.THISNODE.YT618_TASK2_AUTO.F_CV = 0"]
[null,null,"组合启动","设备1组合启动",null,"L5KYPZK_ZHStart_StartDev1","    Fix32.THISNODE.YT618_TASK1_START.F_CV = 1\n    Fix32.THISNODE.YT618_TASK1_STOP.F_CV = 0\n",{"$nulls":3},"YT618_TASK1_START"]
[{"$nulls":3},"设备1取消组合启动","取消","L5KYPZK_ZHStart_StopDev1"," Fix32.THISNODE.YT618_TASK1_START.F_CV = 0"]
[{"$nulls":3},"设备2组合启动",null,"L5KYPZK_ZHStart_StartDev2","Fix32.THISNODE.YT618_TASK2_START.F_CV = 1\nFix32.THISNODE.YT618_TASK2_STOP.F_CV = 0",{"$nulls":3},"YT618_TASK2_START"]
[{"$nulls":3},"设备2取消组合启动","取消","L5KYPZK_ZHStart_StopDev2","Fix32.THISNODE.YT618_TASK2_START.F_CV = 0"]
[null,"生产提升","3353生产提升",null,null,"L5KYPZK_TS_TSstart3353","Fix32.THISNODE.YT618_WP3353_CONSET1.F_CV = 1",{"$nulls":3},"YT618_WP3353_CONSET1"]
[null,null,"3353强制提升",null,null,"L5KYPZK_TS_TSforce3353","Fix32.THISNODE.YT618_WP3353_CONSET2.F_CV = 1",{"$nulls":3},"YT618_WP3353_CONSET2"]
[null,null,"3353强制停止",null,null,"L5KYPZK_TS_TSstop3353","Fix32.THISNODE.YT618_WP3353_CONSET3.F_CV = 1",{"$nulls":3},"YT618_WP3353_CONSET3"]
[null,null,"3360生产提升",null,null,"L5KYPZK_TS_TSstart3360","Fix32.THISNODE.YT618_WP3360_CONSET1.F_CV =1 ",{"$nulls":3},"YT618_WP3360_CONSET1"]
[null,null,"3360强制提升",null,null,"L5KYPZK_TS_TSforce3360","Fix32.THISNODE.YT618_WP3360_CONSET2.F_CV = 1",{"$nulls":3},"YT618_WP3360_CONSET2"]
[null,null,"3360强制停止",null,null,"L5KYPZK_TS_TSstop3360","Fix32.THISNODE.YT618_WP3360_CONSET3.F_CV = 1",{"$nulls":3},"YT618_WP3360_CONSET3"]
[null,"A/B锅切换","选择A锅备料",null,null,"L5KYPZK_BoilerA_Sel","Fix32.THISNODE.YT618_WZ1_SELECT.F_CV = 1",{"$nulls":3},"YT618_WZ1_SELECT"]
[null,null,"选择B锅备料",null,null,"L5KYPZK_BoilerB_Sel","Fix32.THISNODE.YT618_WZ2_SELECT.F_CV = 1",{"$nulls":3},"YT618_WZ2_SELECT"]
[null,null,"取消A锅选择备料",null,null,"L5KYPZK_BoilerA_SelCancel","Fix32.THISNODE.YT618_WZ1_SELECT.F_CV = 0",{"$nulls":3},"YT618_WZ1_SELECT"]
[null,null,"取消B锅选择备料",null,null,"L5KYPZK_BoilerB_SelCancel","Fix32.THISNODE.YT618_WZ2_SELECT.F_CV = 0",{"$nulls":3},"YT618_WZ2_SELECT"]
[null,null,"A锅自动",null,null,"L5KYPZK_BoilerA_Auto","    Fix32.THISNODE.YT618_M3315_MANUAL_SEL.F_CV = 0\n     Fix32.THISNODE.YT618_M3315_lock_SEL.F_CV = 0\n     Fix32.THISNODE.YT618_M3315_AUTO_SEL.F_CV = 1"]
[null,null,"A锅手动",null,null,"L5KYPZK_BoilerA_Manual","    Fix32.THISNODE.YT618_M3315_MANUAL_SEL.F_CV = 1\n     Fix32.THISNODE.YT618_M3315_lock_SEL.F_CV = 0\n     Fix32.THISNODE.YT618_M3315_AUTO_SEL.F_CV = 0"]
[null,null,"A锅闭锁",null,null,"L5KYPZK_BoilerA_Lock","    Fix32.THISNODE.YT618_M3315_MANUAL_SEL.F_CV = 0\n     Fix32.THISNODE.YT618_M3315_lock_SEL.F_CV = 1\n     Fix32.THISNODE.YT618_M3315_AUTO_SEL.F_CV = 0"]
[null,null,"B锅自动",null,null,"L5KYPZK_BoilerB_Auto","    Fix32.THISNODE.YT618_M3316_MANUAL_SEL.F_CV = 0\n     Fix32.THISNODE.YT618_M3316_lock_SEL.F_CV = 0\n     Fix32.THISNODE.YT618_M3316_AUTO_SEL.F_CV = 1"]
[null,null,"B锅手动",null,null,"L5KYPZK_BoilerB_Manual","   Fix32.THISNODE.YT618_M3316_MANUAL_SEL.F_CV = 1\n     Fix32.THISNODE.YT618_M3316_lock_SEL.F_CV = 0\n     Fix32.THISNODE.YT618_M3316_AUTO_SEL.F_CV = 0"]
[null,null,"B锅闭锁",null,null,"L5KYPZK_BoilerB_Lock","   Fix32.THISNODE.YT618_M3316_MANUAL_SEL.F_CV = 0\n     Fix32.THISNODE.YT618_M3316_lock_SEL.F_CV = 1\n     Fix32.THISNODE.YT618_M3316_AUTO_SEL.F_CV = 0"]
[null,null,"A锅前实际进锅数量设定",null,"进锅数","L5KYPZK_BoilerA_InCountSet(int InCount)","Fix32.THISNODE.YT618_WZ1_OUT_NUM.F_CV = ",{"$nulls":3},"YT618_UNIT_12_INFO"]
[null,null,"B锅前实际进锅数量设定",null,"进锅数","L5KYPZK_BoilerB_InCountSet(int InCount)","Fix32.THISNODE.YT618_WZ2_OUT_NUM.F_CV = ",{"$nulls":3},"YT618_UNIT_14_INFO"]
[null,null,"A锅前实际进箱数量设定",null,"进箱数","L5KYPZK_BoilerA_InBoxCountSet(int InCount)","Fix32.THISNODE.YT618_WZ1_INNUM_SET.F_CV = ",{"$nulls":3},"YT618_WZ1_INNUM_SET"]
[null,null,"B锅前实际进箱数量设定",null,"进箱数","L5KYPZK_BoilerB_InBoxCountSet(int InCount)","Fix32.THISNODE.YT618_WZ2_INNUM_SET.F_CV = ",{"$nulls":3},"YT618_WZ2_INNUM_SET"]
[null,"生产停止","批结束",null,null,"L5KYPZK_ZHStop_BatchEnd","     Fix32.thisnode.YT618_TASK1_BSTART.F_CV = 0\n     Fix32.thisnode.YT618_TASK1_BSTOP.F_CV = 1",{"$nulls":3},"YT618_TASK1_BSTOP"]
[null,null,"组合停止","设备1组合停止",null,"L5KYPZK_ZHStop_ZHTZ_Dev1Stop","Fix32.THISNODE.YT618_TASK1_STOP.F_CV = 1\n Fix32.THISNODE.YT618_TASK1_START.F_CV = 0",{"$nulls":3},"YT618_TASK1_STOP"]
[{"$nulls":3},"设备1取消组合停止","取消","L5KYPZK_ZHStop_ZHTZ_Dev1StopCancel","Fix32.THISNODE.YT618_TASK1_STOP.F_CV = 0"]
[{"$nulls":3},"设备2组合停止",null,"L5KYPZK_ZHStop_ZHTZ_Dev2Stop","Fix32.THISNODE.YT618_TASK2_STOP.F_CV = 1\nFix32.THISNODE.YT618_TASK2_START.F_CV = 0",{"$nulls":3},"YT618_TASK2_STOP"]
[{"$nulls":3},"设备2取消组合停止","取消","L5KYPZK_ZHStop_ZHTZ_Dev2StopCancel","Fix32.THISNODE.YT618_TASK2_STOP.F_CV = 0\n"]
[null,null,"信息清零","任务结束","取消","L5KYPZK_StopInfoClear_TaskClear"]
[{"$nulls":3},"批次清零",null,"L5KYPZK_StopInfoClear_BatchClear","YT618_CK3354_ACT2DB \nYT618_WZA_VALUE_ACT12\nYT618_WZA_VALUE_ACT13\nYT618_WZB_VALUE_ACT12\nYT618_WZB_VALUE_ACT13",{"$nulls":4},"清零按钮","YT618_WZ_VALUE_CLEAR"]
[{"$nulls":3},"生产清零",null,"L5KYPZK_StopInfoClear_ProdClear","Fix32.THISNODE.JK_YT618_MIXENTSC_CLEAR.F_CV = 1\n","Fix32.THISNODE.JK_YT618_MIXENTSC_CLEAR_OK.F_CV = 1",null,null,"\nFix32.THISNODE.YT618_WZ_VALUE_CLEAR.F_CV = 0  '生产清零\nFix32.THISNODE.YT618_WZA_VALUE_SET1.F_CV=0 'A一次抽空一级泵停止真空度\nFix32.THISNODE.YT618_WZA_VALUE_SET2.F_CV=0 'A一次抽空一级泵工作限制时间\nFix32.THISNODE.YT618_WZA_VALUE_SET3.F_CV=0 ’A一次加潮水停止真空度\nFix32.THISNODE.YT618_WZA_VALUE_SET4.F_CV=0 'A一次加潮气停止真空度\nFix32.THISNODE.YT618_WZA_VALUE_SET5.F_CV=0 'A一次保压时间\nFix32.THISNODE.YT618_WZA_VALUE_SET6.F_CV=0 'A二次抽空停止真空度\nFix32.THISNODE.YT618_WZA_VALUE_SET7.F_CV=0 'A二次加潮水停止真空度\nFix32.THISNODE.YT618_WZA_VALUE_SET8.F_CV=0 'A二次加潮气停止真空度\nFix32.THISNODE.YT618_WZA_VALUE_SET9.F_CV=0 ’A二次保压时间\nFix32.THISNODE.YT618_WZA_VALUE_SET15.F_CV=0 'A回抽停止真空度\nFix32.THISNODE.YT618_WZA_VALUE_SET10.F_CV=0    A加潮水开度设定\nFix32.THISNODE.YT618_WZA_VALUE_SET11.F_CV 'A加潮气开度设定\nFix32.THISNODE.YT618_WZA_VALUE_SET12.F_CV = 0    A一二次工艺选择\nFix32.THISNODE.YT618_WZB_VALUE_SET1.F_CV =0\nFix32.THISNODE.YT618_WZB_VALUE_SET1.F_CV=0 'B一次抽空一级泵停止真空度\nFix32.THISNODE.YT618_WZB_VALUE_SET2.F_CV=0 'B一次抽空一级泵工作限制时间\nFix32.THISNODE.YT618_WZB_VALUE_SET3.F_CV=0 ’B一次加潮水停止真空度\nFix32.THISNODE.YT618_WZB_VALUE_SET4.F_CV=0 'B一次加潮气停止真空度\nFix32.THISNODE.YT618_WZB_VALUE_SET5.F_CV=0 'B一次保压时间\nFix32.THISNODE.YT618_WZB_VALUE_SET6.F_CV=0 'B二次抽空停止真空度\nFix32.THISNODE.YT618_WZB_VALUE_SET7.F_CV=0 'B二次加潮水停止真空度\nFix32.THISNODE.YT618_WZB_VALUE_SET8.F_CV=0 'B二次加潮气停止真空度\nFix32.THISNODE.YT618_WZB_VALUE_SET9.F_CV=0 ’B二次保压时间\nFix32.THISNODE.YT618_WZB_VALUE_SET15.F_CV=0 'B回抽停止真空度\nFix32.THISNODE.YT618_WZB_VALUE_SET10.F_CV=0    B加潮水开度设定\nFix32.THISNODE.YT618_WZB_VALUE_SET11.F_CV 'B加潮气开度设定\nFix32.THISNODE.YT618_WZB_VALUE_SET12.F_CV = 0    B一二次工艺选择\nFix32.THISNODE.YT618A_BATCHSEQ.F_CV = 0   'YT618A批次顺序  \n\nFix32.THISNODE.YT618A_SJKSSJ.A_CV = \"\"   '真空回潮当前批次号  \nFix32.THISNODE.YT618A_SJJSSJ.A_CV = \"\"  '真空回潮段当前牌号 \nFix32.THISNODE.YT618A_BATCHNO.A_CV = \"\"   'EntryID\nFix32.THISNODE.YT618A_BRAND.A_CV = \"\"   '预计入柜号1\nFix32.THISNODE.YT618A_STUFFBRAND.A_CV = \"\"   '预计入柜号2\nFix32.THISNODE.YT618A_ENTRYID.A_CV = \"\"   '预计入柜号3\nFix32.THISNODE.YT618A_OUTGP.A_CV = \"\"   '真空回潮段计划结束时间\nFix32.THISNODE.YT618A_INGP1.A_CV = \"\"   '真空回潮段计划开始时间\nFix32.THISNODE.YT618A_INGP2.A_CV = \"\"   '真空回潮段出柜号\nFix32.THISNODE.YT618A_INGP1AMOUNT.F_CV = 0  '入1柜料量\nFix32.THISNODE.YT618A_INGP2AMOUNT.F_CV =0  '入2柜料量\nFix32.THISNODE.YT618A_INGP3AMOUNT.F_CV =0  '入3柜料量\nFix32.THISNODE.YT618A_INGPQTY.F_CV =0  '生成物料入的柜子数量\n"]
[{"$nulls":3},"3354电子秤清零",null,"L5KYPZK_StopInfoClear_Aunce3354","Fix32.THISNODE.YT618_CK3354_CLEAR.F_CV = 1"]
[{"$nulls":3},"3361电子秤清零",null,"L5KYPZK_StopInfoClear_Aunce3361","Fix32.THISNODE.YT618_CK3361_CLEAR.F_CV = 1"]
[null,"辅助操作","单机/联机",null,null,"L5KYPJL_FK_DeviceLink(object obj)  示例：string DevName,Bool BSel"]
[null,null,"故障复位",null,null,"L5KYPZK_FK_AlarmReset"," Fix32.thisnode.YT618_RESET.F_CV = 1"]
{"$rows_empty":34}
[null,null,"3315作为物流通道",{"$nulls":3}," Fix32.thisnode.YT618_ASSIST_SET1.F_CV = 1"]
[null,null,"3315作为物流通道取消",{"$nulls":3}," Fix32.thisnode.YT618_ASSIST_SET1.F_CV = 0"]
[null,null,"3316作为物流通道",{"$nulls":3},"Fix32.thisnode.YT618_ASSIST_SET2.F_CV = 1"]
[null,null,"3316作为物流通道取消",{"$nulls":3},"Fix32.thisnode.YT618_ASSIST_SET2.F_CV = 0"]
[null,null,"3315强制出箱",{"$nulls":3},"Fix32.THISNODE.YT618_WZ1_OUT_CMD.F_CV = 1"]
[null,null,"3315强制出箱取消",{"$nulls":3},"Fix32.THISNODE.YT618_WZ1_OUT_CMD.F_CV = 0"]
[null,null,"3316强制出箱",{"$nulls":3},"  Fix32.THISNODE.YT618_WZ2_OUT_CMD.F_CV = 1"]
[null,null,"3316强制出箱取消",{"$nulls":3},"  Fix32.THISNODE.YT618_WZ2_OUT_CMD.F_CV = 0"]

{"sheet":"Sheet6","index":4,"n_rows":66,"n_cols":3,"rows_kept":66,"flags":["formulas_cached_only"]}
{"$rows_empty":9}
["case \"api/L5KYPJL_SBYR_START\":  //预热启动\n                    rlt = new L5K_YP_HC().WriteFunction(\"L5KYPJL_SBYR_START\"); \n                    break;","{ //预热启动\n    \"APIName\": \"L5KYPJL_SBYR_START\",\n    \"WriteTagName\": \"YT6022_C_SJ2147_PREHEAT_START\",\n    \"CheckTagName\": \"YT6022_C_SJ2147_PREHEAT_START\",\n    \"StrValue\": 1,\n    \"DelayTime\": 1200\n  },"]
["case \"api/L5KYPJL_SBYR_CLOSE\":  //预热结束\n                    rlt = new L5K_YP_HC().WriteFunction(\"L5KYPJL_SBYR_CLOSE\"); \n                    break;","{ //预热结束\n    \"APIName\": \"L5KYPJL_SBYR_CLOSE\",\n    \"WriteTagName\": \"YT6022_C_SJ2147_PREHEAT_STOP\",\n    \"CheckTagName\": \"YT6022_C_SJ2147_PREHEAT_STOP\",\n    \"StrValue\": 1,\n    \"DelayTime\": 1200\n  },"]
["case \"api/L5KYPJL_YL_Tank1Select\":  //料筒选择-料筒1\n                    rlt = new L5K_YP_HC().WriteFunction(\"L5KYPJL_YL_Tank1Select\"); \n                    break;","{ //料筒选择-料筒1\n    \"APIName\": \"L5KYPJL_YL_Tank1Select\",\n    \"WriteTagName\": \"YT6022_SJ2147_TANK1_SEL\",\n    \"CheckTagName\": \"YT6022_SJ2147_TANK1_SEL\",\n    \"StrValue\": 1,\n    \"DelayTime\": 1200\n  },"]
["case \"api/L5KYPJL_YL_Tank2Select\":  //料筒选择-料筒2\n                    rlt = new L5K_YP_HC().WriteFunction(\"L5KYPJL_YL_Tank2Select\"); \n                    break;","{ //料筒选择-料筒2\n    \"APIName\": \"L5KYPJL_YL_Tank2Select\",\n    \"WriteTagName\": \"YT6022_SJ2147_TANK2_SEL\",\n    \"CheckTagName\": \"YT6022_SJ2147_TANK2_SEL\",\n    \"StrValue\": 1,\n    \"DelayTime\": 1200\n  },"]
["case \"api/L5KYPJL_YL_Tank1Cancel\":  //取消要料-料筒1\n                    rlt = new L5K_YP_HC().WriteFunction(\"L5KYPJL_YL_Tank1Cancel\"); \n                    break;","{ //取消要料-料筒1\n    \"APIName\": \"L5KYPJL_YL_Tank1Cancel\",\n    \"WriteTagName\": \"YT6022_SJ2147_TANK1_REQUEST\",\n    \"CheckTagName\": \"YT6022_SJ2147_TANK1_REQUEST\",\n    \"StrValue\": 1,\n    \"DelayTime\": 1200\n  },"]
["case \"api/L5KYPJL_YL_Tank2Cancel\":  //取消要料-料筒2\n                    rlt = new L5K_YP_HC().WriteFunction(\"L5KYPJL_YL_Tank2Cancel\"); \n                    break;","{ //取消要料-料筒2\n    \"APIName\": \"L5KYPJL_YL_Tank2Cancel\",\n    \"WriteTagName\": \"YT6022_SJ2147_TANK2_REQUEST\",\n    \"CheckTagName\": \"YT6022_SJ2147_TANK2_REQUEST\",\n    \"StrValue\": 1,\n    \"DelayTime\": 1200\n  },"]
["case \"api/L5KYPJL_ZHStart_GDInfoSet\":  //工单信息下发\n                    rlt = new L5K_YP_HC().WriteFunction(\"L5KYPJL_ZHStart_GDInfoSet\"); \n                    break;","{ //批开始\n    \"APIName\": \"L5KYPJL_ZHStart_BatchStart\",\n    \"WriteTagName\": \"YT6022_TASK2_BSTART\",\n    \"CheckTagName\": \"YT6022_TASK2_BSTART\",\n    \"StrValue\": 1,\n    \"DelayTime\": 1200\n  },"]
["case \"api/L5KYPJL_ZHStart_BatchStart\":  //批开始\n                    rlt = new L5K_YP_HC().WriteFunction(\"L5KYPJL_ZHStart_BatchStart\"); \n                    break;","{ //设备组合启动\n    \"APIName\": \"L5KYPJL_ZHStart_Start\",\n    \"WriteTagName\": \"YT630_IN_TASK2_START\",\n    \"CheckTagName\": \"YT630_IN_TASK2_START\",\n    \"StrValue\": 1,\n    \"DelayTime\": 1200\n  },"]
["case \"api/L5KYPJL_ZHStart_Start\":  //设备组合启动\n                    rlt = new L5K_YP_HC().WriteFunction(\"L5KYPJL_ZHStart_Start\"); \n                    break;","{ //生产提升\n    \"APIName\": \"L5KYPJL_TS_TSStart\",\n    \"WriteTagName\": \"YT6022_WPL2141_ASEND\",\n    \"CheckTagName\": \"YT6022_WPL2141_ASEND\",\n    \"StrValue\": 1,\n    \"DelayTime\": 1200\n  },"]
["case \"api/L5KYPJL_TS_TSStart\":  //生产提升\n                    rlt = new L5K_YP_HC().WriteFunction(\"L5KYPJL_TS_TSStart\"); \n                    break;","{ //强制提升\n    \"APIName\": \"L5KYPJL_TS_TSForceStart\",\n    \"WriteTagName\": \"YT6022_WPL2141_FORCEASEND\",\n    \"CheckTagName\": \"YT6022_WPL2141_FORCEASEND\",\n    \"StrValue\": 1,\n    \"DelayTime\": 1200\n  },"]
["case \"api/L5KYPJL_TS_TSForceStart\":  //强制提升\n                    rlt = new L5K_YP_HC().WriteFunction(\"L5KYPJL_TS_TSForceStart\"); \n                    break;","{ //强制停止提升\n    \"APIName\": \"L5KYPJL_TS_TSForceStop\",\n    \"WriteTagName\": \"YT6022_WPL2141_FORCESTOP\",\n    \"CheckTagName\": \"YT6022_WPL2141_FORCESTOP\",\n    \"StrValue\": 1,\n    \"DelayTime\": 1200\n  },"]
["case \"api/L5KYPJL_TS_TSForceStop\":  //强制停止提升\n                    rlt = new L5K_YP_HC().WriteFunction(\"L5KYPJL_TS_TSForceStop\"); \n                    break;","{ //批结束\n    \"APIName\": \"L5KYPJL_ZHStop_BatchEnd\",\n    \"WriteTagName\": \"YT6022_TASK2_bSTOP\",\n    \"CheckTagName\": \"YT6022_TASK2_bSTOP\",\n    \"StrValue\": 1,\n    \"DelayTime\": 1200\n  },"]
["case \"api/L5KYPJL_ZHStop_BatchEnd\":  //批结束\n                    rlt = new L5K_YP_HC().WriteFunction(\"L5KYPJL_ZHStop_BatchEnd\"); \n                    break;","{ //余料回收\n    \"APIName\": \"L5KYPJL_ZHStopRec_Pipe_InTank\",\n    \"WriteTagName\": \"YT6022_SJ2147_PIPE_REUSE\",\n    \"CheckTagName\": \"YT6022_SJ2147_PIPE_REUSE\",\n    \"StrValue\": 1,\n    \"DelayTime\": 1200\n  },"]
["case \"api/L5KYPJL_ZHStopRec_Pipe_InTank\":  //余料回收\n                    rlt = new L5K_YP_HC().WriteFunction(\"L5KYPJL_ZHStopRec_Pipe_InTank\"); \n                    break;","{ //\n    \"APIName\": \"L5KYPJL_ZHStopRec_Tank1_InMRoom\",\n    \"WriteTagName\": \"YT6022_SJ2147_TANK1_REUSE\",\n    \"CheckTagName\": \"YT6022_SJ2147_TANK1_REUSE\",\n    \"StrValue\": 1,\n    \"DelayTime\": 1200\n  },"]
["case \"api/L5KYPJL_ZHStopRec_Tank1_InMRoom\":  //\n                    rlt = new L5K_YP_HC().WriteFunction(\"L5KYPJL_ZHStopRec_Tank1_InMRoom\"); \n                    break;","{ //\n    \"APIName\": \"L5KYPJL_ZHStopRec_Tank2_InMRoom\",\n    \"WriteTagName\": \"YT6022_SJ2147_TANK2_REUSE\",\n    \"CheckTagName\": \"YT6022_SJ2147_TANK2_REUSE\",\n    \"StrValue\": 1,\n    \"DelayTime\": 1200\n  },"]
["case \"api/L5KYPJL_ZHStopRec_Tank2_InMRoom\":  //\n                    rlt = new L5K_YP_HC().WriteFunction(\"L5KYPJL_ZHStopRec_Tank2_InMRoom\"); \n                    break;","{ //\n    \"APIName\": \"L5KYPJL_ZHStopRec_Pipe_Clear\",\n    \"WriteTagName\": \"YT6022_SJ2147_PIPE_CLEAR\",\n    \"CheckTagName\": \"YT6022_SJ2147_PIPE_CLEAR\",\n    \"StrValue\": 1,\n    \"DelayTime\": 1200\n  },"]
["case \"api/L5KYPJL_ZHStopRec_Pipe_Clear\":  //\n                    rlt = new L5K_YP_HC().WriteFunction(\"L5KYPJL_ZHStopRec_Pipe_Clear\"); \n                    break;","{ //\n    \"APIName\": \"L5KYPJL_ZHStopRec_Tank1_Clear\",\n    \"WriteTagName\": \"YT6022_SJ2147_TANK1_CLEAR_S\",\n    \"CheckTagName\": \"YT6022_SJ2147_TANK1_CLEAR_S\",\n    \"StrValue\": 1,\n    \"DelayTime\": 1200\n  },"]
["case \"api/L5KYPJL_ZHStopRec_Tank1_Clear\":  //\n                    rlt = new L5K_YP_HC().WriteFunction(\"L5KYPJL_ZHStopRec_Tank1_Clear\"); \n                    break;","{ //\n    \"APIName\": \"L5KYPJL_ZHStopRec_Tank2_Clear\",\n    \"WriteTagName\": \"YT6022_SJ2147_TANK2_CLEAR_S\",\n    \"CheckTagName\": \"YT6022_SJ2147_TANK2_CLEAR_S\",\n    \"StrValue\": 1,\n    \"DelayTime\": 1200\n  },"]
["case \"api/L5KYPJL_ZHStopRec_Tank2_Clear\":  //\n                    rlt = new L5K_YP_HC().WriteFunction(\"L5KYPJL_ZHStopRec_Tank2_Clear\"); \n                    break;","{ //信息清零\n    \"APIName\": \"L5KYPJL_ZHStopInfoClear_BatchEnd\",\n    \"WriteTagName\": \"YT6022_TASK2_bSTOP\",\n    \"CheckTagName\": \"YT6022_TASK2_bSTOP\",\n    \"StrValue\": 1,\n    \"DelayTime\": 1200\n  },"]
["case \"api/L5KYPJL_ZHStopInfoClear_BatchEnd\":  //信息清零\n                    rlt = new L5K_YP_HC().WriteFunction(\"L5KYPJL_ZHStopInfoClear_BatchEnd\"); \n                    break;","{ //\n    \"APIName\": \"L5KYPJL_ZHStopInfoClear_TankClear\",\n    \"WriteTagName\": \"YT6022_IN_TASK2_FINISH\",\n    \"CheckTagName\": \"YT6022_IN_TASK2_FINISH\",\n    \"StrValue\": 1,\n    \"DelayTime\": 1200\n  },"]
["case \"api/L5KYPJL_ZHStopInfoClear_TankClear\":  //\n                    rlt = new L5K_YP_HC().WriteFunction(\"L5KYPJL_ZHStopInfoClear_TankClear\"); \n                    break;","{ //\n    \"APIName\": \"L5KYPJL_ZHStopInfoClear_BatchClear\",\n    \"WriteTagName\": \"YT6022_LeafBatchNo\",\n    \"CheckTagName\": \"YT6022_LeafBatchNo\",\n    \"StrValue\": 1,\n    \"DelayTime\": 1200\n  },"]
["case \"api/L5KYPJL_ZHStopInfoClear_BatchClear\":  //\n                    rlt = new L5K_YP_HC().WriteFunction(\"L5KYPJL_ZHStopInfoClear_BatchClear\"); \n                    break;","{ //设备组合停止\n    \"APIName\": \"L5KYPJL_ZHStop_Stop\",\n    \"WriteTagName\": \"YT6022_IN_TASK2_STOP\",\n    \"CheckTagName\": \"YT6022_IN_TASK2_STOP\",\n    \"StrValue\": 1,\n    \"DelayTime\": 1200\n  },"]
["case \"api/L5KYPJL_ZHStopInfoClear_ProdClear\":  //\n                    rlt = new L5K_YP_HC().WriteFunction(\"L5KYPJL_ZHStopInfoClear_ProdClear\"); \n                    break;","{ //故障复位\n    \"APIName\": \"L5KYPJL_FK_AlarmReset\",\n    \"WriteTagName\": \"YT6022_CONTROL_YT6022_RESET\",\n    \"CheckTagName\": \"YT6022_CONTROL_YT6022_RESET\",\n    \"StrValue\": 1,\n    \"DelayTime\": 1200\n  },"]
["case \"api/L5KYPJL_ZHStopInfoClear_OutYPG_PathClear\":  //\n                    rlt = new L5K_YP_HC().WriteFunction(\"L5KYPJL_ZHStopInfoClear_OutYPG_PathClear\"); \n                    break;"]
["case \"api/L5KYPJL_ZHStopInfoClear_OutYPG_InfoClear\":  //\n                    rlt = new L5K_YP_HC().WriteFunction(\"L5KYPJL_ZHStopInfoClear_OutYPG_InfoClear\"); \n                    break;"]
["case \"api/L5KYPJL_ZHStopInfoClear_InYG_PathClear\":  //\n                    rlt = new L5K_YP_HC().WriteFunction(\"L5KYPJL_ZHStopInfoClear_InYG_PathClear\"); \n                    break;"]
["case \"api/L5KYPJL_ZHStopInfoClear_InYG_InfoClear\":  //\n                    rlt = new L5K_YP_HC().WriteFunction(\"L5KYPJL_ZHStopInfoClear_InYG_InfoClear\"); \n                    break;"]
["case \"api/L5KYPJL_ZHStop_Stop\":  //设备组合停止\n                    rlt = new L5K_YP_HC().WriteFunction(\"L5KYPJL_ZHStop_Stop\"); \n                    break;"]
["case \"api/L5KYPJL_FK_AlarmReset\":  //故障复位\n                    rlt = new L5K_YP_HC().WriteFunction(\"L5KYPJL_FK_AlarmReset\"); \n                    break;"]
{"$rows_empty":12}
["public string","工序","{get;set;}"]
["public string","操作按钮","{get;set;}"]
["public string","组件封装","{get;set;}"]
["public string","业务说明","{get;set;}"]
["public string","参数说明","{get;set;}"]
["public string","API接口名","{get;set;}"]
["public string","写入点位","{get;set;}"]
["public string","检查点位","{get;set;}"]
["public string","测试状态","{get;set;}"]
["public string","测试方法","{get;set;}"]
["public string","测试输入","{get;set;}"]
["public string","测试输出","{get;set;}"]
["public string","测试点位变化","{get;set;}"]
["public string","备注","{get;set;}"]
["public string","API状态","{get;set;}"]
["public string","按键逻辑","{get;set;}"]

{"sheet":"API封装需求","index":5,"n_rows":3,"n_cols":1,"rows_kept":3,"flags":["formulas_cached_only"]}
["支持单点位下发/读取"]
["支持批量点位下发/读取"]
["支持条件验证"]

{"sheet":"300加料","index":6,"n_rows":138,"n_cols":12,"rows_kept":138,"merged":[[1,0,39,0],[1,1,4,1],[5,1,10,1],[11,1,19,1],[19,11,22,11],[20,1,22,1],[23,1,37,1],[24,2,29,2],[30,2,36,2],[38,1,39,1],[41,0,60,0],[41,1,44,1],[45,1,50,1],[52,1,54,1],[55,1,58,1],[55,2,57,2],[59,1,60,1],[62,0,98,0],[62,1,65,1],[66,1,71,1],[72,1,80,1],[81,1,83,1],[84,1,96,1],[85,2,88,2],[89,2,95,2],[97,1,98,1],[100,0,137,0],[100,1,103,1],[104,1,109,1],[110,1,118,1],[119,1,121,1],[122,1,135,1],[123,2,127,2],[128,2,134,2],[136,1,137,1]],"flags":["formulas_cached_only"]}
["工序","操作按钮","组件封装","业务说明","参数说明","API接口名","请求类型","测试状态","备注","API状态","写入点位","检查点位"]
["5千加料","设备预热","预热启动",null,"无","L5KYPJL_SBYR_START","Get",{"$nulls":3},"YT6022_C_WQ2126_PREHEAT_START"]
[null,null,"预热温度值设定",null,"温度值","L5KYPJL_SBYR_YRWDSET(float Temp)","Post",{"$nulls":3},"YT6022_C_SJ2116_PREHEAT_START"]
[null,null,"预热生产温度值设定",null,"温度值","L5KYPJL_SBYR_YXWDSET(float Temp)","Post",{"$nulls":3},"YT6022_VALUE_WQ2126_P_SET_1"]
[null,null,"预热结束",null,"无","L5KYPJL_SBYR_CLOSE","Get",{"$nulls":3},"YT6022_VALUE_WQ2116_P_SET_1"]
[null,"要料","料筒选择-料筒1",null,"无","L5KYPJL_YL_Tank1Select","Get",{"$nulls":3},"YT6022_VALUE_WQ2126_PID4_SP"]
[null,null,"料筒选择-料筒2",null,"无","L5KYPJL_YL_Tank2Select","Get",{"$nulls":3},"YT6022_VALUE_WQ2116_PID4_SP"]
[null,null,"要料信息下发-料筒1",null,"料液重量、料液代码、批次号","L5KYPJL_YL_Tank1Info_Set(object info)","Post",{"$nulls":3},"YT6022_C_WQ2126_PREHEAT_STOP"]
[null,null,"要料信息下发-料筒2",null,"料液重量、料液代码、批次号","L5KYPJL_YL_Tank2Info_Set(object info)","Post",{"$nulls":3},"YT6022_C_SJ2116_PREHEAT_STOP"]
[null,null,"取消要料-料筒1",null,"无","L5KYPJL_YL_Tank1Cancel","Get",{"$nulls":3},"YT6022_TASK1_R09（真空））"]
[null,null,"取消要料-料筒2",null,"无","L5KYPJL_YL_Tank2Cancel","Get",{"$nulls":3},"YT6022_TASK1_R06（薄片）"]
[null,"组合启动","工单信息下发",null,"工单号、批次号、牌号","L5KYPJL_ZHStart_GDInfoSet(string YPGno,string BatchNo,string BrandNo）JSON格式","Post",{"$nulls":3},"YT6022_TASK1_R09（真空）"]
[null,null,"批开始",null,"无","L5KYPJL_ZHStart_BatchStart","Get",{"$nulls":3},"YT6022_TASK1_R06（薄片）"]
[null,null,"出预配柜条件验证及路径下发",null,"柜号","L5KYPJL_ZHStart_OutYPGCheck(string YPGno）","Post",{"$nulls":3},"YT6022_MIXENTRYID（工单）/YT6022_MIXBATCHNO（批次）/YT6022_MIXBRAND（牌号）"]
[null,null,"出预配柜路径取消",null,"柜号","L5KYPJL_ZHStart_OutYPGCancel(string YPGno）","Post",{"$nulls":3},"YT6022_TASK1_BSTART"]
[null,null,"出预配柜信息下发",null,"柜号","L5KYPJL_ZHStart_OutPGInfoSet(string YPGno）","Post",{"$nulls":3},"JK_YT6022_TANK1_TAG"]
[null,null,"进叶柜条件验证及路径下发",null,"柜号","L5KYPJL_ZHStart_InYGCheck(string YPGno）","Post",{"$nulls":3},"JK_YT6022_TANK1_TAG"]
[null,null,"进叶柜路径取消",null,"柜号",null,"Post",{"$nulls":3},"JK_YT6022_TASK1_A04（YP04）/JK_YT6022_TASK1_A03（YP05）/JK_YT6022_TASK1_A02（YP06）/JK_YT6022_TASK1_A01（YP07）","JK_YT6022_YP04_INT_UNITERR\n/JK_YT6022_YP05_INT_UNITERR\n/JK_YT6022_YP06_INT_UNITERR\n/JK_YT6022_YP07_INT_UNITERR"]
[null,null,"进叶柜信息下发",null,"柜号、批次号、牌号","L5KYPJL_ZHStart_InYgInfoSet(string YPGno,string BatchNo,string BrandNo）JSON格式","Post",{"$nulls":3},"JK_YT6022_TASK1_A04（YP04）/JK_YT6022_TASK1_A03（YP05）/JK_YT6022_TASK1_A02（YP06）/JK_YT6022_TASK1_A01（YP07）"]
[null,null,"设备组合启动",null,"无","L5KYPJL_ZHStart_Start","Get",{"$nulls":3},"YT6022_GP_2139R_JOB(YP04批次)\n/YT6022_GP_2139R_BRAND（牌号）"]
[null,"生产提升","生产提升",null,"无","L5KYPJL_TS_TSStart","Get",{"$nulls":3},"YT6022_GP_2139L_JOB(YP05批次)\n/YT6022_GP_2139L_BRAND（牌号）"]
[null,null,"强制提升",null,"无","L5KYPJL_TS_TSForceStart","Get",{"$nulls":3},"YT6022_GP_2138R_JOB(YP06批次)\n/YT6022_GP_2138R_BRAND（牌号）"]
[null,null,"强制停止提升",null,"无","L5KYPJL_TS_TSForceStop","Get",{"$nulls":3},"YT6022_GP_2138L_JOB(YP07批次)\n/YT6022_GP_2138L_BRAND（牌号）"]
[null,"组合停止","批结束",null,"无","L5KYPJL_ZHStop_BatchEnd","Get",{"$nulls":3},"YT6022_IN_TASK1_START"]
[null,null,"余料回收","管路余料回到料筒","无","L5KYPJL_ZHStopRec_Pipe_InTank","Get",{"$nulls":3},"YT6022_WPL3373_ASEND"]
[{"$nulls":3},"回料到料房-料筒1","无","L5KYPJL_ZHStopRec_Tank1_InMRoom","Get",{"$nulls":3},"YT6022_WPL3373_FORCEASEND"]
[{"$nulls":3},"回料到料房-料筒2","无","L5KYPJL_ZHStopRec_Tank2_InMRoom","Get",{"$nulls":3},"YT6022_WPL3373_FORCESTOP"]
[{"$nulls":3},"管路清洗","无","L5KYPJL_ZHStopRec_Pipe_Clear","Get",{"$nulls":3},"YT6022_WPL2122_ASEND"]
[{"$nulls":3},"料筒清洗-料筒1","无","L5KYPJL_ZHStopRec_Tank1_Clear","Get",{"$nulls":3},"YT6022_WPL2122_FORCEASEND"]
[{"$nulls":3},"料筒清洗-料筒2","无","L5KYPJL_ZHStopRec_Tank2_Clear","Get",{"$nulls":3},"YT6022_WPL2122_FORCESTOP"]
[null,null,"信息清零","任务结束","无","L5KYPJL_ZHStopInfoClear_TankClear","Get",{"$nulls":3},"YT6022_TASK1_BSTOP"]
[{"$nulls":3},"批次清零","无","L5KYPJL_ZHStopInfoClear_BatchClear","Get",{"$nulls":3},"YT6022_IN_TASK1_FINISH"]
[{"$nulls":3},"生产清零","无","L5KYPJL_ZHStopInfoClear_ProdClear","Get",{"$nulls":3},"JK_YT6022_MIXENTPC_CLEAR","JK_YT6022_MIXENTPC_UNITERR"]
[{"$nulls":3},"出预配柜路径清零","无","L5KYPJL_ZHStopInfoClear_OutYPG_PathClear","Get",{"$nulls":3},"JK_YT6022_MIXENTSC_CLEAR","JK_YT6022_MIXENTSC_UNITERR"]
[{"$nulls":3},"出预配柜柜号清零","无","L5KYPJL_ZHStopInfoClear_OutYPG_InfoClear","Get",{"$nulls":3},"YT6022_TASK1_NODEA\n"]
[{"$nulls":3},"进叶柜路径清零","无","L5KYPJL_ZHStopInfoClear_InYG_PathClear","Get"]
[{"$nulls":3},"进叶柜柜号清零","无","L5KYPJL_ZHStopInfoClear_InYG_InfoClear","Get",{"$nulls":3},"YT6022_IN_TASK1_STOP"]
[null,null,"设备组合停止",null,"无","L5KYPJL_ZHStop_Stop","Get"]
[null,"辅助操作","单机/联机",null,"段号","L5KYPJL_FK_DeviceLink(string DeviceName,Bool Bsel)","Post",{"$nulls":3},"YT6022_CONTROL_YT6022_RESET"]
[null,null,"故障复位",null,"无","L5KYPJL_FK_AlarmReset","Get"]
[{"$nulls":10},"YT6022_WQ2_SEL"]
["3千一次加料","设备预热","预热启动",null,"无","L3KYPJL1_SBYR_START","Get"]
[null,null,"预热温度值设定",null,"温度值","L3KYPJL1_SBYR_YRWDSET(float Temp)","Post"]
[null,null,"预热生产温度值设定",null,"温度值","L3KYPJL1_SBYR_YXWDSET(float Temp)","Post"]
[null,null,"预热结束",null,"无","L3KYPJL1_SBYR_CLOSE","Get"]
[null,"要料","料筒选择-料筒1",null,"无","L3KYPJL1_YL_Tank1Select","Get"]
[null,null,"料筒选择-料筒2",null,"无","L3KYPJL1_YL_Tank2Select","Get"]
[null,null,"要料信息下发-料筒1",null,"料液重量、料液代码、批次号","L3KYPJL1_YL_Tank1Info_Set(object info)","Post"]
[null,null,"要料信息下发-料筒2",null,"料液重量、料液代码、批次号","L3KYPJL1_YL_Tank2Info_Set(object info)","Post"]
[null,null,"取消要料-料筒1",null,"无","L3KYPJL1_YL_Tank1Cancel","Get"]
[null,null,"取消要料-料筒2",null,"无","L3KYPJL1_YL_Tank2Cancel","Get"]
[null,"组合启动","设备组合启动",null,"无","L3KYPJL1_ZHStart_GDInfoSet","Get"]
[null,"生产提升","生产提升",null,"无","L3KYPJL1_TS_TSStart","Get"]
[null,null,"强制提升",null,"无","L3KYPJL1_TS_TSForceStart","Get"]
[null,null,"强制停止提升",null,"无","L3KYPJL1_TS_TSForceStop","Get"]
[null,"组合停止","余料回收","管路余料回到料筒","无","L3KYPJL1_ZHStopRec_Pipe_InTank","Get"]
[{"$nulls":3},"料筒清洗-料筒1","无","L3KYPJL1_ZHStopRec_Tank1_InMRoom","Get"]
[{"$nulls":3},"料筒清洗-料筒2","无","L3KYPJL1_ZHStopRec_Tank2_InMRoom","Get"]
[null,null,"设备组合停止",null,"无","L3KYPJL1_ZHSTOP_STOP","Get"]
[null,"辅助操作","单机/联机",null,"段号","L3KYPJL1_FK_DeviceLink(string DeviceName,Bool Bsel)","Post"]
[null,null,"故障复位",null,"无","L3KYPJL1_FK_AlarmReset","Get"]
[]
["3千二次加料","设备预热","预热启动",null,"无","L3KYPJL2_SBYR_START","Get"]
[null,null,"预热温度值设定",null,"温度值","L3KYPJL2_SBYR_YRWDSET(float Temp)","Post"]
[null,null,"预热生产温度值设定",null,"温度值","L3KYPJL2_SBYR_YXWDSET(float Temp)","Post"]
[null,null,"预热结束",null,"无","L3KYPJL2_SBYR_CLOSE","Get"]
[null,"要料","料筒选择-料筒1",null,"无","L3KYPJL2_YL_Tank1Select","Get"]
[null,null,"料筒选择-料筒2",null,"无","L3KYPJL2_YL_Tank2Select","Get"]
[null,null,"要料信息下发-料筒1",null,"料液重量、料液代码、批次号","L3KYPJL2_YL_Tank1Info_Set(object info)","Post"]
[null,null,"要料信息下发-料筒2",null,"料液重量、料液代码、批次号","L3KYPJL2_YL_Tank2Info_Set(object info)","Post"]
[null,null,"取消要料-料筒1",null,"无","L3KYPJL2_YL_Tank1Cancel","Get"]
[null,null,"取消要料-料筒2",null,"无","L3KYPJL2_YL_Tank2Cancel","Get"]
[null,"组合启动","工单信息下发",null,"工单号、批次号、牌号","L3KYPJL2_ZHStart_GDInfoSet","Post"]
[null,null,"批开始",null,"无","L3KYPJL2_ZHStart_BatchStart","Get"]
[null,null,"出预配柜条件验证及路径下发",null,"柜号","L3KYPJL2_ZHStart_OutYPGCheck(string YPGno）","Post"]
[null,null,"出预配柜路径取消",null,"柜号","L3KYPJL2_ZHStart_OutYPGcancel(string YPGno）","Post"]
[null,null,"出预配柜信息下发",null,"柜号","L3KYPJL2_ZHStart_OutPGInfoSet(string YPGno）","Post"]
[null,null,"进配叶柜条件验证及路径下发",null,"柜号","L3KYPJL2_ZHStart_InYGCheck(string YPGno）","Post"]
[null,null,"进配叶柜路径取消",null,"柜号","L3KYPJL2_ZHStart_InYGCancel(string YPGno）","Post"]
[null,null,"进配叶柜信息下发",null,"柜号、批次号、牌号","L3KYPJL2_ZHStart_InYgInfoSet(string YPGno）","Post"]
[null,null,"设备组合启动",null,"无","L3KYPJL2_ZHStart_Start","Get"]
[null,"生产提升","生产提升",null,"无","L3KYPJL2_TS_TSStart","Get"]
[null,null,"强制提升",null,"无","L3KYPJL2_TS_TSForceStart","Get"]
[null,null,"强制停止提升",null,"无","L3KYPJL2_TS_TSForceStop","Get"]
[null,"组合停止","批结束",null,"无","L3KYPJL2_ZHStop_BatchEnd","Get"]
[null,null,"余料回收","管路余料回到料筒","无","L3KYPJL2_ZHStopRec_Pipe_InTank","Get"]
[{"$nulls":3},"管路清洗","无","L3KYPJL2_ZHStopRec_Pipe_Clear","Get"]
[{"$nulls":3},"料筒清洗-料筒1","无","L3KYPJL2_ZHStopRec_Tank1_InMRoom","Get"]
[{"$nulls":3},"料筒清洗-料筒2","无","L3KYPJL2_ZHStopRec_Tank2_InMRoom","Get"]
[null,null,"信息清零","任务结束","无","L3KYPJL2_ZHSTOP_TASK_END","Get"]
[{"$nulls":3},"批次清零","无","L3KYPJL2_ZHSTOP_CLEAR_BATCH","Get"]
[{"$nulls":3},"生产清零","无","L3KYPJL2_ZHSTOP_CLEAR_PRODINFO","Get"]
[{"$nulls":3},"出预配柜路径清零","无","L3KYPJL2_ZHStopInfoClear_OutYPG_PathClear","Get"]
[{"$nulls":3},"出预配柜柜号清零","无","L3KYPJL2_ZHStopInfoClear_OutYPG_InfoClear","Get"]
[{"$nulls":3},"进配叶柜路径清零","无","L3KYPJL2_ZHStopInfoClear_InYG_PathClear","Get"]
[{"$nulls":3},"进配叶柜柜号清零","无","L3KYPJL2_ZHStopInfoClear_InYG_InfoClear","Get"]
[null,null,"设备组合停止",null,"无","L3KYPJL2_ZHStop_Stop","Get"]
[null,"辅助操作","单机/联机",null,"段号","L3KYPJL2_FK_DeviceLink(string DeviceName,Bool Bsel)","Post"]
[null,null,"故障复位",null,"无","L3KYPJL2_FK_AlarmReset","Get"]
[]
["9千加料","设备预热","预热启动",null,"无"]
[null,null,"预热温度值设定",null,"温度值"]
[null,null,"预热生产温度值设定",null,"温度值"]
[null,null,"预热结束",null,"无"]
[null,"要料","料筒选择-料筒1",null,"无"]
[null,null,"料筒选择-料筒2",null,"无"]
[null,null,"要料信息下发-料筒1",null,"料液重量、料液代码、批次号"]
[null,null,"要料信息下发-料筒2",null,"料液重量、料液代码、批次号"]
[null,null,"取消要料-料筒1",null,"无"]
[null,null,"取消要料-料筒2",null,"无"]
[null,"组合启动","工单信息下发",null,"工单号、批次号、牌号"]
[null,null,"批开始",null,"无"]
[null,null,"出预配柜条件验证及路径下发",null,"柜号"]
[null,null,"出预配柜路径取消",null,"柜号"]
[null,null,"出预配柜信息下发",null,"柜号"]
[null,null,"进叶柜条件验证及路径下发",null,"柜号"]
[null,null,"进叶柜路径取消",null,"柜号"]
[null,null,"进叶柜信息下发",null,"柜号、批次号、牌号"]
[null,null,"设备组合启动",null,"无"]
[null,"生产提升","生产提升",null,"无"]
[null,null,"强制提升",null,"无"]
[null,null,"强制停止提升",null,"无"]
[null,"组合停止","批结束",null,"无"]
[null,null,"余料回收","管路余料回到料筒","无"]
[{"$nulls":3},"回料到料房-料筒1","无"]
[{"$nulls":3},"回料到料房-料筒2","无"]
[{"$nulls":3},"料筒清洗-料筒1","无"]
[{"$nulls":3},"料筒清洗-料筒2","无"]
[null,null,"信息清零","任务结束","无"]
[{"$nulls":3},"批次清零","无"]
[{"$nulls":3},"生产清零","无"]
[{"$nulls":3},"出预配柜路径清零","无"]
[{"$nulls":3},"出预配柜柜号清零","无"]
[{"$nulls":3},"进叶柜路径清零","无"]
[{"$nulls":3},"进叶柜柜号清零","无"]
[null,null,"设备组合停止",null,"无"]
[null,"辅助操作","单机/联机",null,"段号"]
[null,null,"故障复位",null,"无"]

{"sheet":"白肋烟","index":7,"n_rows":157,"n_cols":18,"rows_kept":157,"merged":[[5,0,22,0],[5,1,15,1],[10,2,12,2],[13,2,14,2],[13,4,14,4],[16,1,20,1],[21,1,22,1],[24,0,81,0],[24,1,27,1],[28,1,58,1],[56,2,57,2],[56,4,57,4],[59,1,61,1],[62,1,79,1],[63,2,74,2],[80,1,81,1],[83,0,119,0],[83,1,86,1],[87,1,102,1],[95,2,99,2],[100,2,101,2],[103,1,108,1],[109,2,112,2],[113,1,117,1],[118,1,119,1],[122,0,137,0],[122,1,130,1],[127,2,129,2],[131,1,135,1],[136,1,137,1],[142,0,156,0],[142,1,156,1]],"flags":["formulas_cached_only"]}
["工序","操作按钮","组件封装","业务说明","参数说明","API接口名","API方式","API传入参数","API测试结果","API接口检查点位","API接口写入点","触发脚本","备注","API状态","IFIX点位","代码生成","配置文件","代码标记"]
["加里料调度模式",{"$nulls":9},"Fix32.ThISNODE.InnerStuffDDMS.F_CV = 0","Fix32.ThISNODE.InnerStuffDDMS.F_CV = 0"]
["加里料调度模式取消",{"$nulls":9},"Fix32.ThISNODE.InnerStuffDDMS.F_CV = 1","Fix32.ThISNODE.InnerStuffDDMS.F_CV = 1"]
["加表料调度模式",{"$nulls":9},"Fix32.ThISNODE.LEAFINGPDDMS.F_CV = 0","Fix32.ThISNODE.OuterStuffDDMS.F_CV = 0"]
["加表料调度模式取消",{"$nulls":9}," Fix32.ThISNODE.LEAFINGPDDMS.F_CV = 1","Fix32.ThISNODE.OuterStuffDDMS.F_CV = 1"]
["白肋烟进柜段",null,"工单信息下发",null,"工单号、批次号、牌号",{"$nulls":6},"Fix32.THISNODE.PreMixEntryID.A_CV\nFix32.THISNODE.PreMixBatchNo.A_CV\nFix32.THISNODE.PreMixBrand.A_CV"]
[null,null,"批开始",null,"无",{"$nulls":6},"     Fix32.THISNODE.YT612InGPBatchStart.F_CV = 1\n     Fix32.THISNODE.YT612InGPBatchStop.F_CV = 0"]
[null,null,"设备单元自动",{"$nulls":8},"     Fix32.THISNODE.YT612InGPMAN.F_CV = 0\n     Fix32.THISNODE.YT612InGPAUTO.F_CV = 1\n     Fix32.THISNODE.YT612InGPLOCK.F_CV = 0"]
[null,null,"设备单元单机",{"$nulls":8},"     Fix32.THISNODE.YT612InGPMAN.F_CV = 1\n     Fix32.THISNODE.YT612InGPAUTO.F_CV = 0\n     Fix32.THISNODE.YT612InGPLOCK.F_CV = 0"]
[null,null,"设备单元闭锁",{"$nulls":8},"     Fix32.THISNODE.YT612InGPMAN.F_CV = 0\n     Fix32.THISNODE.YT612InGPAUTO.F_CV = 0\n     Fix32.THISNODE.YT612InGPLOCK.F_CV = 1"]
[null,null,"进预配柜条件验证","BLG1",{"$nulls":7},"     Fix32.THISNODE.GP3104InSelCur.F_CV = 1\n      Fix32.THISNODE.GP3104_1InSelCur.F_CV = 0\n"]
[{"$nulls":3},"BLG2",{"$nulls":7},"    Fix32.THISNODE.GP3104InSelCur.F_CV = 0\n      Fix32.THISNODE.GP3104_1InSelCur.F_CV = 1"]
[{"$nulls":3},"不进柜",{"$nulls":7},"       Fix32.THISNODE.GP3104InSelCur.F_CV = 0\n      Fix32.THISNODE.GP3104_1InSelCur.F_CV = 0"]
[null,null,"进预配柜信息下发(增加柜号写入ifix点)","BLG1",{"$nulls":7},"Fix32.thisnode.BLG1BatchNo1.A_CV/Fix32.thisnode.BLG1Brand1.A_CV/"]
[{"$nulls":3},"BLG2",{"$nulls":7},"Fix32.thisnode.BLG2BatchNo1.A_CV/Fix32.thisnode.BLG2Brand1.A_CV"]
[null,null,"进柜段组合启动",null,"无",{"$nulls":6},"Fix32.THISNODE.YT612InGPGStart.F_CV = 1"]
[null,"组合停止","批结束【确认】",null,"无",{"$nulls":6},"     Fix32.THISNODE.YT612InGPBatchStart.F_CV = 0\n     Fix32.THISNODE.YT612InGPBatchStop.F_CV = 1"]
[null,null,"批次清零","无信息","无"]
[null,null,"生产清零","无信息","无"]
[null,null,"预配柜清零（工单信息下发的业务柜号）",null,"无"]
[null,null,"设备组合停止",null,"无",{"$nulls":6},"Fix32.THISNODE.YT612InGPGStop.F_CV = 1"]
[null,"辅助操作","单机/联机【待定】","需根据昆船系统的单机/联机功能把所有段都单独封装","段号"]
[null,null,"故障复位","参考昆船原的功能？","无",{"$nulls":6}," Fix32.THISNODE.YT612InGPReset.F_CV = 1"]
[]
["白肋烟加里料","设备预热","预热启动",null,"无",{"$nulls":6},"Fix32.THISNODE.SJ3112PreHeatStart.F_CV = 1"]
[null,null,"预热温度值设定","无信息","温度值"]
[null,null,"生产温度值设定",null,"温度值",{"$nulls":6},"SJ3112WORKTEMPSET"]
[null,null,"预热结束",null,"无",{"$nulls":6}," Fix32.THISNODE.SJ3112PreHeatStop.F_CV = 1"]
[null,null,"工单信息下发",null,"工单号、批次号、牌号",{"$nulls":6},"Fix32.THISNODE.InnerStuffEntryID.A_CV\nFix32.THISNODE.InnerStuffBatchNo.A_CV\nFix32.THISNODE.InnerStuffBrand.A_CV"]
[null,null,"单机",{"$nulls":8},"     Fix32.THISNODE.YT612InnerStuffMAN.F_CV = 1\n     Fix32.THISNODE.YT612InnerStuffAUTO.F_CV = 0\n     Fix32.THISNODE.YT612InnerStuffLOCK.F_CV = 0"]
[null,null,"自动",{"$nulls":8},"     Fix32.THISNODE.YT612InnerStuffMAN.F_CV = 0\n     Fix32.THISNODE.YT612InnerStuffAUTO.F_CV = 1\n     Fix32.THISNODE.YT612InnerStuffLOCK.F_CV = 0"]
[null,null,"闭锁",{"$nulls":8},"     Fix32.THISNODE.YT612InnerStuffMAN.F_CV = 0\n     Fix32.THISNODE.YT612InnerStuffAUTO.F_CV = 0\n     Fix32.THISNODE.YT612InnerStuffLOCK.F_CV = 1\n     Call Modlogin.Oplog((1), (0), (1), \"加里料段段"]
[null,null,"要料信息下发-料筒1",null,"料液重量、料液代码、批次号",{"$nulls":6},"    Fix32.THISNODE.SJ3112Tank1AskQty.F_CV = \nFix32.THISNODE.SJ3112Tank1AskBatch.A_CV =\n   Fix32.THISNODE.SJ3112Tank1AskBrand.A_CV = \n\n"]
[null,null,"要料信息下发-料筒2",null,"料液重量、料液代码、批次号",{"$nulls":6},"  Fix32.THISNODE.SJ3112Tank2AskQty.F_CV = \n Fix32.THISNODE.SJ3112Tank2AskBatch.A_CV =\n   Fix32.THISNODE.SJ3112Tank2AskBrand.A_CV =\n  \n"]
[null,null,"要料请求-料筒1",null,"无",{"$nulls":6}," Fix32.THISNODE.SJ3112Tank1AskStuff.F_CV = 1"]
[null,null,"要料请求-料筒2",null,"无",{"$nulls":6},"   Fix32.THISNODE.SJ3112Tank2AskStuff.F_CV = 1"]
[null,null,"取消要料请求-料筒1",null,"无",{"$nulls":6},"Fix32.THISNODE.SJ3112Tank1AskStuff.F_CV = 0"]
[null,null,"取消要料请求-料筒2",null,"无",{"$nulls":6},"   Fix32.THISNODE.SJ3112Tank2AskStuff.F_CV = 0"]
[null,null,"批开始",null,"无",{"$nulls":6},"     Fix32.THISNODE.YT612InnerStuffBatchStart.F_CV = 1\n     Fix32.THISNODE.YT612InnerStuffBatchStop.F_CV = 0"]
[{"$nulls":3},"白肋烟加里料段生产方式不进柜",{"$nulls":7},"Fix32.THISNODE.InnerStuffProdModeCur.F_CV = 0"]
[{"$nulls":3},"加里料段生产方式进中柜",{"$nulls":7},"  Fix32.THISNODE.InnerStuffProdModeCur.F_CV = 1"]
[{"$nulls":3},"出柜段出BLG1柜操作",{"$nulls":7}," Fix32.THISNODE.GP3104OutSelCur.F_CV = 1"]
[{"$nulls":3},"出柜段出BLG2柜操作",{"$nulls":7}," Fix32.THISNODE.GP3104_1OutSelCur.F_CV = 1"]
[{"$nulls":3},"加里料段不出柜",{"$nulls":7},"      Fix32.THISNODE.GP3104OutSelCur.F_CV = 0\n      Fix32.THISNODE.GP3104_1OutSelCur.F_CV = 0"]
[{"$nulls":3},"加表料段SJ3115料筒1选择",{"$nulls":7},"       Fix32.THISNODE.SJ3112Tank1SelCur.F_CV = 1\n      Fix32.THISNODE.SJ3112Tank2SelCur.F_CV = 0"]
[{"$nulls":3},"加表料段SJ3115料筒2选择",{"$nulls":7},"        Fix32.THISNODE.SJ3112Tank1SelCur.F_CV = 0\n      Fix32.THISNODE.SJ3112Tank2SelCur.F_CV = 1"]
[{"$nulls":3},"加表料段SJ3115不选择料筒",{"$nulls":7},"          Fix32.THISNODE.SJ3112Tank1SelCur.F_CV = 0\n      Fix32.THISNODE.SJ3112Tank2SelCur.F_CV = 0"]
[{"$nulls":3},"加里料段不加水",{"$nulls":7}," If Fix32.THISNODE.YT612_SJ3112Tank1SelNW.F_CV = 0 Then\n    If MsgBox(\"确定要不加水操作吗？\", vbYesNo, \"不加水操作\") = vbYes Then\n       Fix32.THISNODE.YT612_SJ3112Tank1SelNW.F_CV = 1\n       Call Modlogin.Oplog((0), (0), (1), \"白肋烟加里料段不加水\")\n    End If\n  Else\n    If MsgBox(\"确定要取消白肋烟加里料段不加水启动吗？\", vbYesNo, \"里料段不加水\") = vbYes Then\n       Fix32.THISNODE.YT612_SJ3112Tank1SelNW.F_CV = 0\n       Call Modlogin.Oplog((0), (0), (1), \"取消白肋烟加里料段不加水\")\n    End If\n  End If"]
[{"$nulls":3},"加里料段加料方向柜选择",{"$nulls":7}," Fix32.THISNODE.ZGOutRoadCur.F_CV = 0"]
[{"$nulls":3},"加里料段非加料方向选择",{"$nulls":7},"  Fix32.THISNODE.ZGOutRoadCur.F_CV = 1"]
[{"$nulls":3},"加里料段出BLG3柜操作",{"$nulls":7},"      Fix32.THISNODE.GP3119OutSelCur.F_CV = 1\n      Fix32.THISNODE.GP3119_1OutSelCur.F_CV = 0"]
[{"$nulls":3},"加里料段出BLG4柜操作",{"$nulls":7},"      Fix32.THISNODE.GP3119OutSelCur.F_CV = 0\n      Fix32.THISNODE.GP3119_1OutSelCur.F_CV = 1"]
[{"$nulls":3},"加里料段不出柜",{"$nulls":7},"  Fix32.THISNODE.GP3119OutSelCur.F_CV = 0\n      Fix32.THISNODE.GP3119_1OutSelCur.F_CV = 0"]
[{"$nulls":3},"加里料段中柜进BLG3选择",{"$nulls":7},"     Fix32.THISNODE.GP3119InSelCur.F_CV = 1\n      Fix32.THISNODE.GP3119_1InSelCur.F_CV = 0"]
[{"$nulls":3},"加里料段中柜进BLG4选择",{"$nulls":7},"      Fix32.THISNODE.GP3119InSelCur.F_CV = 0\n      Fix32.THISNODE.GP3119_1InSelCur.F_CV = 1"]
[{"$nulls":3},"加里料段不进中柜选",{"$nulls":7}," Fix32.THISNODE.GP3119InSelCur.F_CV = 0\n      Fix32.THISNODE.GP3119_1InSelCur.F_CV = 0"]
[null,null,"进预配柜信息下","BLG3","单柜号、批次号、牌号",{"$nulls":6},"Fix32.thisnode.BLG3BatchNo1.A_CV/Fix32.thisnode.BLG3Brand1.A_CV"]
[{"$nulls":3},"BLG4",{"$nulls":7},"Fix32.thisnode.BLG4BatchNo1.A_CV/Fix32.thisnode.BLG4Brand1.A_CV"]
[null,null,"进柜段组合启动",null,"无",{"$nulls":6},"      Fix32.THISNODE.YT612InnerStuffGStart.F_CV = 1"]
[null,"生产提升","生产提升-松散回潮",null,"无",{"$nulls":6},"Fix32.THISNODE.yt612_wp3107_asend.F_CV = 1"]
[null,null,"强制提升-松散回潮",null,"无",{"$nulls":6},"Fix32.THISNODE.yt612_wp3107_forceasend.F_CV = 1"]
[null,null,"强制停止提升-松散回潮",null,"无",{"$nulls":6},"Fix32.THISNODE.YT612_WP3107_FORCESTOP.F_CV = 1"]
[null,"组合停止","批结束【确认】",null,"无",{"$nulls":6},"     Fix32.THISNODE.YT612InnerStuffBatchStart.F_CV = 0\n     Fix32.THISNODE.YT612InnerStuffBatchStop.F_CV = 1"]
[null,null,"余料回收","桶一余料回收",{"$nulls":7},"     Fix32.thisnode.SJ3112tank1BackStuff.f_cv = 1\n     Fix32.thisnode.SJ3112tank1AskStuff.f_cv = 0"]
[{"$nulls":3},"桶一余料回收取消",{"$nulls":7},"     Fix32.thisnode.SJ3112tank1BackStuff.f_cv = 0\n     Fix32.thisnode.SJ3112tank1AskStuff.f_cv = 0"]
[{"$nulls":3},"桶二余料回收",{"$nulls":7},"     Fix32.thisnode.SJ3112tank2BackStuff.f_cv = 1\n     Fix32.thisnode.SJ3112tank2AskStuff.f_cv = 0"]
[{"$nulls":3},"桶二余料回收取消",{"$nulls":7},"     Fix32.thisnode.SJ3112tank2BackStuff.f_cv = 0\n     Fix32.thisnode.SJ3112tank2AskStuff.f_cv = 0"]
[{"$nulls":3},"桶一加热",{"$nulls":7}," Fix32.thisnode.SJ3112Tank1Warmup.f_cv = 1"]
[{"$nulls":3},"桶一加热停止",{"$nulls":7}," Fix32.thisnode.SJ3112Tank1Warmup.f_cv = 0"]
[{"$nulls":3},"桶二加热",{"$nulls":7}," Fix32.thisnode.SJ3112Tank2Warmup.f_cv = 1"]
[{"$nulls":3},"桶二加热停止",{"$nulls":7}," Fix32.thisnode.SJ3112Tank2Warmup.f_cv = 0"]
[{"$nulls":3},"桶一喷吹",{"$nulls":7}," Fix32.thisnode.SJ3112Tank1Blow.f_cv = 1"]
[{"$nulls":3},"桶一清洗",{"$nulls":7}," Fix32.thisnode.SJ3112Tank1AutoClear.f_cv = 1"]
[{"$nulls":3},"桶二喷吹",{"$nulls":7},"Fix32.thisnode.SJ3112Tank2Blow.f_cv = 1"]
[{"$nulls":3},"桶二清洗",{"$nulls":7}," Fix32.thisnode.SJ3112Tank1AutoClear.f_cv = 1"]
[null,null,"批次清零",null,"无",{"$nulls":6}," Fix32.thisnode.CH3108Clear.f_cv = 1\n Fix32.thisnode.SJ3112WaterClear.f_cv = 1\n Fix32.thisnode.SJ3112StuffClear.f_cv = 1"]
[null,null,"生产清零",null,"无",{"$nulls":6},"Fix32.thisnode.CH3108AccmFlowDB.f_cv = 0\nFix32.thisnode.CH3108ChannelSet.f_cv = 0\nFix32.thisnode.CH3108FlowSet.f_cv = 0\nFix32.thisnode.CH3133ChannelSet.f_cv = 0\nFix32.thisnode.CH3133FlowSet.f_cv = 0\nFix32.thisnode.GP3104OutSelCur.f_cv = 0\nFix32.thisnode.GP3104_1OutSelCur.f_cv = 0\nFix32.thisnode.GP3119OutSelCur.f_cv = 0\nFix32.thisnode.GP3119_1OutSelCur.f_cv = 0\nFix32.thisnode.GP3119InSelCur.f_cv = 0\nFix32.thisnode.GP3119_1InSelCur.f_cv = 0\nFix32.thisnode.InnerStuffProdModeCur.f_cv = 0\nFix32.thisnode.SJ3112AddStuffAcuDB.f_cv = 0\nFix32.thisnode.SJ3112Tank1SelCur.f_cv = 0\nFix32.thisnode.SJ3112Tank2SelCur.f_cv = 0\nFix32.thisnode.ZGOutRoadCur.f_cv = 0\nFix32.thisnode.CH3108Clear.f_cv = 0\nFix32.thisnode.CH31INNERSTUFFBATCHSEQ08Clear.f_cv = 0\nFix32.thisnode.INNERSTUFFINGP1AMOUNT.f_cv = 0\nFix32.thisnode.INNERSTUFFINGP2AMOUNT.f_cv = 0\nFix32.thisnode.INNERSTUFFINGP3AMOUNT.f_cv = 0\nFix32.thisnode.INNERSTUFFINGPQTY.f_cv = 0\nFix32.thisnode.INNERSTUFFPRODMIX.f_cv = 0\nFix32.thisnode.INNERSTUFFROAD.f_cv = 0\nFix32.thisnode.INNERSTUFFWEIGHT.f_cv = 0\n\nFix32.thisnode.INNERSTUFFBATCHNO.A_cv = \"\"\nFix32.thisnode.INNERSTUFFBRAND.A_cv = \"\"\nFix32.thisnode.INNERSTUFFENTRYID.A_cv = \"\"\nFix32.thisnode.INNERSTUFFINGP1.A_cv = \"\"\nFix32.thisnode.INNERSTUFFINGP2.A_cv = \"\"\nFix32.thisnode.INNERSTUFFINGP3.A_cv = \"\"\nFix32.thisnode.INNERSTUFFJHJSSJ.A_cv = \"\"\nFix32.thisnode.INNERSTUFFJHKSSJ.A_cv = \"\"\nFix32.thisnode.INNERSTUFFOUTGP.A_cv = \"\"\nFix32.thisnode.INNERSTUFFSTUFFBRAND.A_cv = \"\"\n\n\n\n"]
[null,null,"前柜信息清零",null,"无",{"$nulls":6},"Fix32.thisnode.BLG1BatchNo1.A_CV/Fix32.thisnode.BLG3Brand1.A_CV\nFix32.thisnode.BLG2BatchNo1.A_CV/Fix32.thisnode.BLG4Brand1.A_CV\n"]
[null,null,"预配柜清零（工单信息下发的业务柜号）",null,"无"]
[null,null,"设备组合停止",null,"无",{"$nulls":6}," Fix32.THISNODE.YT612InnerStuffGStop.F_CV = 1"]
[null,"辅助操作","单机/联机【待定】",null,"段号"]
[null,null,"故障复位","参考昆船原的功能？","无",{"$nulls":6},"Fix32.THISNODE.YT612OuterStuffReset.F_CV = 1"]
[]
["白肋烟加表料",null,"预热启动",null,"无",{"$nulls":6},"Fix32.thisnode.SJ3135PreHeatStart.f_cv = 1"]
[null,null,"预热温度值设定",null,"温度值"]
[null,null,"预热生产温度值设定",null,"温度值",{"$nulls":6},"SJ3135WORKTEMPSET"]
[null,null,"预热结束",null,"无",{"$nulls":6},"Fix32.thisnode.SJ3135PreHeatStop.f_cv = 1"]
[null,null,"工单信息下发",null,"工单号、批次号、牌号",{"$nulls":6},"Fix32.THISNODE.OuterStuffEntryID.A_CV\nFix32.THISNODE.OuterStuffBatchNo.A_CV\nFix32.THISNODE.OuterStuffBrand.A_CV\n"]
[null,null,"单机",{"$nulls":8},"     Fix32.THISNODE.YT612OuterStuffAUTO.F_CV = 0\n     Fix32.THISNODE.YT612OuterStuffLOCK.F_CV = 0\n     Fix32.THISNODE.YT612OuterStuffMAN.F_CV = 1"]
[null,null,"自动",{"$nulls":8},"     Fix32.THISNODE.YT612OuterStuffMAN.F_CV = 0\n     Fix32.THISNODE.YT612OuterStuffAUTO.F_CV = 1\n     Fix32.THISNODE.YT612OuterStuffLOCK.F_CV = 0"]
[null,null,"闭锁",{"$nulls":8},"     Fix32.THISNODE.YT612OuterStuffMAN.F_CV = 0\n     Fix32.THISNODE.YT612OuterStuffAUTO.F_CV = 0\n     Fix32.THISNODE.YT612OuterStuffLOCK.F_CV = 1"]
[null,null,"要料信息下发-料筒1",null,"料液重量、料液代码、批次号",{"$nulls":6},"    Fix32.THISNODE.SJ3135Tank1AskQty.F_CV =   \nFix32.THISNODE.SJ3135Tank1AskBatch.A_CV = \n   Fix32.THISNODE.SJ3135Tank1AskBrand.A_CV = \n   Fix32.THISNODE.SJ3135Tank1AskQty.F_CV = "]
[null,null,"要料请求-料筒1",null,"无",{"$nulls":6},"   Fix32.THISNODE.SJ3135Tank1AskStuff.F_CV = 1"]
[null,null,"取消要料请求-料筒1",null,"无",{"$nulls":6},"   Fix32.THISNODE.SJ3135Tank1AskStuff.F_CV = 0"]
[null,null,"批开始",null,"无",{"$nulls":6},"     Fix32.THISNODE.YT612OuterStuffBatchStart.F_CV = 1\n     Fix32.THISNODE.YT612OuterStuffBatchStop.F_CV = 0"]
[null,null,"临时","加表料段进BLG5柜",{"$nulls":7},"      Fix32.THISNODE.GP3139InSelCur.F_CV = 1\n      Fix32.THISNODE.GP3139_1InSelCur.F_CV = 0"]
[{"$nulls":3},"加表料段进BLG6柜",{"$nulls":7},"      Fix32.THISNODE.GP3139InSelCur.F_CV = 0\n      Fix32.THISNODE.GP3139_1InSelCur.F_CV = 1"]
[{"$nulls":3},"加表料段不进柜",{"$nulls":7},"      Fix32.THISNODE.GP3139InSelCur.F_CV = 0\n      Fix32.THISNODE.GP3139_1InSelCur.F_CV = 0"]
[{"$nulls":3},"加表料段SJ3115料筒1选择",{"$nulls":7},"  Fix32.THISNODE.SJ3135Tank1SelCur.F_CV = 1"]
[{"$nulls":3},"加表料段SJ3115不选择料筒",{"$nulls":7},"  Fix32.THISNODE.SJ3135Tank1SelCur.F_CV = 0"]
[null,null,"进预配柜信息下发(增加柜号写入ifix点)","BLG5","单柜号、批次号、牌号",{"$nulls":6},"Fix32.thisnode.BLG5BatchNo1.A_CV/Fix32.thisnode.BLG5Brand1.A_CV"]
[{"$nulls":3},"BLG6",{"$nulls":7},"Fix32.thisnode.BLG6BatchNo1.A_CV/Fix32.thisnode.BLG6Brand1.A_CV"]
[null,null,"进柜段组合启动",null,"无",{"$nulls":6}," Fix32.THISNODE.YT612OuterStuffGStart.F_CV = 1"]
[null,"生产提升","生产提升-松散回潮",null,"无"]
[null,null,"强制提升-松散回潮",null,"无"]
[null,null,"强制停止提升-松散回潮",null,"无"]
[null,null,"生产提升-薄片",null,"无"]
[null,null,"强制提升-薄片",null,"无"]
[null,null,"强制停止提升-薄片",null,"无"]
[null,null,"余料回收","桶一余料回收",{"$nulls":7},"      Fix32.thisnode.SJ3135tank1BackStuff.f_cv = 1\n     Fix32.thisnode.SJ3135tank1AskStuff.f_cv = 0"]
[{"$nulls":3},"桶一余料回收取消",{"$nulls":7},"     Fix32.thisnode.SJ3135tank1BackStuff.f_cv = 0\n     Fix32.thisnode.SJ3135tank1AskStuff.f_cv = 0"]
[{"$nulls":3},"桶一喷吹",{"$nulls":7}," Fix32.thisnode.SJ3135Tank1Blow.f_cv = 1"]
[{"$nulls":3},"桶一清洗",{"$nulls":7},"     Fix32.thisnode.SJ3135Tank1AutoClear.f_cv = 1"]
[null,"组合停止","批结束【确认】",null,"无",{"$nulls":6},"     Fix32.THISNODE.YT612OuterStuffBatchStart.F_CV = 0\n     Fix32.THISNODE.YT612OuterStuffBatchStop.F_CV = 1"]
[null,null,"批次清零",null,"无",{"$nulls":6}," Fix32.thisnode.CH3133Clear.f_cv = 1\n Fix32.thisnode.SJ3135WaterClear.f_cv = 1\n Fix32.thisnode.SJ3135StuffClear.f_cv = 1"]
[null,null,"生产清零",null,"无",{"$nulls":6},"\"Fix32.thisnode.CH3133AccmFlowDB.f_cv = 0\nFix32.thisnode.GP3139InSelCur.f_cv = 0\nFix32.thisnode.GP3139_1InSelCur.f_cv = 0\nFix32.thisnode.SJ3112AddProportion.f_cv = 0\nFix32.thisnode.SJ3112OutWaterSet.f_cv = 0\nFix32.thisnode.SJ3112WorkTempSet.f_cv = 0\nFix32.thisnode.SJ3135AddProportion.f_cv = 0\nFix32.thisnode.SJ3135AddStuffAcuDB.f_cv = 0\nFix32.thisnodeS.J3135OutWaterSet.f_cv = 0\nFix32.thisnode.SJ3135Tank1SelCur.f_cv = 0\nFix32.thisnode.GP3119OutSelCur.f_cv = 0\nFix32.thisnode.GP3119_1OutSelCur.f_cv = 0\nFix32.thisnode.SJ3112AddStuffAcuDB.f_cv = 0\nFix32.thisnode.SJ3112Tank1SelCur.f_cv = 0\nFix32.thisnode.SJ3112Tank2SelCur.f_cv = 0\nFix32.thisnode.ZGOutRoadCur.f_cv = 0\nFix32.thisnode.CH3108Clear.f_cv = 0\nFix32.thisnode.CH31INNERSTUFFBATCHSEQ08Clear.f_cv = 0\nFix32.thisnode.INNERSTUFFINGP1AMOUNT.f_cv = 0\nFix32.thisnode.INNERSTUFFINGP2AMOUNT.f_cv = 0\nFix32.thisnode.INNERSTUFFINGP3AMOUNT.f_cv = 0\nFix32.thisnode.INNERSTUFFINGPQTY.f_cv = 0\nFix32.thisnode.INNERSTUFFPRODMIX.f_cv = 0\nFix32.thisnode.INNERSTUFFROAD.f_cv = 0\nFix32.thisnode.INNERSTUFFWEIGHT.f_cv = 0\n\nFix32.thisnode.INNERSTUFFBATCHNO.A_cv = \"\"\"\"\nFix32.thisnode.INNERSTUFFBRAND.A_cv = \"\"\"\"\nFix32.thisnode.INNERSTUFFENTRYID.A_cv = \"\"\"\"\nFix32.thisnode.INNERSTUFFINGP1.A_cv = \"\"\"\"\nFix32.thisnode.INNERSTUFFINGP2.A_cv = \"\"\"\"\nFix32.thisnode.INNERSTUFFINGP3.A_cv = \"\"\"\"\nFix32.thisnode.INNERSTUFFJHJSSJ.A_cv = \"\"\"\"\nFix32.thisnode.INNERSTUFFJHKSSJ.A_cv = \"\"\"\"\nFix32.thisnode.INNERSTUFFOUTGP.A_cv = \"\"\"\"\nFix32.thisnode.INNERSTUFFSTUFFBRAND.A_cv = \"\"\"\"\n\n\n\n\"\n"]
[null,null,"预配柜清零（工单信息下发的业务柜号）",null,"无"]
[null,null,"设备组合停止",null,"无",{"$nulls":6},"       Fix32.THISNODE.YT612OuterStuffGStop.F_CV = 1"]
[null,"辅助操作","单机/联机【待定】","需根据昆船系统的单机/联机功能把所有段都单独封装","段号"]
[null,null,"故障复位","参考昆船原的功能？","无",{"$nulls":6},"Fix32.THISNODE.YT606InnerStuffReset.F_CV = 1"]
[]
[]
[null,null,"工单信息下发",null,"工单号、批次号、牌号"]
[null,null,"批开始",null,"无",{"$nulls":6},"     Fix32.THISNODE.YT612OutGPBatchStart.F_CV = 1\n     Fix32.THISNODE.YT612OutGPBatchStop.F_CV = 0"]
[null,null,"设备单元自动",{"$nulls":8},"     Fix32.THISNODE.YT612OutGPMAN.F_CV = 0\n     Fix32.THISNODE.YT612OutGPAUTO.F_CV = 1\n     Fix32.THISNODE.YT612OutGPLOCK.F_CV = 0"]
[null,null,"设备单元单机",{"$nulls":8},"     Fix32.THISNODE.YT612OutGPAUTO.F_CV = 0\n     Fix32.THISNODE.YT612OutGPLOCK.F_CV = 0\n     Fix32.THISNODE.YT612OutGPMAN.F_CV = 1"]
[null,null,"设备单元闭锁",{"$nulls":8},"     Fix32.THISNODE.YT612OutGPMAN.F_CV = 0\n     Fix32.THISNODE.YT612OutGPAUTO.F_CV = 0\n     Fix32.THISNODE.YT612OutGPLOCK.F_CV = 1"]
[null,null,"临时",null,"出柜段出BLG5柜",{"$nulls":6},"      Fix32.THISNODE.GP3139OutSelCur.F_CV = 1\n      Fix32.THISNODE.GP3139_1OutSelCur.F_CV = 0"]
[{"$nulls":4},"出柜段出BLG6柜",{"$nulls":6},"      Fix32.THISNODE.GP3139OutSelCur.F_CV = 0\n      Fix32.THISNODE.GP3139_1OutSelCur.F_CV = 1"]
[{"$nulls":4},"出柜段不出柜",{"$nulls":6},"      Fix32.THISNODE.GP3139OutSelCur.F_CV = 0\n      Fix32.THISNODE.GP3139_1OutSelCur.F_CV = 0"]
[null,null,"进柜段组合启动",null,"无",{"$nulls":6}," Fix32.THISNODE.YT612OutGPGStart.F_CV = 1"]
[null,"组合停止","批结束【确认】",null,"无",{"$nulls":6},"     Fix32.THISNODE.YT612OutGPBatchStart.F_CV = 0\n     Fix32.THISNODE.YT612OutGPBatchStop.F_CV = 1"]
[null,null,"批次清零",null,"无"]
[null,null,"生产清零",null,"无"]
[null,null,"预配柜清零（工单信息下发的业务柜号）",null,"无"]
[null,null,"设备组合停止",null,"无",{"$nulls":6}," Fix32.THISNODE.YT612OutGPGStop.F_CV = 1"]
[null,"辅助操作","单机/联机【待定】","需根据昆船系统的单机/联机功能把所有段都单独封装","段号"]
[null,null,"故障复位","参考昆船原的功能？","无",{"$nulls":6},"Fix32.THISNODE.YT606OutGPReset.F_CV = 1"]
[]
[]
[]
[]
["烤机操作",null,"单机",{"$nulls":8},"writevalue \"0\", \"Fix32.ThISNODE.kzmb-lj.f_cv\", 2"]
[null,null,"联机",{"$nulls":8},"writevalue \"1\", \"Fix32.ThISNODE.kzmb-lj.f_cv\", 2"]
[null,null,"手动",{"$nulls":8},"writevalue \"0\", \"Fix32.ThISNODE.kzmb-zd.f_cv\", 2"]
[null,null,"自动",{"$nulls":8}," writevalue \"1\", \"Fix32.ThISNODE.kzmb-zd.f_cv\", 2"]
[null,null,"关灯",{"$nulls":8},"writevalue \"0\", \"Fix32.ThISNODE.kzmb-qyzmkg.f_cv\", 2"]
[null,null,"开灯",{"$nulls":8}," writevalue \"1\", \"Fix32.ThISNODE.kzmb-qyzmkg.f_cv\", 2"]
[null,null,"组合启动",{"$nulls":8}," writevalue \"1\", \"Fix32.ThISNODE.kzmb-zhqd.f_cv\", "]
[null,null,"组合停止",{"$nulls":8},"  writevalue \"1\", \"Fix32.ThISNODE.kzmb-zhtz.f_cv\", 2"]
[null,null,"强制回潮",{"$nulls":8}," writevalue \"1\", \"Fix32.ThISNODE.SBForceTide.f_cv\", 2"]
[null,null,"取消强制回潮",{"$nulls":8},"  writevalue \"0\", \"Fix32.ThISNODE.SBForceTide.f_cv\", 2"]
[null,null,"纯干燥选择",{"$nulls":8},"  writevalue \"1\", \"Fix32.ThISNODE.ytsb_cgzxz.f_cv\", 2"]
[null,null,"纯干燥选择取消",{"$nulls":8},"  writevalue \"0\", \"Fix32.ThISNODE.ytsb_cgzxz.f_cv\", 2"]
[null,null,"消防解除",{"$nulls":8},"\n  writevalue \"1\", \"Fix32.ThISNODE.xfjc.f_cv\", 2"]
[null,null,"报警消音",{"$nulls":8}," writevalue \"1\", \"Fix32.ThISNODE.bjxy.f_cv\", 2"]
[null,null,"变频器故障复位",{"$nulls":8},"  Fix32.thisnode.VFERRRESET.f_cv = 1"]

{"sheet":"Sheet1","index":8,"n_rows":86,"n_cols":4,"rows_kept":86,"flags":["formulas_cached_only"]}
["public","string","工序","{get;set;}"]
["public","string","操作按钮","{get;set;}"]
["public","string","组件封装","{get;set;}"]
["public","string","业务说明","{get;set;}"]
["public","string","参数说明","{get;set;}"]
["public","string","API接口名1","{get;set;}"]
["public","string","是否验证","{get;set;}"]
["public","string","生成类型","{get;set;}"]
["public","string","选写多值","{get;set;}"]
["public","string","API接口名","{get;set;}"]
["public","string","写入点位","{get;set;}"]
["public","string","测试方法","{get;set;}"]
["public","string","检查点位","{get;set;}"]
["public","string","测试状态","{get;set;}"]
["public","string","测试输入","{get;set;}"]
["public","string","测试输出","{get;set;}"]
["public","string","测试点位变化","{get;set;}"]
["public","string","备注","{get;set;}"]
["public","string","API状态","{get;set;}"]
["public","string","按键逻辑","{get;set;}"]
["public","string","逻辑代码","{get;set;}"]
[]
[]
[]
[]
[]
["YG02",","]
["YG04",","]
["YG06",","]
["YG08",","]
["YG10",","]
["YG12",","]
["YG14",","]
["YG16",","]
["YG01",","]
["YG03",","]
["YG05",","]
["YG07",","]
["YG09",","]
["YG11",","]
["YG13",","]
["YG15"]
[]
[]
[]
[]
[]
["YG01",","]
["YG02",","]
["YG03",","]
["YG04",","]
["YG05",","]
["YG06",","]
["YG07",","]
["YG08",","]
["YG09",","]
["YG10",","]
["YG11",","]
["YG12",","]
["YG13",","]
["YG14",","]
["YG15"]
{"$rows_empty":9}
["YG02"]
["YG06"]
["YG08"]
["YG10"]
["YG12"]
["YG14"]
["YG16"]
["YG01"]
["YG03"]
["YG05"]
["YG07"]
["YG09"]
["YG11"]
["YG13"]
["YG15"]